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		ORIGINAL ISSUE: AUGUST 11, 2026
The information contained in this document serves as the official FAA guidance, Holdover Times and Allowance Times for use during the 
2026-2027 winter season. 
Direct questions or comments concerning FAA aircraft ground de/anti-icing requirements and policies, technical content of the holdover time tables and allowance time tables or access issues to 9-AFS-200‑Correspondence@faa.gov with HOT 26/27 in the subject line.
The Holdover Times Tables and related information can be found at the FAA’s Aircraft Ground Deicing website.
To receive notifications on updates to the Holdover Times Tables and related information, subscribe to the Aircraft Ground Deicing website by clicking on this link.


This document is intended to be used in conjunction with the 
FAA Ground Deicing Program General Information Document,
Winter 2026-2027, located on the FAA’s Aircraft Ground Deicing website.



This is a guidance document. Its content is not legally binding in its own right and will not be relied upon by the Department as a separate basis for affirmative enforcement action or other administrative penalty. Conformity with the guidance document is voluntary only. Nonconformity will not affect rights and obligations under existing statutes and regulations.
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[bookmark: _Toc234306034]How to Use This Document
Complementary Documents
[bookmark: _Hlk76975378]This document is designed to be used in conjunction with the FAA N 8900 series notice “Revised FAA-Approved Deicing Program Updates, Winter 2026-2027” and the latest FAA General Information Ground Deicing Program. These documents complement each other and should be used together for a thorough understanding of the subject matter.
Beginning in the winter of 2021-22, the FAA has published an annual database of degree-specific holdover times (DSHOTs) for snow and snow-related precipitation conditions (including snow, snow grains, and snow pellets). The DSHOT database contains an expanded set of snow precipitation HOTs for all undiluted Type II, III and IV anti-icing fluids listed in the FAA HOT Guidelines. This database can be found at the following website: 
https://www.faa.gov/other_visit/aviation_industry/airline_operators/airline_safety/deicing/.
Guidance and conditions on the use of DSHOT data can be found in the latest FAA General Information Ground Deicing Program document. 
Applicability
A new version of this document is published for each winter operating season, typically in early August preceding the winter operating season. Updates to the winter’s document may be published at any time after the Original Issue document is published. When a new document is published, either mid-season or each new season, the previous document becomes obsolete. It is the responsibility of the end user to periodically check for document updates on the following website:
https://www.faa.gov/other_visit/aviation_industry/airline_operators/airline_safety/deicing/.
Main Document Structure and Content
This document is divided into several sections.
· Change Control Records: Provides details of any changes made to the document in mid-season document updates.
· Table of Contents: Provides a list of sections, tables, and appendices in the document.
· How to Use This Document: Provides top-level guidance on how to use the document.
· Highlights and Changes for Winter 2026-2027: Describes key changes made to the document for the current winter operating season.
· Holdover Time Guidelines: Series of tables that provide estimated holdover times (in hh:mm). Fluids are divided by fluid type (Type I, II, III, and IV), aircraft construction materials (Type I only), fluid brand (Type II, III, IV), aircraft rotation speed (Type III only), and fluid application temperature (Type III only). Columns in the tables divide the information by precipitation type; rows in the tables divide the information by temperature and fluid dilution. Notes in the tables refer to additional information on the specific HOTs. Cautions that apply to all tables in a section are located on the flysheets before each section.
· [bookmark: _Hlk107319870][bookmark: _Hlk170966679]Allowance Times Tables: Tables that provide allowance times (in minutes) for Type III and Type IV fluids. Rows in the tables divide the information by precipitation type; columns in the tables divide the information by temperature. Notes in the tables refer to additional information on the specific allowance times. Cautions that apply to all allowance times tables are located on the flysheet before the section. Use of these tables must be validated by first confirming that the fluid being used is listed in the “Validation Status of Fluids for Use with Allowance Times” (Table 53). 
· Supplementary Guidance: Series of tables that provide supplementary information for using the holdover time guidelines and allowance times tables. Includes a table for estimating snowfall intensity from prevailing visibility, tables of fluid information (one table per fluid type), and tables of fluid application guidance (by fluid type).


Appendices
The appendices contain complementary content.
· Appendix A: Provides adjusted holdover time guidelines (holdover time tables and allowance time tables) for operations when flaps and slats are deployed prior to de/anti-icing.
· Appendix B: Provides information on laboratories involved in testing de/anti-icing fluids.
· Appendix C: Provides the latest de/anti-icing fluid manufacturer contact information at the time of publication.

[bookmark: _Toc14867829][bookmark: _Toc106020664][bookmark: _Toc198720845][bookmark: _Toc234306035][bookmark: _Toc508704800][bookmark: _Toc43986149]Highlights and Changes for Winter 2026-2027
CHANGED THIS YEAR
The principal changes from this year are briefly indicated herein.
Holdover Time Tables
Fluid-specific HOT guidelines tables have been created for four new fluids: 
· LNT Solutions P250 (Type II) 
· LNT Solutions P450 (Type IV)
· MAX TECH AIRCRAFT MAINTENANCE AND REPAIR LLC MTL 4-EG (Type IV)
· MAX TECH AIRCRAFT MAINTENANCE AND REPAIR LLC MTL 4-PG (Type IV)
Fluid-specific HOT guidelines tables have been updated for seven existing fluids:
· Aviation Xi’an High-Tech Cleanwing II (Type II)
· Kilfrost Limited ABC-K Plus (Type II)
· AllClear Systems LLC AeroClear MAX (Type III)
· ALAB International PROFLIGHT EG4 (Type IV)
· CHEMCO Inc. ChemR EG IV (Type IV)
· CHEMCO Inc. ChemR Nordik IV (Type IV)
· JSC RCP Nordix Defrost NORTH 4 (Type IV)
The HOT Guidelines for AVIAFLUID AVIAFLIGHT EG (Type IV) have been removed.
Some decreases have been made to the Type IV generic holdover times as a result of the newly added fluids. 
Editorial revisions have been made to the AllClear AeroClear MAX (Type III) HOT tables relating to ramp speed.
Editorial changes have been made to several notes to improve clarity and reduce redundancy.
Allowance Times Tables
Table 53 title has been revised from “List of Fluids Validated for Use with Allowance Times” to “Validation Status of Fluids for Use with Allowance Times” to better reflect the content of the table.
METAR codes FZDZPL and DZPL have been reassigned from “Light Ice Pellets mixed with Drizzle or Freezing Drizzle” to “Moderate Ice Pellets mixed with Drizzle or Freezing Drizzle.” The codes +FZDZPL and +DZPL have been removed. Related descriptors have also been revised: “Moderate” and “Heavy” were removed from the Light Ice Pellets condition, and “Heavy” was removed from the Moderate Ice Pellets condition, to align with the revised classifications.
Minor editorial changes have been made to notes and references to improve clarity and reduce redundancy.
Supplemental Guidance
The list of fluids (Table 58 - Table 61) has been updated to reflect the latest information available on all de/anti-icing fluids. 
Three snowfall intensity classifications within the “Snowfall Intensities as a Function of Prevailing Visibility” table (Table 57) have been revised from “Very Light” to “Light.”


UNCHANGED FROM PREVIOUS YEAR
Holdover Time Tables
The Active Frost HOTs are unchanged.
The Generic Type II HOTs are unchanged.
Supplemental Guidance
The fluid application tables are unchanged.
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[bookmark: _Hlk107318671]
The HOT Guidelines are provided for information and guidance purposes. The HOT Guidelines on their own do not change, create, amend or permit deviations from regulatory requirements.

The HOT Guidelines may use mandatory terms such as “must”, “shall” and “is/are required” so as to convey the intent of meeting regulatory requirements and SAE Standards, where applicable. The term “should” is to be understood, unless an alternative method of achieving safety is implemented that would meet or exceed the intent of the recommendation.


[bookmark: _Hlk107237964]
[bookmark: ActiveFrostCautions]CAUTIONS
The responsibility for the application of these data remains with the user.
Fluids used during ground de/anti-icing do not provide in-flight icing protection.
This table is for departure planning only and should be used in conjunction with pre-takeoff check procedures.
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[bookmark: _Toc508704802][bookmark: _Toc43986151][bookmark: _Toc234306037]Table 1: Active Frost Holdover Times for SAE Type I, Type II, Type III, and Type IV Fluids1
	Outside Air 
Temperature2,3,4
	Type I Aluminum
	Type I Composite
	
	Outside Air 
Temperature3,4
	Concentration Fluid/Water
By % Volume
	Type II
	Type III5
	Type IV

	-1 °C and above
(30 °F and above)
	0:45
	0:35
	
	-1 °C and above
(30 °F and above)
	100/0
	8:00
	2:00
	12:00

	
	
	
	
	
	75/25
	5:00
	1:00
	5:00

	
	
	
	
	
	50/50
	2:00
	0:30
	3:00

	below -1 to -3 °C
(below 30 to 27 °F)
	
	
	
	below -1 to -3 °C
(below 30 to 27 °F)
	100/0
	8:00
	2:00
	12:00

	
	
	
	
	
	75/25
	5:00
	1:00
	5:00

	
	
	
	
	
	50/50
	1:30
	0:30
	3:00

	below -3 to -10 °C
(below 27 to 14 °F)
	
	
	
	below -3 to -10 °C
(below 27 to 14 °F)
	100/0
	8:00
	2:00
	10:00

	
	
	
	
	
	75/25
	4:00
	1:00
	5:00

	below -10 to -14 °C
(below 14 to 7 °F)
	
	
	
	below -10 to -14 °C
(below 14 to 7 °F)
	100/0
	6:00
	2:00
	6:00

	
	
	
	
	
	75/25
	1:00
	1:00
	1:00

	below -14 to -21 °C
(below 7 to -6 °F)
	
	
	
	below -14 to -21 °C
(below 7 to -6 °F)
	100/0
	3:00
	2:00
	6:00

	below -21 to -25 °C
(below -6 to -13 °F)
	
	
	
	below -21 to -25 °C
(below -6 to -13 °F)
	100/0
	2:00
	2:00
	4:00

	below -25 °C 
(below -13 °F)
	
	
	
	below -25 °C 
(below -13 °F)
	100/0
	No Holdover Time Guidelines Exist


NOTES
To use the holdover times in this table, ensure that the fluid and dilution being used is listed in the List of Fluids Tested for Anti-Icing Performance and Aerodynamic Acceptance table (Table 58 - Table 61). Any restrictions on the use of the fluid have to be identified and applied.
Type I Fluid / Water Mixture must be selected so that the freezing point of the mixture is at least 10 °C (18 °F) below outside air temperature.
Ensure that the lowest operational use temperature (LOUT) is respected. 
Changes in outside air temperature (OAT) over the course of longer frost events can be significant; the appropriate holdover time to use is the one provided for the coldest OAT that has occurred in the time between the de/anti-icing fluid application and takeoff.
To use the Type III fluid frost holdover times, the fluid brand being used must be known. AllClear AeroClear MAX must be applied unheated. 
CAUTIONS
The cautions that apply to the holdover times in the table above can be found on page 9.

FAA 2016-2017 Holdover Time Guidelines		08/05/16
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[bookmark: _Toc234306038]HOT Guidelines for SAE Type I Fluids
Winter 2026-2027

The HOT Guidelines are provided for information and guidance purposes. The HOT Guidelines on their own do not change, create, amend or permit deviations from regulatory requirements.

The HOT Guidelines may use mandatory terms such as “must”, “shall” and “is/are required” so as to convey the intent of meeting regulatory requirements and SAE Standards, where applicable. The term “should” is to be understood, unless an alternative method of achieving safety is implemented that would meet or exceed the intent of the recommendation.


[bookmark: _Hlk107238002]
[bookmark: TypeICautions]CAUTIONS
The responsibility for the application of these data remains with the user.
The time of protection will be shortened in heavy weather conditions, heavy precipitation rates or high moisture content.
High wind velocity, jet blast or blowing snow may reduce holdover time below the lowest time stated in the range.
The holdover time may be reduced when aircraft skin temperature is lower than outside air temperature.
Fluids used during ground de/anti-icing do not provide in-flight icing protection.
This table is for departure planning only and should be used in conjunction with pre-takeoff check procedures.
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[bookmark: _Toc234306039]Table 2: Holdover Times for SAE Type I Fluid on Critical Aircraft Surfaces
Composed Predominantly of Aluminum1
	Outside Air 
Temperature2,3
	Freezing Fog, Freezing Mist4, or Ice Crystals5
	Snow 
mixed with 
Freezing Fog6
	Very Light Snow, Snow Grains or Snow Pellets6,7
	Light 
Snow, Snow Grains or Snow Pellets6,7
	Moderate Snow, Snow Grains or Snow Pellets6,7
	Freezing 
Drizzle8
	Light 
Freezing Rain
	Moderate Snow mixed with Rain9,10
	Rain on Cold‑Soaked Wing10
	Other11

	-3 °C and above
(27 °F and above)
	0:11 - 0:17
	0:06 - 0:11
	0:18 - 0:22
	0:11 - 0:18
	0:06 - 0:11
	0:09 - 0:13
	0:02 - 0:05
	0:02 - 0:02
	0:02 - 0:05
	 

	below -3 to -6 °C
(below 27 to 21 °F)
	0:08 - 0:13
	0:05 - 0:08
	0:14 - 0:17
	0:08 - 0:14
	0:05 - 0:08
	0:05 - 0:09
	0:02 - 0:05
	CAUTION: 
No holdover time 
guidelines exist

	below -6 to -10 °C
(below 21 to 14 °F)
	0:06 - 0:10
	0:04 - 0:06
	0:11 - 0:13
	0:06 - 0:11
	0:04 - 0:06
	0:04 - 0:07
	0:02 - 0:05
	

	below -10 °C
(below 14 °F)
	0:05 - 0:09
	0:02 - 0:04
	0:07 - 0:08
	0:04 - 0:07
	0:02 - 0:04
	 
	 
	


NOTES
1. To use the holdover times in this table, ensure that the fluid and dilution being used is listed in the Type I Fluids Tested for Anti-Icing Performance and Aerodynamic Acceptance table (Table 58). Any restrictions on the use of the fluid have to be identified and applied.
1 Type I fluid / water mixture must be selected so that the freezing point of the mixture is at least 10 °C (18 °F) below outside air temperature.
Ensure that the lowest operational use temperature (LOUT) is respected.
Freezing mist is best confirmed by observation. It is never reported by METAR; however, it can occur when mist is present at 0 °C (32 °F) and below. 
Use freezing fog holdover times in conditions of ice crystals mixed with freezing fog or freezing mist.
To determine snowfall intensity, the Snowfall Intensities as a Function of Prevailing Visibility table (Table 57) is required. No holdover times exist if the reported visibility correlates to a “heavy” precipitation intensity. 
Use snow holdover times in conditions of very light, light, or moderate snow mixed with ice crystals.
Includes light, moderate and heavy freezing drizzle. Use light freezing rain holdover times if positive identification of freezing drizzle is not possible.
These holdover times apply to conditions of “moderate” precipitation intensity. In cases of very light or light snow mixed with light rain or drizzle, use light freezing rain holdover times. The Snowfall Intensities as a Function of Prevailing Visibility table (Table 57) is required to confirm the precipitation intensity. No holdover times exist if the reported visibility correlates to a “heavy” precipitation intensity.
No holdover time guidelines exist for this condition for 0 °C (32 °F) and below.
Heavy snow, ice pellets, moderate and heavy freezing rain, small hail and hail.
CAUTIONS
The cautions that apply to the holdover times in the table above can be found on page 11.


[bookmark: _TABLE_1C._HOLDOVER][bookmark: _Toc508704804][bookmark: _Toc43986153][bookmark: _Toc234306040][bookmark: _Toc436349419]Table 3: Holdover Times for SAE Type I Fluid on Critical Aircraft Surfaces
Composed Predominantly of Composites1
	Outside Air 
Temperature2,3
	Freezing Fog, Freezing Mist4, or Ice Crystals5
	Snow 
mixed with 
Freezing Fog6
	Very Light Snow, Snow Grains or Snow Pellets6,7
	Light 
Snow, Snow Grains or Snow Pellets6,7
	Moderate Snow, Snow Grains or Snow Pellets6,7
	Freezing 
Drizzle8
	Light 
Freezing Rain
	Moderate Snow mixed with Rain9,10
	Rain on Cold‑Soaked Wing10
	Other11

	-3 °C and above
(27 °F and above)
	0:09 - 0:16
	0:03 - 0:06
	0:12 - 0:15
	0:06 - 0:12
	0:03 - 0:06
	0:08 - 0:13
	0:02 - 0:05
	0:01 - 0:01
	0:01 - 0:05
	 

	below -3 to -6 °C
(below 27 to 21 °F)
	0:06 - 0:08
	0:02 - 0:05
	0:11 - 0:13
	0:05 - 0:11
	0:02 - 0:05
	0:05 - 0:09
	0:02 - 0:05
	CAUTION: 
No holdover time 
guidelines exist

	below -6 to -10 °C
(below 21 to 14 °F)
	0:04 - 0:08
	0:02 - 0:05
	0:09 - 0:12
	0:05 - 0:09
	0:02 - 0:05
	0:04 - 0:07
	0:02 - 0:05
	

	below -10 °C
(below 14 °F)
	0:04 - 0:07
	0:02 - 0:04
	0:07 - 0:08
	0:04 - 0:07
	0:02 - 0:04
	 
	 
	


NOTES
1. To use the holdover times in this table, ensure that the fluid and dilution being used is listed in the Type I Fluids Tested for Anti-Icing Performance and Aerodynamic Acceptance table (Table 58). Any restrictions on the use of the fluid have to be identified and applied.
3 Type I fluid / water mixture must be selected so that the freezing point of the mixture is at least 10 °C (18 °F) below outside air temperature.
Ensure that the lowest operational use temperature (LOUT) is respected.
Freezing mist is best confirmed by observation. It is never reported by METAR; however, it can occur when mist is present at 0 °C (32 °F) and below. 
Use freezing fog holdover times in conditions of ice crystals mixed with freezing fog or freezing mist.
To determine snowfall intensity, the Snowfall Intensities as a Function of Prevailing Visibility table (Table 57) is required. No holdover times exist if the reported visibility correlates to a “heavy” precipitation intensity. 
Use snow holdover times in conditions of very light, light, or moderate snow mixed with ice crystals.
Includes light, moderate and heavy freezing drizzle. Use light freezing rain holdover times if positive identification of freezing drizzle is not possible.
These holdover times apply to conditions of “moderate” precipitation intensity. In cases of very light or light snow mixed with light rain or drizzle, use light freezing rain holdover times. The Snowfall Intensities as a Function of Prevailing Visibility table (Table 57) is required to confirm the precipitation intensity. No holdover times exist if the reported visibility correlates to a “heavy” precipitation intensity.
No holdover time guidelines exist for this condition for 0 °C (32 °F) and below.
Heavy snow, ice pellets, moderate and heavy freezing rain, small hail and hail.
CAUTIONS
The cautions that apply to the holdover times in the table above can be found on page 11.
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[bookmark: _Toc234306041]HOT Guidelines for SAE Type II Fluids
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The HOT Guidelines are provided for information and guidance purposes. The HOT Guidelines on their own do not change, create, amend or permit deviations from regulatory requirements.

The HOT Guidelines may use mandatory terms such as “must”, “shall” and “is/are required” so as to convey the intent of meeting regulatory requirements and SAE Standards, where applicable. The term “should” is to be understood, unless an alternative method of achieving safety is implemented that would meet or exceed the intent of the recommendation.


[bookmark: _Hlk107238025]
[bookmark: TypeIICautions]CAUTIONS
The responsibility for the application of these data remains with the user.
The time of protection will be shortened in heavy weather conditions, heavy precipitation rates or high moisture content.
High wind velocity, jet blast or blowing snow may reduce holdover time below the lowest time stated in the range.
The holdover time may be reduced when aircraft skin temperature is lower than outside air temperature.
Fluids used during ground de/anti-icing do not provide in-flight icing protection.
This table is for departure planning only and should be used in conjunction with pre-takeoff check procedures.
Whenever frost or ice occurs on the lower surface of the wing in the area of the fuel tank, indicating a cold-soaked wing, the 50/50 dilution of Type II or IV are not to be used for the anti-icing step because fluid freezing may occur.
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[bookmark: _Toc234306042]Table 4: Generic Holdover Times for SAE Type II Fluids1
	Outside Air 
Temperature2
	Fluid 
Concentration 
Fluid/Water 
By % Volume
	Freezing Fog, Freezing Mist3, 
or Ice Crystals4
	Snow 
mixed with 
Freezing Fog5
	Snow, 
Snow Grains or Snow Pellets5,6
	Freezing 
Drizzle7
	Light 
Freezing Rain
	Moderate
Snow mixed with Rain8,9
	Rain on Cold‑Soaked Wing9
	Other10

	-3 °C and above
(27 °F and above)
	100/0
	0:55 - 1:50
	0:20 - 0:40
	0:30 - 0:55
	0:35 - 1:05
	0:25 - 0:35
	0:05 - 0:05
	0:07 - 0:45
	 

	
	75/25
	0:40 - 1:10
	0:15 - 0:25
	0:15 - 0:30
	0:25 - 0:40
	0:15 - 0:25
	0:03 - 0:03
	0:04 - 0:25
	 

	
	50/50
	0:15 - 0:30
	0:05 - 0:10
	0:07 - 0:15
	0:09 - 0:15
	0:06 - 0:09
	CAUTION: 
No holdover time 
guidelines exist

	below -3 to -8 °C
(below 27 to 18 °F)
	100/0
	0:30 - 0:45
	0:15 - 0:30
	0:20 - 0:40
	0:20 - 0:45
	0:15 - 0:20
	

	
	75/25
	0:25 - 0:55
	0:09 - 0:15
	0:10 - 0:25
	0:15 - 0:30
	0:09 - 0:20
	

	below -8 to -14 °C
(below 18 to 7 °F)
	100/0
	0:30 - 0:45
	0:10 - 0:25
	0:15 - 0:30
	0:20 - 0:4511
	0:15 - 0:2011
	

	
	75/25
	0:25 - 0:55
	0:07 - 0:15
	0:09 - 0:20
	0:15 - 0:3011
	0:09 - 0:2011
	

	below -14 to -18 °C
(below 7 to 0 °F)
	100/0
	0:15 - 0:20
	0:01 - 0:05
	0:02 - 0:07
	 
	

	below -18 to -25 °C
(below 0 to -13 °F)
	100/0
	0:15 - 0:20
	0:00 - 0:02
	0:01 - 0:03
	 
	 
	

	below -25 °C 
(below -13 °F)
	100/0
	0:15 - 0:20
	0:00 - 0:00
	0:00 - 0:01
	 
	


NOTES
1. To use the holdover times in this table, ensure that the fluid and dilution being used is listed in the Type II Fluids Tested for Anti-Icing Performance and Aerodynamic Acceptance table (Table 59). Any restrictions on the use of the fluid have to be identified and applied.
1. Ensure that the lowest operational use temperature (LOUT) is respected. Consider use of Type I fluid when Type II fluid cannot be used.
Freezing mist is best confirmed by observation. It is never reported by METAR; however, it can occur when mist is present at 0 °C (32 °F) and below. 
Use freezing fog holdover times in conditions of ice crystals mixed with freezing fog or freezing mist.
To determine snowfall intensity, the Snowfall Intensities as a Function of Prevailing Visibility table (Table 57) is required. No holdover times exist if the reported visibility correlates to a “heavy” precipitation intensity. 
Use snow holdover times in conditions of very light, light, or moderate snow mixed with ice crystals.
Includes light, moderate and heavy freezing drizzle. Use light freezing rain holdover times if positive identification of freezing drizzle is not possible.
These holdover times apply to conditions of “moderate” precipitation intensity. In cases of very light or light snow mixed with light rain or drizzle, use light freezing rain holdover times. The Snowfall Intensities as a Function of Prevailing Visibility table (Table 57) is required to confirm the precipitation intensity. No holdover times exist if the reported visibility correlates to a “heavy” precipitation intensity.
No holdover time guidelines exist for this condition for 0 °C (32 °F) and below.
Heavy snow, ice pellets, moderate and heavy freezing rain, small hail and hail.
No holdover time guidelines exist for this condition below -10 °C (14 °F).
CAUTIONS
The cautions that apply to the holdover times in the table above can be found on page 14.

[bookmark: _TABLE_2A._TYPE][bookmark: _TABLE_2B._Type][bookmark: _Toc508704807][bookmark: _Toc43986155][bookmark: _Toc234306043][bookmark: _Toc425184863][bookmark: _Toc436349422]Table 5: Type II Holdover Times for ABAX ECOWING AD-2
	Outside Air 
Temperature1
	Fluid 
Concentration 
Fluid/Water 
By % Volume
	Freezing Fog, Freezing Mist2, or Ice Crystals3
	Snow 
mixed with 
Freezing Fog4
	Very Light Snow, Snow Grains or Snow Pellets4,5
	Light 
Snow, Snow Grains or Snow Pellets4,5
	Moderate Snow, Snow Grains or Snow Pellets4,5
	Freezing 
Drizzle6
	Light 
Freezing Rain
	Moderate
Snow mixed with Rain7,8
	Rain on 
Cold‑Soaked Wing8
	Other9

	-3 °C and above
(27 °F and above)
	100/0
	1:20 - 3:00
	0:30 - 0:55
	2:25 - 2:55
	1:15 - 2:25
	0:40 - 1:15
	0:40 - 1:40
	0:30 - 0:45
	0:07 - 0:07
	0:09 - 1:25
	 

	
	75/25
	1:15 - 1:25
	0:20 - 0:40
	1:45 - 2:10
	0:55 - 1:45
	0:25 - 0:55
	0:35 - 1:05
	0:20 - 0:30
	0:03 - 0:03
	0:04 - 0:50
	 

	
	50/50
	0:15 - 0:30
	0:05 - 0:10
	0:35 - 0:40
	0:15 - 0:35
	0:07 - 0:15
	0:09 - 0:15
	0:06 - 0:09
	CAUTION: 
No holdover time 
guidelines exist

	below -3 to -8 °C
(below 27 to 18 °F)
	100/0
	0:45 - 2:30
	0:25 - 0:45
	2:00 - 2:25
	1:00 - 2:00
	0:30 - 1:00
	0:25 - 1:10
	0:20 - 0:30
	

	
	75/25
	0:35 - 1:55
	0:20 - 0:35
	1:40 - 2:05
	0:50 - 1:40
	0:25 - 0:50
	0:15 - 0:55
	0:20 - 0:35
	

	below -8 to -14 °C
(below 18 to 7 °F)
	100/0
	0:45 - 2:30
	0:20 - 0:40
	1:45 - 2:05
	0:55 - 1:45
	0:30 - 0:55
	0:25 - 1:1010
	0:20 - 0:3010
	

	
	75/25
	0:35 - 1:55
	0:20 - 0:35
	1:35 - 2:00
	0:50 - 1:35
	0:25 - 0:50
	0:15 - 0:5510
	0:20 - 0:3510
	

	below -14 to -18 °C
(below 7 to 0 °F)
	100/0
	0:15 - 0:40
	0:01 - 0:05
	0:20 - 0:30
	0:07 - 0:20
	0:02 - 0:07
	
	

	below -18 to -25 °C
(below 0 to -13 °F)
	100/0
	0:15 - 0:40
	0:00 - 0:02
	0:09 - 0:15
	0:03 - 0:09
	0:01 - 0:03
	
	

	below -25 to -27 °C
(below -13 to -17 °F)
	100/0
	0:15 - 0:40
	0:00 - 0:00
	0:05 - 0:07
	0:01 - 0:05
	0:00 - 0:01
	
	


NOTES
1. Ensure that the lowest operational use temperature (LOUT) is respected. Consider use of Type I fluid when Type II fluid cannot be used.
1. Freezing mist is best confirmed by observation. It is never reported by METAR; however, it can occur when mist is present at 0 °C (32 °F) and below. 
1. Use freezing fog holdover times in conditions of ice crystals mixed with freezing fog or freezing mist.
1. To determine snowfall intensity, the Snowfall Intensities as a Function of Prevailing Visibility table (Table 57) is required. No holdover times exist if the reported visibility correlates to a “heavy” precipitation intensity.
1. Use snow holdover times in conditions of very light, light, or moderate snow mixed with ice crystals.
1. Includes light, moderate and heavy freezing drizzle. Use light freezing rain holdover times if positive identification of freezing drizzle is not possible.
1. These holdover times apply to conditions of “moderate” precipitation intensity. In cases of very light or light snow mixed with light rain or drizzle, use light freezing rain holdover times. The Snowfall Intensities as a Function of Prevailing Visibility table (Table 57) is required to confirm the precipitation intensity. No holdover times exist if the reported visibility correlates to a “heavy” precipitation intensity.
1. No holdover time guidelines exist for this condition for 0 °C (32 °F) and below.
1. Heavy snow, ice pellets, moderate and heavy freezing rain, small hail and hail.
1. No holdover time guidelines exist for this condition below -10 °C (14 °F).
CAUTIONS
The cautions that apply to the holdover times in the table above can be found on page 14.


[bookmark: _Toc508704808][bookmark: _Toc43986156][bookmark: _Toc234306044]Table 6: Type II Holdover Times for Aviation Xi’an High-Tech Cleanwing II
	Outside Air 
Temperature1
	Fluid 
Concentration 
Fluid/Water 
By % Volume
	Freezing Fog, Freezing Mist2, or Ice Crystals3
	Snow 
mixed with 
Freezing Fog4
	Very Light Snow, Snow Grains or Snow Pellets4,5
	Light 
Snow, Snow Grains or Snow Pellets4,5
	Moderate Snow, Snow Grains or Snow Pellets4,5
	Freezing 
Drizzle6
	Light 
Freezing Rain
	Moderate
Snow mixed with Rain7,8
	Rain on 
Cold‑Soaked Wing8
	Other9

	-3 °C and above
(27 °F and above)
	100/0
	0:55 - 1:50
	0:20 - 0:40
	1:35 - 1:55
	0:55 - 1:35
	0:30 - 0:55
	0:35 - 1:05
	0:25 - 0:35
	0:07 - 0:07
	0:10 - 0:55
	 

	
	75/25
	0:50 - 1:20
	0:15 - 0:25
	1:05 - 1:15
	0:35 - 1:05
	0:20 - 0:35
	0:35 - 1:00
	0:20 - 0:30
	0:05 - 0:05
	0:07 - 0:50
	 

	
	50/50
	0:35 - 1:00
	0:10 - 0:20
	0:50 - 1:05
	0:25 - 0:50
	0:15 - 0:25
	0:20 - 0:40
	0:10 - 0:20
	CAUTION: 
No holdover time 
guidelines exist

	below -3 to -8 °C
(below 27 to 18 °F)
	100/0
	0:45 - 1:50
	0:15 - 0:30
	1:20 - 1:35
	0:40 - 1:20
	0:25 - 0:40
	0:30 - 0:55
	0:20 - 0:25
	

	
	75/25
	0:40 - 1:45
	0:15 - 0:25
	1:05 - 1:15
	0:35 - 1:05
	0:20 - 0:35
	0:35 - 0:40
	0:20 - 0:25
	

	below -8 to -14 °C
(below 18 to 7 °F)
	100/0
	0:45 - 1:50
	0:15 - 0:25
	1:05 - 1:20
	0:35 - 1:05
	0:20 - 0:35
	0:30 - 0:5510
	0:20 - 0:2510
	

	
	75/25
	0:40 - 1:45
	0:15 - 0:25
	1:05 - 1:15
	0:35 - 1:05
	0:20 - 0:35
	0:35 - 0:4010
	0:20 - 0:2510
	

	below -14 to -18 °C
(below 7 to 0 °F)
	100/0
	0:20 - 0:50
	0:09 - 0:20
	0:45 - 1:00
	0:25 - 0:45
	0:15 - 0:25
	
	

	below -18 to -25 °C
(below 0 to -13 °F)
	100/0
	0:20 - 0:50
	0:05 - 0:10
	0:30 - 0:35
	0:15 - 0:30
	0:07 - 0:15
	
	


NOTES
1. Ensure that the lowest operational use temperature (LOUT) is respected. Consider use of Type I fluid when Type II fluid cannot be used.
1. Freezing mist is best confirmed by observation. It is never reported by METAR; however, it can occur when mist is present at 0 °C (32 °F) and below. 
1. Use freezing fog holdover times in conditions of ice crystals mixed with freezing fog or freezing mist.
1. To determine snowfall intensity, the Snowfall Intensities as a Function of Prevailing Visibility table (Table 57) is required. No holdover times exist if the reported visibility correlates to a “heavy” precipitation intensity. 
1. Use snow holdover times in conditions of very light, light, or moderate snow mixed with ice crystals.
1. Includes light, moderate and heavy freezing drizzle. Use light freezing rain holdover times if positive identification of freezing drizzle is not possible.
1. These holdover times apply to conditions of “moderate” precipitation intensity. In cases of very light or light snow mixed with light rain or drizzle, use light freezing rain holdover times. The Snowfall Intensities as a Function of Prevailing Visibility table (Table 57) is required to confirm the precipitation intensity. No holdover times exist if the reported visibility correlates to a “heavy” precipitation intensity.
1. No holdover time guidelines exist for this condition for 0 °C (32 °F) and below.
1. Heavy snow, ice pellets, moderate and heavy freezing rain, small hail and hail.
1. No holdover time guidelines exist for this condition below -10 °C (14 °F).
CAUTIONS
The cautions that apply to the holdover times in the table above can be found on page 14.


[bookmark: _TABLE_2C._Type][bookmark: _TABLE_2D._TYPE_1][bookmark: _Toc425184864][bookmark: _Toc436349423][bookmark: _Toc508704810][bookmark: _Toc43986158][bookmark: _Toc234306045]Table 7: Type II Holdover Times for Clariant Safewing MP II FLIGHT
	Outside Air 
Temperature1
	Fluid 
Concentration 
Fluid/Water 
By % Volume
	Freezing Fog, Freezing Mist2, or Ice Crystals3
	Snow 
mixed with 
Freezing Fog4
	Very Light Snow, Snow Grains or Snow Pellets4,5
	Light 
Snow, Snow Grains or Snow Pellets4,5
	Moderate Snow, Snow Grains or Snow Pellets4,5
	Freezing 
Drizzle6
	Light 
Freezing Rain
	Moderate
Snow mixed with Rain7,8
	Rain on 
Cold‑Soaked Wing8
	Other9

	-3 °C and above
(27 °F and above)
	100/0
	3:30 - 4:00
	0:45 - 1:10
	2:35 - 3:00
	1:35 - 2:35
	1:00 - 1:35
	1:20 - 2:00
	0:45 - 1:25
	0:08 - 0:08
	0:10 - 1:30
	 

	
	75/25
	1:50 - 2:45
	0:30 - 1:00
	2:35 - 3:00
	1:20 - 2:35
	0:40 - 1:20
	1:10 - 1:30
	0:30 - 0:55
	0:04 - 0:04
	0:06 - 0:50
	 

	
	50/50
	0:55 - 1:45
	0:09 - 0:20
	0:45 - 0:55
	0:25 - 0:45
	0:10 - 0:25
	0:20 - 0:30
	0:10 - 0:15
	CAUTION: 
No holdover time 
guidelines exist

	below -3 to -8 °C
(below 27 to 18 °F)
	100/0
	0:55 - 1:45
	0:35 - 1:00
	2:05 - 2:30
	1:15 - 2:05
	0:45 - 1:15
	0:35 - 1:30
	0:25 - 0:45
	

	
	75/25
	0:25 - 1:05
	0:20 - 0:40
	1:45 - 2:10
	0:55 - 1:45
	0:30 - 0:55
	0:25 - 1:10
	0:20 - 0:35
	

	below -8 to -14 °C
(below 18 to 7 °F)
	100/0
	0:55 - 1:45
	0:30 - 0:50
	1:50 - 2:10
	1:05 - 1:50
	0:40 - 1:05
	0:35 - 1:3010
	0:25 - 0:4510
	

	
	75/25
	0:25 - 1:05
	0:15 - 0:30
	1:20 - 1:40
	0:40 - 1:20
	0:20 - 0:40
	0:25 - 1:1010
	0:20 - 0:3510
	

	below -14 to -18 °C
(below 7 to 0 °F)
	100/0
	0:30 - 0:50
	0:06 - 0:20
	1:10 - 1:40
	0:25 - 1:10
	0:08 - 0:25
	
	

	below -18 to -25 °C
(below 0 to -13 °F)
	100/0
	0:30 - 0:50
	0:02 - 0:07
	0:30 - 0:40
	0:10 - 0:30
	0:03 - 0:10
	
	

	below -25 to -29 °C
(below -13 to -20 °F)
	100/0
	0:30 - 0:50
	0:01 - 0:05
	0:20 - 0:30
	0:07 - 0:20
	0:02 - 0:07
	
	


NOTES
1. Ensure that the lowest operational use temperature (LOUT) is respected. Consider use of Type I fluid when Type II fluid cannot be used.
1. Freezing mist is best confirmed by observation. It is never reported by METAR; however, it can occur when mist is present at 0 °C (32 °F) and below. 
1. Use freezing fog holdover times in conditions of ice crystals mixed with freezing fog or freezing mist.
1. To determine snowfall intensity, the Snowfall Intensities as a Function of Prevailing Visibility table (Table 57) is required. No holdover times exist if the reported visibility correlates to a “heavy” precipitation intensity. 
1. Use snow holdover times in conditions of very light, light, or moderate snow mixed with ice crystals.
1. Includes light, moderate and heavy freezing drizzle. Use light freezing rain holdover times if positive identification of freezing drizzle is not possible.
1. These holdover times apply to conditions of “moderate” precipitation intensity. In cases of very light or light snow mixed with light rain or drizzle, use light freezing rain holdover times. The Snowfall Intensities as a Function of Prevailing Visibility table (Table 57) is required to confirm the precipitation intensity. No holdover times exist if the reported visibility correlates to a “heavy” precipitation intensity.
1. No holdover time guidelines exist for this condition for 0 °C (32 °F) and below.
1. Heavy snow, ice pellets, moderate and heavy freezing rain, small hail and hail.
1. No holdover time guidelines exist for this condition below -10 °C (14 °F).
CAUTIONS
The cautions that apply to the holdover times in the table above can be found on page 14.


[bookmark: _TABLE_2E._TYPE][bookmark: _Toc436349425][bookmark: _Toc508704812][bookmark: _Toc43986160][bookmark: _Toc234306046]Table 8: Type II Holdover Times for Cryotech Polar Guard® II
	Outside Air 
Temperature1
	Fluid 
Concentration 
Fluid/Water 
By % Volume
	Freezing Fog, Freezing Mist2, or Ice Crystals3
	Snow 
mixed with 
Freezing Fog4
	Very Light Snow, Snow Grains or Snow Pellets4,5
	Light 
Snow, Snow Grains or Snow Pellets4,5
	Moderate Snow, Snow Grains or Snow Pellets4,5
	Freezing 
Drizzle6
	Light 
Freezing Rain
	Moderate
Snow mixed with Rain7,8
	Rain on 
Cold‑Soaked Wing8
	Other9

	-3 °C and above
(27 °F and above)
	100/0
	2:50 - 4:00
	0:50 - 1:25
	3:00 - 3:00
	1:55 - 3:00
	1:05 - 1:55
	1:35 - 2:00
	1:15 - 1:30
	0:10 - 0:10
	0:15 - 2:00
	 

	
	75/25
	2:30 - 4:00
	0:30 - 1:05
	3:00 - 3:00
	1:25 - 3:00
	0:40 - 1:25
	1:40 - 2:00
	0:40 - 1:10
	0:07 - 0:07
	0:09 - 1:40
	 

	
	50/50
	0:50 - 1:25
	0:07 - 0:20
	1:10 - 1:35
	0:25 - 1:10
	0:10 - 0:25
	0:20 - 0:45
	0:09 - 0:20
	CAUTION: 
No holdover time 
guidelines exist

	below -3 to -8 °C
(below 27 to 18 °F)
	100/0
	0:55 - 2:30
	0:35 - 1:05
	2:25 - 2:50
	1:25 - 2:25
	0:50 - 1:25
	0:35 - 1:35
	0:35 - 0:45
	

	
	75/25
	0:40 - 1:30
	0:25 - 0:50
	2:20 - 3:00
	1:05 - 2:20
	0:30 - 1:05
	0:25 - 1:05
	0:35 - 0:45
	

	below -8 to -14 °C
(below 18 to 7 °F)
	100/0
	0:55 - 2:30
	0:30 - 0:50
	2:00 - 2:20
	1:10 - 2:00
	0:40 - 1:10
	0:35 - 1:3510
	0:35 - 0:4510
	

	
	75/25
	0:40 - 1:30
	0:20 - 0:45
	2:00 - 2:30
	0:55 - 2:00
	0:25 - 0:55
	0:25 - 1:0510
	0:35 - 0:4510
	

	below -14 to -18 °C
(below 7 to 0 °F)
	100/0
	0:25 - 0:50
	0:08 - 0:25
	1:35 - 2:15
	0:35 - 1:35
	0:10 - 0:35
	
	

	below -18 to -25 °C
(below 0 to -13 °F)
	100/0
	0:25 - 0:50
	0:03 - 0:10
	0:40 - 0:55
	0:15 - 0:40
	0:04 - 0:15
	
	

	below -25 to -30.5 °C
(below -13 to -23 °F)
	100/0
	0:25 - 0:50
	0:02 - 0:05
	0:25 - 0:30
	0:07 - 0:25
	0:02 - 0:07
	
	


NOTES
1. Ensure that the lowest operational use temperature (LOUT) is respected. Consider use of Type I fluid when Type II fluid cannot be used.
1. Freezing mist is best confirmed by observation. It is never reported by METAR; however, it can occur when mist is present at 0 °C (32 °F) and below. 
1. Use freezing fog holdover times in conditions of ice crystals mixed with freezing fog or freezing mist. 
1. To determine snowfall intensity, the Snowfall Intensities as a Function of Prevailing Visibility table (Table 57) is required. No holdover times exist if the reported visibility correlates to a “heavy” precipitation intensity. 
1. Use snow holdover times in conditions of very light, light, or moderate snow mixed with ice crystals.
1. Includes light, moderate and heavy freezing drizzle. Use light freezing rain holdover times if positive identification of freezing drizzle is not possible.
1. These holdover times apply to conditions of “moderate” precipitation intensity. In cases of very light or light snow mixed with light rain or drizzle, use light freezing rain holdover times. The Snowfall Intensities as a Function of Prevailing Visibility table (Table 57) is required to confirm the precipitation intensity. No holdover times exist if the reported visibility correlates to a “heavy” precipitation intensity.
1. No holdover time guidelines exist for this condition for 0 °C (32 °F) and below.
1. Heavy snow, ice pellets, moderate and heavy freezing rain, small hail and hail.
1. No holdover time guidelines exist for this condition below -10 °C (14 °F).
CAUTIONS
The cautions that apply to the holdover times in the table above can be found on page 14.


[bookmark: _Toc234306047]Table 9: Type II Holdover Times for ESSPO CHEMICALS D.O.O Nordwing PG2
	Outside Air 
Temperature1
	Fluid 
Concentration 
Fluid/Water 
By % Volume
	Freezing Fog, Freezing Mist2, or Ice Crystals3
	Snow 
mixed with 
Freezing Fog4
	Very Light Snow, Snow Grains or Snow Pellets4,5
	Light 
Snow, Snow Grains or Snow Pellets4,5
	Moderate Snow, Snow Grains or Snow Pellets4,5
	Freezing 
Drizzle6
	Light 
Freezing Rain
	Moderate
Snow mixed with Rain7,8
	Rain on 
Cold‑Soaked Wing8
	Other9

	-3 °C and above
(27 °F and above)
	100/0
	1:40 - 3:10
	0:30 - 1:00
	2:35 - 3:00
	1:20 - 2:35
	0:40 - 1:20
	1:05 - 1:50
	0:50 - 1:05
	0:15 - 0:15
	0:20 - 1:45
	 

	
	75/25
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	 

	
	50/50
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	CAUTION: 
No holdover time 
guidelines exist

	below -3 to -8 °C
(below 27 to 18 °F)
	100/0
	1:05 - 2:20
	0:25 - 0:45
	2:00 - 2:30
	1:00 - 2:00
	0:30 - 1:00
	0:50 - 1:30
	0:25 - 0:50
	

	
	75/25
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	

	below -8 to -14 °C
(below 18 to 7 °F)
	100/0
	1:05 - 2:20
	0:20 - 0:40
	1:45 - 2:10
	0:50 - 1:45
	0:25 - 0:50
	0:50 - 1:3010
	0:25 - 0:5010
	

	
	75/25
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	

	below -14 to -18 °C
(below 7 to 0 °F)
	100/0
	0:20 - 0:35
	0:10 - 0:25
	1:15 - 1:40
	0:30 - 1:15
	0:15 - 0:30
	
	

	below -18 to -25 °C
(below 0 to -13 °F)
	100/0
	0:20 - 0:35
	0:06 - 0:15
	0:50 - 1:05
	0:20 - 0:50
	0:08 - 0:20
	
	

	below -25 to -30 °C
(below -13 to -22 °F)
	100/0
	0:20 - 0:30
	0:03 - 0:07
	0:25 - 0:30
	0:09 - 0:25
	0:04 - 0:09
	
	


NOTES
1. Ensure that the lowest operational use temperature (LOUT) is respected. Consider use of Type I fluid when Type II fluid cannot be used.
1. Freezing mist is best confirmed by observation. It is never reported by METAR; however, it can occur when mist is present at 0 °C (32 °F) and below. 
1. Use freezing fog holdover times in conditions of ice crystals mixed with freezing fog or freezing mist. 
1. To determine snowfall intensity, the Snowfall Intensities as a Function of Prevailing Visibility table (Table 57) is required. No holdover times exist if the reported visibility correlates to a “heavy” precipitation intensity. 
1. Use snow holdover times in conditions of very light, light, or moderate snow mixed with ice crystals.
1. Includes light, moderate and heavy freezing drizzle. Use light freezing rain holdover times if positive identification of freezing drizzle is not possible.
1. These holdover times apply to conditions of “moderate” precipitation intensity. In cases of very light or light snow mixed with light rain or drizzle, use light freezing rain holdover times. The Snowfall Intensities as a Function of Prevailing Visibility table (Table 57) is required to confirm the precipitation intensity. No holdover times exist if the reported visibility correlates to a “heavy” precipitation intensity.
1. No holdover time guidelines exist for this condition for 0 °C (32 °F) and below.
1. Heavy snow, ice pellets, moderate and heavy freezing rain, small hail and hail.
1. No holdover time guidelines exist for this condition below -10 °C (14 °F).
CAUTIONS
The cautions that apply to the holdover times in the table above can be found on page 14.


[bookmark: _TABLE_2F._TYPE][bookmark: _TABLE_2G._TYPE][bookmark: _Toc436349427][bookmark: _Toc508704814][bookmark: _Toc43986162][bookmark: _Toc234306048]Table 10: Type II Holdover Times for Kilfrost ABC-K Plus
	Outside Air 
Temperature1
	Fluid 
Concentration 
Fluid/Water 
By % Volume
	Freezing Fog, Freezing Mist2, 
or Ice Crystals3
	Snow 
mixed with 
Freezing Fog4
	Snow, 
Snow Grains or Snow Pellets4,5
	Freezing 
Drizzle6
	Light 
Freezing Rain
	Moderate
Snow mixed with Rain7,8
	Rain on Cold‑Soaked Wing8
	Other9

	-3 °C and above
(27 °F and above)
	100/0
	2:15 - 3:45
	0:45 - 1:15
	1:00 - 1:40
	1:50 - 2:00
	1:00 - 1:25
	0:15 - 0:15
	0:20 - 2:00
	 

	
	75/25
	1:40 - 2:30
	0:25 - 0:45
	0:30 - 1:00
	1:25 - 2:00
	0:50 - 1:10
	0:10 - 0:10
	0:15 - 2:00
	 

	
	50/50
	0:35 - 1:05
	0:05 - 0:10
	0:07 - 0:15
	0:20 - 0:30
	0:10 - 0:15
	CAUTION: 
No holdover time 
guidelines exist

	below -3 to -8 °C
(below 27 to 18 °F)
	100/0
	0:30 - 1:05
	0:40 - 1:10
	0:55 - 1:30
	0:25 - 1:00
	0:15 - 0:35
	

	
	75/25
	0:25 - 1:25
	0:25 - 0:45
	0:30 - 1:00
	0:20 - 0:55
	0:09 - 0:30
	

	below -8 to -14 °C
(below 18 to 7 °F)
	100/0
	0:30 - 1:05
	0:40 - 1:05
	0:50 - 1:25
	0:25 - 1:0010
	0:15 - 0:3510
	

	
	75/25
	0:25 - 1:25
	0:25 - 0:45
	0:30 - 1:00
	0:20 - 0:5510
	0:09 - 0:3010
	

	below -14 to -18 °C
(below 7 to 0 °F)
	100/0
	0:30 - 0:55
	0:01 - 0:05
	0:02 - 0:07
	 
	

	below -18 to -25 °C
(below 0 to -13 °F)
	100/0
	0:30 - 0:55
	0:00 - 0:02
	0:01 - 0:03
	 
	 
	

	below -25 to -29 °C
(below -13 to -20 °F)
	100/0
	0:30 - 0:55
	0:00 - 0:00
	0:00 - 0:01
	 
	


NOTES
1. Ensure that the lowest operational use temperature (LOUT) is respected. Consider use of Type I fluid when Type II fluid cannot be used.
Freezing mist is best confirmed by observation. It is never reported by METAR; however, it can occur when mist is present at 0 °C (32 °F) and below. 
Use freezing fog holdover times in conditions of ice crystals mixed with freezing fog or freezing mist.
To determine snowfall intensity, the Snowfall Intensities as a Function of Prevailing Visibility table (Table 57) is required. No holdover times exist if the reported visibility correlates to a “heavy” precipitation intensity. 
Use snow holdover times in conditions of very light, light, or moderate snow mixed with ice crystals.
Includes light, moderate and heavy freezing drizzle. Use light freezing rain holdover times if positive identification of freezing drizzle is not possible.
These holdover times apply to conditions of “moderate” precipitation intensity. In cases of very light or light snow mixed with light rain or drizzle, use light freezing rain holdover times. The Snowfall Intensities as a Function of Prevailing Visibility table (Table 57) is required to confirm the precipitation intensity. No holdover times exist if the reported visibility correlates to a “heavy” precipitation intensity.
No holdover time guidelines exist for this condition for 0 °C (32 °F) and below.
Heavy snow, ice pellets, moderate and heavy freezing rain, small hail and hail.
No holdover time guidelines exist for this condition below -10 °C (14 °F).
CAUTIONS
[bookmark: _Hlk105395598]The cautions that apply to the holdover times in the table above can be found on page 14.


[bookmark: _TABLE_2H._TYPE][bookmark: _TABLE_2I._TYPE][bookmark: _Toc234306049][bookmark: _Toc436349429][bookmark: _Toc508704815][bookmark: _Toc43986164]Table 11: Type II Holdover Times for Kilfrost Ice Clear II
	Outside Air 
Temperature1
	Fluid 
Concentration 
Fluid/Water 
By % Volume
	Freezing Fog, Freezing Mist2, or Ice Crystals3
	Snow 
mixed with 
Freezing Fog4
	Very Light Snow, Snow Grains or Snow Pellets4,5
	Light 
Snow, Snow Grains or Snow Pellets4,5
	Moderate Snow, Snow Grains or Snow Pellets4,5
	Freezing 
Drizzle6
	Light 
Freezing Rain
	Moderate
Snow mixed with Rain7,8
	Rain on 
Cold‑Soaked Wing8
	Other9

	-3 °C and above
(27 °F and above)
	100/0
	1:25 - 2:25
	0:30 - 1:00
	2:25 - 2:55
	1:20 - 2:25
	0:40 - 1:20
	1:00 - 1:35
	0:40 - 1:05
	0:10 - 0:10
	0:15 - 2:00
	 

	
	75/25
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	 

	
	50/50
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	CAUTION: 
No holdover time 
guidelines exist

	below -3 to -8 °C
(below 27 to 18 °F)
	100/0
	1:05 - 2:35
	0:30 - 0:50
	2:10 - 2:35
	1:10 - 2:10
	0:40 - 1:10
	0:30 - 1:15
	0:35 - 0:55
	

	
	75/25
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	

	below -8 to -14 °C
(below 18 to 7 °F)
	100/0
	1:05 - 2:35
	0:25 - 0:50
	2:00 - 2:25
	1:05 - 2:00
	0:35 - 1:05
	0:30 - 1:1510
	0:35 - 0:5510
	

	
	75/25
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	

	below -14 to -18 °C
(below 7 to 0 °F)
	100/0
	0:35 - 0:45
	0:10 - 0:20
	0:55 - 1:05
	0:30 - 0:55
	0:15 - 0:30
	
	

	below -18 to -25 °C
(below 0 to -13 °F)
	100/0
	0:35 - 0:45
	0:06 - 0:10
	0:30 - 0:35
	0:15 - 0:30
	0:08 - 0:15
	
	

	below -25 to -28 °C
(below -13 to -18 °F)
	100/0
	0:35 - 0:45
	0:05 - 0:09
	0:25 - 0:30
	0:10 - 0:25
	0:06 - 0:10
	
	


NOTES
1. Ensure that the lowest operational use temperature (LOUT) is respected. Consider use of Type I fluid when Type II fluid cannot be used.
Freezing mist is best confirmed by observation. It is never reported by METAR; however, it can occur when mist is present at 0 °C (32 °F) and below. 
Use freezing fog holdover times in conditions of ice crystals mixed with freezing fog or freezing mist.
To determine snowfall intensity, the Snowfall Intensities as a Function of Prevailing Visibility table (Table 57) is required. No holdover times exist if the reported visibility correlates to a “heavy” precipitation intensity. 
Use snow holdover times in conditions of very light, light, or moderate snow mixed with ice crystals.
Includes light, moderate and heavy freezing drizzle. Use light freezing rain holdover times if positive identification of freezing drizzle is not possible.
These holdover times apply to conditions of “moderate” precipitation intensity. In cases of very light or light snow mixed with light rain or drizzle, use light freezing rain holdover times. The Snowfall Intensities as a Function of Prevailing Visibility table (Table 57) is required to confirm the precipitation intensity. No holdover times exist if the reported visibility correlates to a “heavy” precipitation intensity.
No holdover time guidelines exist for this condition for 0 °C (32 °F) and below.
Heavy snow, ice pellets, moderate and heavy freezing rain, small hail and hail.
No holdover time guidelines exist for this condition below -10 °C (14 °F).
CAUTIONS
The cautions that apply to the holdover times in the table above can be found on page 14.


[bookmark: _Toc234306050]Table 12: Type II Holdover Times for LNT Solutions P250
	Outside Air 
Temperature1
	Fluid 
Concentration 
Fluid/Water 
By % Volume
	Freezing Fog, Freezing Mist2, or Ice Crystals3
	Snow 
mixed with 
Freezing Fog4
	Very Light Snow, Snow Grains or Snow Pellets4,5
	Light 
Snow, Snow Grains or Snow Pellets4,5
	Moderate Snow, Snow Grains or Snow Pellets4,5
	Freezing 
Drizzle6
	Light 
Freezing Rain
	Moderate
Snow mixed with Rain7,8
	Rain on 
Cold‑Soaked Wing8
	Other9

	-3 °C and above
(27 °F and above)
	100/0
	3:00 - 4:00
	0:40 - 1:20
	3:00 - 3:00
	1:50 - 3:00
	0:50 - 1:50
	1:50 - 2:00
	1:00 - 1:30
	0:20 - 0:20
	0:30 - 1:50
	 

	
	75/25
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	 

	
	50/50
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	CAUTION: 
No holdover time 
guidelines exist

	below -3 to -8 °C
(below 27 to 18 °F)
	100/0
	0:55 - 2:45
	0:30 - 1:05
	2:55 - 3:00
	1:25 - 2:55
	0:40 - 1:25
	0:35 - 1:45
	0:25 - 0:45
	

	
	75/25
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	

	below -8 to -14 °C
(below 18 to 7 °F)
	100/0
	0:55 - 2:45
	0:25 - 0:50
	2:30 - 3:00
	1:10 - 2:30
	0:35 - 1:10
	0:35 - 1:4510
	0:25 - 0:4510
	

	
	75/25
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	

	below -14 to -18 °C
(below 7 to 0 °F)
	100/0
	0:20 - 0:30
	0:01 - 0:05
	0:20 - 0:30
	0:07 - 0:20
	0:02 - 0:07
	
	

	below -18 to -25 °C
(below 0 to -13 °F)
	100/0
	0:20 - 0:30
	0:00 - 0:02
	0:09 - 0:15
	0:03 - 0:09
	0:01 - 0:03
	
	

	below -25 to -29 °C
(below -13 to -20 °F)
	100/0
	0:20 - 0:30
	0:00 - 0:00
	0:05 - 0:07
	0:01 - 0:05
	0:00 - 0:01
	
	


NOTES
1. Ensure that the lowest operational use temperature (LOUT) is respected. Consider use of Type I fluid when Type II fluid cannot be used.
Freezing mist is best confirmed by observation. It is never reported by METAR; however, it can occur when mist is present at 0 °C (32 °F) and below. 
Use freezing fog holdover times in conditions of ice crystals mixed with freezing fog or freezing mist.
To determine snowfall intensity, the Snowfall Intensities as a Function of Prevailing Visibility table (Table 57) is required. No holdover times exist if the reported visibility correlates to a “heavy” precipitation intensity. 
Use snow holdover times in conditions of very light, light, or moderate snow mixed with ice crystals.
Includes light, moderate and heavy freezing drizzle. Use light freezing rain holdover times if positive identification of freezing drizzle is not possible.
These holdover times apply to conditions of “moderate” precipitation intensity. In cases of very light or light snow mixed with light rain or drizzle, use light freezing rain holdover times. The Snowfall Intensities as a Function of Prevailing Visibility table (Table 57) is required to confirm the precipitation intensity. No holdover times exist if the reported visibility correlates to a “heavy” precipitation intensity.
No holdover time guidelines exist for this condition for 0 °C (32 °F) and below.
Heavy snow, ice pellets, moderate and heavy freezing rain, small hail and hail.
No holdover time guidelines exist for this condition below -10 °C (14 °F).
CAUTIONS
The cautions that apply to the holdover times in the table above can be found on page 14.


[bookmark: _Toc106885005][bookmark: _Toc234306051]Table 13: Type II Holdover Times for MKS DevO Chemicals COREICEPHOB TYPE II
	Outside Air 
Temperature1
	Fluid 
Concentration 
Fluid/Water 
By % Volume
	Freezing Fog, Freezing Mist2, or Ice Crystals3
	Snow 
mixed with 
Freezing Fog4
	Very Light Snow, Snow Grains or Snow Pellets4,5
	Light 
Snow, Snow Grains or Snow Pellets4,5
	Moderate Snow, Snow Grains or Snow Pellets4,5
	Freezing 
Drizzle6
	Light 
Freezing Rain
	Moderate
Snow mixed with Rain7,8
	Rain on 
Cold‑Soaked Wing8
	Other9

	-3 °C and above
(27 °F and above)
	100/0
	1:55 - 2:45
	0:30 - 1:00
	2:35 - 3:00
	1:25 - 2:35
	0:40 - 1:25
	1:10 - 2:00
	0:45 - 1:00
	0:09 - 0:09
	0:15 - 1:35
	 

	
	75/25
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	 

	
	50/50
	1:05 - 1:45
	0:15 - 0:35
	1:35 - 1:55
	0:45 - 1:35
	0:25 - 0:45
	0:50 - 1:15
	0:25 - 0:30
	CAUTION: 
No holdover time 
guidelines exist

	below -3 to -8 °C
(below 27 to 18 °F)
	100/0
	0:45 - 1:25
	0:25 - 0:45
	1:50 - 2:15
	1:00 - 1:50
	0:30 - 1:00
	0:30 - 1:10
	0:25 - 0:35
	

	
	75/25
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	

	below -8 to -14 °C
(below 18 to 7 °F)
	100/0
	0:45 - 1:25
	0:20 - 0:35
	1:30 - 1:50
	0:50 - 1:30
	0:25 - 0:50
	0:30 - 1:1010
	0:25 - 0:3510
	

	
	75/25
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	

	below -14 to -18 °C
(below 7 to 0 °F)
	100/0
	0:15 - 0:25
	0:08 - 0:15
	0:35 - 0:40
	0:20 - 0:35
	0:10 - 0:20
	
	

	below -18 to -25 °C
(below 0 to -13 °F)
	100/0
	0:15 - 0:25
	0:03 - 0:05
	0:15 - 0:15
	0:07 - 0:15
	0:04 - 0:07
	
	

	below -25 to -27 °C
(below -13 to -17 °F)
	100/0
	0:15 - 0:25
	0:02 - 0:04
	0:10 - 0:10
	0:05 - 0:10
	0:03 - 0:05
	
	


NOTES
1 Ensure that the lowest operational use temperature (LOUT) is respected. Consider use of Type I fluid when Type II fluid cannot be used.
2 Freezing mist is best confirmed by observation. It is never reported by METAR; however, it can occur when mist is present at 0 °C (32 °F) and below.
3 Use freezing fog holdover times in conditions of ice crystals mixed with freezing fog or freezing mist.
4 To determine snowfall intensity, the Snowfall Intensities as a Function of Prevailing Visibility table (Table 57) is required. No holdover times exist if the reported visibility correlates to a “heavy” precipitation intensity. 
5 Use snow holdover times in conditions of very light, light, or moderate snow mixed with ice crystals.
6 Includes light, moderate and heavy freezing drizzle. Use light freezing rain holdover times if positive identification of freezing drizzle is not possible.
7 These holdover times apply to conditions of “moderate” precipitation intensity. In cases of very light or light snow mixed with light rain or drizzle, use light freezing rain holdover times. The Snowfall Intensities as a Function of Prevailing Visibility table (Table 57) is required to confirm the precipitation intensity. No holdover times exist if the reported visibility correlates to a “heavy” precipitation intensity.
8 No holdover time guidelines exist for this condition for 0 °C (32 °F) and below.
9 Heavy snow, ice pellets, moderate and heavy freezing rain, small hail and hail.
10 No holdover time guidelines exist for this condition below -10 °C (14 °F).
CAUTIONS
The cautions that apply to the holdover times in the table above can be found on page 14.


[bookmark: _Toc234306052]Table 14: Type II Holdover Times for Newave Aerochemical FCY-2
	Outside Air 
Temperature1
	Fluid 
Concentration 
Fluid/Water 
By % Volume
	Freezing Fog, Freezing Mist2, 
or Ice Crystals3
	Snow 
mixed with 
Freezing Fog4
	Snow, 
Snow Grains or Snow Pellets4,5
	Freezing 
Drizzle6
	Light 
Freezing Rain
	Moderate
Snow mixed with Rain7,8
	Rain on Cold‑Soaked Wing8
	Other9

	-3 °C and above
(27 °F and above)
	100/0
	1:15 - 2:25
	0:25 - 0:40
	0:30 - 0:55
	0:35 - 1:05
	0:25 - 0:35
	0:06 - 0:06
	0:08 - 0:45
	 

	
	75/25
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	 

	
	50/50
	N/A
	N/A
	N/A
	N/A
	N/A
	CAUTION: 
No holdover time 
guidelines exist

	below -3 to -8 °C
(below 27 to 18 °F)
	100/0
	0:45 - 1:30
	0:15 - 0:30
	0:20 - 0:40
	0:20 - 0:45
	0:15 - 0:20
	

	
	75/25
	N/A
	N/A
	N/A
	N/A
	N/A
	

	below -8 to -14 °C
(below 18 to 7 °F)
	100/0
	0:45 - 1:30
	0:10 - 0:25
	0:15 - 0:30
	0:20 - 0:4510
	0:15 - 0:2010
	

	
	75/25
	N/A
	N/A
	N/A
	N/A
	N/A
	

	below -14 to -18 °C
(below 7 to 0 °F)
	100/0
	0:25 - 0:35
	0:01 - 0:05
	0:02 - 0:07
	 
	

	below -18 to -25 °C
(below 0 to -13 °F)
	100/0
	0:25 - 0:35
	0:00 - 0:02
	0:01 - 0:03
	 
	 
	

	below -25 to -28 °C
(below -13 to -18 °F)
	100/0
	0:25 - 0:35
	0:00 - 0:00
	0:00 - 0:01
	 
	


NOTES
1. Ensure that the lowest operational use temperature (LOUT) is respected. Consider use of Type I fluid when Type II fluid cannot be used.
Freezing mist is best confirmed by observation. It is never reported by METAR; however, it can occur when mist is present at 0 °C (32 °F) and below. 
Use freezing fog holdover times in conditions of ice crystals mixed with freezing fog or freezing mist.
To determine snowfall intensity, the Snowfall Intensities as a Function of Prevailing Visibility table (Table 57) is required. No holdover times exist if the reported visibility correlates to a “heavy” precipitation intensity. 
Use snow holdover times in conditions of very light, light, or moderate snow mixed with ice crystals.
Includes light, moderate and heavy freezing drizzle. Use light freezing rain holdover times if positive identification of freezing drizzle is not possible.
These holdover times apply to conditions of “moderate” precipitation intensity. In cases of very light or light snow mixed with light rain or drizzle, use light freezing rain holdover times. The Snowfall Intensities as a Function of Prevailing Visibility table (Table 57) is required to confirm the precipitation intensity. No holdover times exist if the reported visibility correlates to a “heavy” precipitation intensity.
No holdover time guidelines exist for this condition for 0 °C (32 °F) and below.
Heavy snow, ice pellets, moderate and heavy freezing rain, small hail and hail.
No holdover time guidelines exist for this condition below -10 °C (14 °F).
CAUTIONS
The cautions that apply to the holdover times in the table above can be found on page 14.


[bookmark: _TABLE_2J._TYPE][bookmark: _TABLE_3A-LS._LOW][bookmark: _Toc234306053][bookmark: _Toc43986166][bookmark: _Toc508704817][bookmark: _Toc436349431]Table 15: Type II Holdover Times for ROMCHIM ADD-PROTECT NG Type II
	Outside Air 
Temperature1
	Fluid 
Concentration 
Fluid/Water 
By % Volume
	Freezing Fog, Freezing Mist2, or Ice Crystals3
	Snow 
mixed with 
Freezing Fog4
	Very Light Snow, Snow Grains or Snow Pellets4,5
	Light 
Snow, Snow Grains or Snow Pellets4,5
	Moderate Snow, Snow Grains or Snow Pellets4,5
	Freezing 
Drizzle6
	Light 
Freezing Rain
	Moderate
Snow mixed with Rain7,8
	Rain on 
Cold‑Soaked Wing8
	Other9

	-3 °C and above
(27 °F and above)
	100/0
	1:10 - 2:25
	0:25 - 0:55
	2:35 - 3:00
	1:10 - 2:35
	0:35 - 1:10
	0:50 - 1:20
	0:35 - 0:50
	0:05 - 0:05
	0:07 - 1:10
	 

	
	75/25
	1:00 - 1:50
	0:20 - 0:40
	1:55 - 2:25
	0:55 - 1:55
	0:25 - 0:55
	0:40 - 1:15
	0:25 - 0:40
	0:05 - 0:05
	0:07 - 0:55
	 

	
	50/50
	0:25 - 0:55
	0:10 - 0:20
	0:55 - 1:05
	0:30 - 0:55
	0:15 - 0:30
	0:20 - 0:35
	0:10 - 0:20
	CAUTION: 
No holdover time 
guidelines exist

	below -3 to -8 °C
(below 27 to 18 °F)
	100/0
	0:55 - 1:35
	0:20 - 0:40
	1:50 - 2:20
	0:50 - 1:50
	0:25 - 0:50
	0:35 - 1:10
	0:25 - 0:35
	

	
	75/25
	0:55 - 1:25
	0:15 - 0:30
	1:25 - 1:45
	0:40 - 1:25
	0:20 - 0:40
	0:25 - 1:05
	0:20 - 0:30
	

	below -8 to -14 °C
(below 18 to 7 °F)
	100/0
	0:55 - 1:35
	0:15 - 0:30
	1:25 - 1:50
	0:40 - 1:25
	0:20 - 0:40
	0:35 - 1:1010
	0:25 - 0:3510
	

	
	75/25
	0:55 - 1:25
	0:10 - 0:25
	1:05 - 1:25
	0:30 - 1:05
	0:15 - 0:30
	0:25 - 1:0510
	0:20 - 0:3010
	

	below -14 to -18 °C
(below 7 to 0 °F)
	100/0
	0:15 - 0:20
	0:01 - 0:05
	0:20 - 0:30
	0:07 - 0:20
	0:02 - 0:07
	
	

	below -18 to -25 °C
(below 0 to -13 °F)
	100/0
	0:15 - 0:20
	0:00 - 0:02
	0:09 - 0:15
	0:03 - 0:09
	0:01 - 0:03
	
	

	below -25 to -28 °C
(below -13 to -18 °F)
	100/0
	0:15 - 0:20
	0:00 - 0:00
	0:05 - 0:07
	0:01 - 0:05
	0:00 - 0:01
	
	


NOTES
1. Ensure that the lowest operational use temperature (LOUT) is respected. Consider use of Type I fluid when Type II fluid cannot be used.
Freezing mist is best confirmed by observation. It is never reported by METAR; however, it can occur when mist is present at 0 °C (32 °F) and below. 
Use freezing fog holdover times in conditions of ice crystals mixed with freezing fog or freezing mist.
To determine snowfall intensity, the Snowfall Intensities as a Function of Prevailing Visibility table (Table 57) is required. No holdover times exist if the reported visibility correlates to a “heavy” precipitation intensity. 
Use snow holdover times in conditions of very light, light, or moderate snow mixed with ice crystals.
Includes light, moderate and heavy freezing drizzle. Use light freezing rain holdover times if positive identification of freezing drizzle is not possible.
These holdover times apply to conditions of “moderate” precipitation intensity. In cases of very light or light snow mixed with light rain or drizzle, use light freezing rain holdover times. The Snowfall Intensities as a Function of Prevailing Visibility table (Table 57) is required to confirm the precipitation intensity. No holdover times exist if the reported visibility correlates to a “heavy” precipitation intensity.
No holdover time guidelines exist for this condition for 0 °C (32 °F) and below.
Heavy snow, ice pellets, moderate and heavy freezing rain, small hail and hail.
No holdover time guidelines exist for this condition below -10 °C (14 °F).
CAUTIONS
The cautions that apply to the holdover times in the table above can be found on page 14.


[bookmark: _Toc234306054]Table 16: Type II Holdover Times for ROMCHIM ADD-PROTECT Type II
	Outside Air 
Temperature1
	Fluid 
Concentration 
Fluid/Water 
By % Volume
	Freezing Fog, Freezing Mist2, or Ice Crystals3
	Snow 
mixed with 
Freezing Fog4
	Very Light Snow, Snow Grains or Snow Pellets4,5
	Light 
Snow, Snow Grains or Snow Pellets4,5
	Moderate Snow, Snow Grains or Snow Pellets4,5
	Freezing 
Drizzle6
	Light 
Freezing Rain
	Moderate
Snow mixed with Rain7,8
	Rain on 
Cold‑Soaked Wing8
	Other9

	-3 °C and above
(27 °F and above)
	100/0
	1:40 - 3:30
	0:20 - 0:45
	1:55 - 2:25
	1:00 - 1:55
	0:30 - 1:00
	0:40 - 1:35
	0:25 - 0:45
	0:06 - 0:06
	0:09 - 0:50
	 

	
	75/25
	0:40 - 1:10
	0:15 - 0:25
	1:00 - 1:10
	0:30 - 1:00
	0:15 - 0:30
	0:25 - 0:40
	0:15 - 0:25
	0:04 - 0:04
	0:05 - 0:25
	 

	
	50/50
	0:20 - 0:35
	0:07 - 0:15
	0:30 - 0:35
	0:15 - 0:30
	0:09 - 0:15
	0:10 - 0:30
	0:08 - 0:10
	CAUTION: 
No holdover time 
guidelines exist

	below -3 to -8 °C
(below 27 to 18 °F)
	100/0
	0:30 - 0:45
	0:15 - 0:30
	1:20 - 1:40
	0:40 - 1:20
	0:20 - 0:40
	0:25 - 0:50
	0:20 - 0:30
	

	
	75/25
	0:30 - 0:55
	0:09 - 0:15
	0:40 - 0:50
	0:25 - 0:40
	0:10 - 0:25
	0:20 - 0:30
	0:15 - 0:20
	

	below -8 to -14 °C
(below 18 to 7 °F)
	100/0
	0:30 - 0:45
	0:15 - 0:25
	1:05 - 1:20
	0:35 - 1:05
	0:15 - 0:35
	0:25 - 0:5010
	0:20 - 0:3010
	

	
	75/25
	0:30 - 0:55
	0:07 - 0:15
	0:35 - 0:40
	0:20 - 0:35
	0:09 - 0:20
	0:20 - 0:3010
	0:15 - 0:2010
	

	below -14 to -18 °C
(below 7 to 0 °F)
	100/0
	0:15 - 0:25
	0:01 - 0:05
	0:20 - 0:30
	0:07 - 0:20
	0:02 - 0:07
	
	

	below -18 to -25 °C
(below 0 to -13 °F)
	100/0
	0:15 - 0:25
	0:00 - 0:02
	0:09 - 0:15
	0:03 - 0:09
	0:01 - 0:03
	
	

	below -25 to -28 °C
(below -13 to -18 °F)
	100/0
	0:15 - 0:25
	0:00 - 0:00
	0:05 - 0:07
	0:01 - 0:05
	0:00 - 0:01
	
	


NOTES
1. Ensure that the lowest operational use temperature (LOUT) is respected. Consider use of Type I fluid when Type II fluid cannot be used.
Freezing mist is best confirmed by observation. It is never reported by METAR; however, it can occur when mist is present at 0 °C (32 °F) and below. 
Use freezing fog holdover times in conditions of ice crystals mixed with freezing fog or freezing mist.
To determine snowfall intensity, the Snowfall Intensities as a Function of Prevailing Visibility table (Table 57) is required. No holdover times exist if the reported visibility correlates to a “heavy” precipitation intensity. 
Use snow holdover times in conditions of very light, light, or moderate snow mixed with ice crystals.
Includes light, moderate and heavy freezing drizzle. Use light freezing rain holdover times if positive identification of freezing drizzle is not possible.
These holdover times apply to conditions of “moderate” precipitation intensity. In cases of very light or light snow mixed with light rain or drizzle, use light freezing rain holdover times. The Snowfall Intensities as a Function of Prevailing Visibility table (Table 57) is required to confirm the precipitation intensity. No holdover times exist if the reported visibility correlates to a “heavy” precipitation intensity.
No holdover time guidelines exist for this condition for 0 °C (32 °F) and below.
Heavy snow, ice pellets, moderate and heavy freezing rain, small hail and hail.
No holdover time guidelines exist for this condition below -10 °C (14 °F).
CAUTIONS
The cautions that apply to the holdover times in the table above can be found on page 14.
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The HOT Guidelines are provided for information and guidance purposes. The HOT Guidelines on their own do not change, create, amend or permit deviations from regulatory requirements.

The HOT Guidelines may use mandatory terms such as “must”, “shall” and “is/are required” so as to convey the intent of meeting regulatory requirements and SAE Standards, where applicable. The term “should” is to be understood, unless an alternative method of achieving safety is implemented that would meet or exceed the intent of the recommendation.



[bookmark: TypeIIICautions]CAUTIONS
The responsibility for the application of these data remains with the user.
The time of protection will be shortened in heavy weather conditions, heavy precipitation rates or high moisture content.
High wind velocity, jet blast or blowing snow may reduce holdover time below the lowest time stated in the range.
The holdover time may be reduced when aircraft skin temperature is lower than outside air temperature.
Fluids used during ground de/anti-icing do not provide in-flight icing protection.
This table is for departure planning only and should be used in conjunction with pre-takeoff check procedures.
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[bookmark: _Toc234306056]Table 17: Type III Holdover Times for AllClear AeroClear MAX
Applied Unheated – Low Speed Ramp Test1,2
	Outside Air 
Temperature3
	Fluid 
Concentration 
Fluid/Water 
By % Volume
	Freezing Fog, Freezing Mist4, or Ice Crystals5
	Snow 
mixed with 
Freezing Fog6
	Very Light Snow, Snow Grains or Snow Pellets6,7
	Light 
Snow, Snow Grains or Snow Pellets6,7
	Moderate Snow, Snow Grains or Snow Pellets6,7
	Freezing 
Drizzle8
	Light 
Freezing Rain
	Moderate
Snow mixed with Rain9,10
	Rain on
Cold‑Soaked Wing10
	Other11

	-3 °C and above
(27 °F and above)
	100/0
	0:45 - 1:55
	0:11 - 0:25
	1:10 - 1:30
	0:35 - 1:10
	0:15 - 0:35
	0:25 - 0:50
	0:14 - 0:25
	0:04 - 0:04
	0:05 - 0:40
	 

	
	75/25
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	 

	
	50/50
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	CAUTION: 
No holdover time 
guidelines exist

	below -3 to -10 °C
(below 27 to 14 °F)
	100/0
	0:50 - 1:40
	0:11 - 0:25
	1:10 - 1:30
	0:35 - 1:10
	0:15 - 0:35
	0:25 - 0:45
	0:15 - 0:25
	

	
	75/25
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	

	below -10 to -16 °C
(below 14 to 3 °F)
	100/0
	0:40 - 1:45
	0:11 - 0:25
	1:10 - 1:30
	0:35 - 1:10
	0:15 - 0:35
	
	


NOTES
1. Consult the aircraft manufacturer’s documentation to determine application of low, middle, or high speed ramp test values. If uncertain, apply low speed test values.
1. Fluid must be applied unheated to use these holdover times. No holdover times exist for this fluid applied heated.
Ensure that the lowest operational use temperature (LOUT) is respected. Consider use of Type I fluid when Type III fluid cannot be used.
Freezing mist is best confirmed by observation. It is never reported by METAR; however, it can occur when mist is present at 0 °C (32 °F) and below. 
Use freezing fog holdover times in conditions of ice crystals mixed with freezing fog or freezing mist.
To determine snowfall intensity, the Snowfall Intensities as a Function of Prevailing Visibility table (Table 57) is required. No holdover times exist if the reported visibility correlates to a “heavy” precipitation intensity. 
Use snow holdover times in conditions of very light, light, or moderate snow mixed with ice crystals.
Includes light, moderate and heavy freezing drizzle. Use light freezing rain holdover times if positive identification of freezing drizzle is not possible.
These holdover times apply to conditions of “moderate” precipitation intensity. In cases of very light or light snow mixed with light rain or drizzle, use light freezing rain holdover times. The Snowfall Intensities as a Function of Prevailing Visibility table (Table 57) is required to confirm the precipitation intensity. No holdover times exist if the reported visibility correlates to a “heavy” precipitation intensity.
No holdover time guidelines exist for this condition for 0 °C (32 °F) and below.
Heavy snow, ice pellets, moderate and heavy freezing rain, small hail and hail.
CAUTIONS
The cautions that apply to the holdover times in the table above can be found on page 28.


[bookmark: _TABLE_3A-HS._HIGH][bookmark: _Toc234306057][bookmark: _Toc508704818][bookmark: _Toc43986168][bookmark: _Toc436349432]Table 18: Type III Holdover Times for AllClear AeroClear MAX
Applied Unheated – Middle Speed Ramp Test1,2
	Outside Air 
Temperature3
	Fluid 
Concentration 
Fluid/Water 
By % Volume
	Freezing Fog, Freezing Mist4, or Ice Crystals5
	Snow 
mixed with 
Freezing Fog6
	Very Light Snow, Snow Grains or Snow Pellets6,7
	Light 
Snow, Snow Grains or Snow Pellets6,7
	Moderate Snow, Snow Grains or Snow Pellets6,7
	Freezing 
Drizzle8
	Light 
Freezing Rain
	Moderate
Snow mixed with Rain9,10
	Rain on
Cold‑Soaked Wing10
	Other11

	-3 °C and above
(27 °F and above)
	100/0
	0:45 - 1:55
	0:11 - 0:25
	1:10 - 1:30
	0:35 - 1:10
	0:15 - 0:35
	0:25 - 0:50
	0:14 - 0:25
	0:04 - 0:04
	0:05 - 0:40
	 

	
	75/25
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	 

	
	50/50
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	CAUTION: 
No holdover time 
guidelines exist

	below -3 to -10 °C
(below 27 to 14 °F)
	100/0
	0:50 - 1:40
	0:11 - 0:25
	1:10 - 1:30
	0:35 - 1:10
	0:15 - 0:35
	0:25 - 0:45
	0:15 - 0:25
	

	
	75/25
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	

	below -10 to -20.5 °C
(below 14 to -5 °F)
	100/0
	0:40 - 1:45
	0:11 - 0:25
	1:10 - 1:30
	0:35 - 1:10
	0:15 - 0:35
	
	


NOTES
1. Consult the aircraft manufacturer’s documentation to determine application of low, middle, or high speed ramp test values. If uncertain, apply low speed test values.
Fluid must be applied unheated to use these holdover times. No holdover times exist for this fluid applied heated.
Ensure that the lowest operational use temperature (LOUT) is respected. Consider use of Type I fluid when Type III fluid cannot be used.
Freezing mist is best confirmed by observation. It is never reported by METAR; however, it can occur when mist is present at 0 °C (32 °F) and below. 
Use freezing fog holdover times in conditions of ice crystals mixed with freezing fog or freezing mist.
To determine snowfall intensity, the Snowfall Intensities as a Function of Prevailing Visibility table (Table 57) is required. No holdover times exist if the reported visibility correlates to a “heavy” precipitation intensity. 
Use snow holdover times in conditions of very light, light, or moderate snow mixed with ice crystals.
Includes light, moderate and heavy freezing drizzle. Use light freezing rain holdover times if positive identification of freezing drizzle is not possible.
These holdover times apply to conditions of “moderate” precipitation intensity. In cases of very light or light snow mixed with light rain or drizzle, use light freezing rain holdover times. The Snowfall Intensities as a Function of Prevailing Visibility table (Table 57) is required to confirm the precipitation intensity. No holdover times exist if the reported visibility correlates to a “heavy” precipitation intensity.
No holdover time guidelines exist for this condition for 0 °C (32 °F) and below.
Heavy snow, ice pellets, moderate and heavy freezing rain, small hail and hail.
CAUTIONS
The cautions that apply to the holdover times in the table above can be found on page 28.


[bookmark: _Toc234306058]Table 19: Type III Holdover Times for AllClear AeroClear MAX
Applied Unheated – High Speed Ramp Test1,2
	Outside Air 
Temperature3
	Fluid 
Concentration 
Fluid/Water 
By % Volume
	Freezing Fog, Freezing Mist4, or Ice Crystals5
	Snow 
mixed with 
Freezing Fog6
	Very Light Snow, Snow Grains or Snow Pellets6,7
	Light 
Snow, Snow Grains or Snow Pellets6,7
	Moderate Snow, Snow Grains or Snow Pellets6,7
	Freezing 
Drizzle8
	Light 
Freezing Rain
	Moderate
Snow mixed with Rain9,10
	Rain on
Cold‑Soaked Wing10
	Other11

	-3 °C and above
(27 °F and above)
	100/0
	0:45 - 1:55
	0:11 - 0:25
	1:10 - 1:30
	0:35 - 1:10
	0:15 - 0:35
	0:25 - 0:50
	0:14 - 0:25
	0:04 - 0:04
	0:05 - 0:40
	 

	
	75/25
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	 

	
	50/50
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	CAUTION: 
No holdover time 
guidelines exist

	below -3 to -10 °C
(below 27 to 14 °F)
	100/0
	0:50 - 1:40
	0:11 - 0:25
	1:10 - 1:30
	0:35 - 1:10
	0:15 - 0:35
	0:25 - 0:45
	0:15 - 0:25
	

	
	75/25
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	

	below -10 to -25 °C
(below 14 to -13 °F)
	100/0
	0:40 - 1:45
	0:11 - 0:25
	1:10 - 1:30
	0:35 - 1:10
	0:15 - 0:35
	
	

	below -25 to -35 °C (below -13 to -31 °F)
	100/0
	0:25 - 1:00
	0:06 - 0:13
	0:40 - 0:50
	0:18 - 0:40
	0:08 - 0:18
	
	


NOTES
1. Consult the aircraft manufacturer’s documentation to determine application of low, middle, or high speed ramp test values. If uncertain, apply low speed test values.
Fluid must be applied unheated to use these holdover times. No holdover times exist for this fluid applied heated.
Ensure that the lowest operational use temperature (LOUT) is respected. Consider use of Type I fluid when Type III fluid cannot be used.
Freezing mist is best confirmed by observation. It is never reported by METAR; however, it can occur when mist is present at 0 °C (32 °F) and below. 
Use freezing fog holdover times in conditions of ice crystals mixed with freezing fog or freezing mist.
To determine snowfall intensity, the Snowfall Intensities as a Function of Prevailing Visibility table (Table 57) is required. No holdover times exist if the reported visibility correlates to a “heavy” precipitation intensity. 
Use snow holdover times in conditions of very light, light, or moderate snow mixed with ice crystals.
Includes light, moderate and heavy freezing drizzle. Use light freezing rain holdover times if positive identification of freezing drizzle is not possible.
These holdover times apply to conditions of “moderate” precipitation intensity. In cases of very light or light snow mixed with light rain or drizzle, use light freezing rain holdover times. The Snowfall Intensities as a Function of Prevailing Visibility table (Table 57) is required to confirm the precipitation intensity. No holdover times exist if the reported visibility correlates to a “heavy” precipitation intensity.
No holdover time guidelines exist for this condition for 0 °C (32 °F) and below.
Heavy snow, ice pellets, moderate and heavy freezing rain, small hail and hail (Table 54 provides allowance times for ice pellets and small hail for SAE Type III fluids, applied unheated).
CAUTIONS
The cautions that apply to the holdover times in the table above can be found on page 28.
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The HOT Guidelines are provided for information and guidance purposes. The HOT Guidelines on their own do not change, create, amend, or permit deviations from regulatory requirements.

The HOT Guidelines may use mandatory terms such as “must”, “shall” and “is/are required” so as to convey the intent of meeting regulatory requirements and SAE Standards, where applicable. The term “should” is to be understood, unless an alternative method of achieving safety is implemented that would meet or exceed the intent of the recommendation.



[bookmark: TypeIVCautions]CAUTIONS
The responsibility for the application of these data remains with the user.
The time of protection will be shortened in heavy weather conditions, heavy precipitation rates or high moisture content.
High wind velocity, jet blast or blowing snow may reduce holdover time below the lowest time stated in the range.
The holdover time may be reduced when aircraft skin temperature is lower than outside air temperature.
Fluids used during ground de/anti-icing do not provide in-flight icing protection.
This table is for departure planning only and should be used in conjunction with pre-takeoff check procedures.
Whenever frost or ice occurs on the lower surface of the wing in the area of the fuel tank, indicating a cold-soaked wing, the 50/50 dilution of Type II or IV are not to be used for the anti-icing step because fluid freezing may occur.
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[bookmark: _Toc234306060]Table 20: Generic Holdover Times for SAE Type IV Fluids1
	Outside Air 
Temperature2
	Fluid 
Concentration 
Fluid/Water 
By % Volume
	Freezing Fog, Freezing Mist3, or Ice Crystals4
	Snow 
mixed with 
Freezing Fog5
	Very Light Snow, Snow Grains or Snow Pellets5,6
	Light 
Snow, Snow Grains or Snow Pellets5,6
	Moderate Snow, Snow Grains or Snow Pellets5,6
	Freezing 
Drizzle7
	Light 
Freezing Rain
	Moderate
Snow mixed with Rain8,9
	Rain on 
Cold‑Soaked Wing9
	Other10

	-3 °C and above
(27 °F and above)
	100/0
	1:15 - 2:15
	0:20 - 0:40
	1:50 - 2:15
	0:55 - 1:50
	0:25 - 0:55
	0:35 - 1:10
	0:15 - 0:30
	0:06 - 0:06
	0:08 - 1:05
	 

	
	75/25
	1:25 - 2:40
	0:30 - 0:55
	2:05 - 2:25
	1:15 - 2:05
	0:40 - 1:15
	1:00 - 1:20
	0:30 - 0:50
	0:07 - 0:07
	0:09 - 1:20
	 

	
	50/50
	0:30 - 0:55
	0:07 - 0:20
	1:00 - 1:10
	0:25 - 1:00
	0:10 - 0:25
	0:15 - 0:40
	0:09 - 0:20
	CAUTION: 
No holdover time 
guidelines exist

	below -3 to -8 °C
(below 27 to 18 °F)
	100/0
	0:15 - 0:35
	0:20 - 0:35
	1:35 - 2:00
	0:45 - 1:35
	0:25 - 0:45
	0:25 - 1:00
	0:20 - 0:25
	

	
	75/25
	0:40 - 1:20
	0:25 - 0:50
	1:50 - 2:10
	1:05 - 1:50
	0:30 - 1:05
	0:20 - 1:05
	0:15 - 0:25
	

	below -8 to -14 °C
(below 18 to 7 °F)
	100/0
	0:15 - 0:35
	0:15 - 0:30
	1:25 - 1:50
	0:45 - 1:25
	0:20 - 0:45
	0:25 - 1:0011
	0:15 - 0:2511
	

	
	75/25
	0:40 - 1:20
	0:20 - 0:45
	1:45 - 2:00
	0:55 - 1:45
	0:25 - 0:55
	0:20 - 1:0511
	0:15 - 0:2511
	

	below -14 to -18 °C
(below 7 to 0 °F)
	100/0
	0:15 - 0:25
	0:01 - 0:06
	0:30 - 0:45
	0:09 - 0:30
	0:02 - 0:09
	
	

	below -18 to -25 °C
(below 0 to -13 °F)
	100/0
	0:15 - 0:25
	0:00 - 0:02
	0:10 - 0:20
	0:03 - 0:10
	0:01 - 0:03
	
	

	below -25 °C 
(below -13 °F)
	100/0
	0:15 - 0:25
	0:00 - 0:01
	0:07 - 0:10
	0:02 - 0:07
	0:00 - 0:02
	
	


NOTES
1. To use the holdover times in this table, ensure that the fluid and dilution being used is listed in the Type IV Fluids Tested for Anti-Icing Performance and Aerodynamic Acceptance table (Table 61). Any restrictions on the use of the fluid have to be identified and applied.
1. Ensure that the lowest operational use temperature (LOUT) is respected. Consider use of Type I fluid when Type IV fluid cannot be used.
Freezing mist is best confirmed by observation. It is never reported by METAR; however, it can occur when mist is present at 0 °C (32 °F) and below. 
Use freezing fog holdover times in conditions of ice crystals mixed with freezing fog or freezing mist.
To determine snowfall intensity, the Snowfall Intensities as a Function of Prevailing Visibility table (Table 57) is required. No holdover times exist if the reported visibility correlates to a “heavy” precipitation intensity. 
Use snow holdover times in conditions of very light, light, or moderate snow mixed with ice crystals.
Includes light, moderate and heavy freezing drizzle. Use light freezing rain holdover times if positive identification of freezing drizzle is not possible.
These holdover times apply to conditions of “moderate” precipitation intensity. In cases of very light or light snow mixed with light rain or drizzle, use light freezing rain holdover times. The Snowfall Intensities as a Function of Prevailing Visibility table (Table 57) is required to confirm the precipitation intensity. No holdover times exist if the reported visibility correlates to a “heavy” precipitation intensity.
No holdover time guidelines exist for this condition for 0 °C (32 °F) and below.
[bookmark: _Hlk77764058]Heavy snow, ice pellets, moderate and heavy freezing rain, small hail and hail (Table 55 and Table 56 provides allowance times for Type IV EG and Type IV PG fluids in ice pellets and small hail. To use these allowance times, ensure that the fluid being used is listed as validated in Table 53). 
No holdover time guidelines exist for this condition below -10 °C (14 °F).
CAUTIONS
The cautions that apply to the holdover times in the table above can be found on page 32.

[bookmark: _TABLE_4A._TYPE][bookmark: _Toc436349436][bookmark: _Toc508704822][bookmark: _Toc43986170][bookmark: _Toc234306061]Table 21: Type IV Holdover Times for ABAX ECOWING AD-49
	Outside Air 
Temperature1
	Fluid 
Concentration 
Fluid/Water 
By % Volume
	Freezing Fog, Freezing Mist2, or Ice Crystals3
	Snow 
mixed with 
Freezing Fog4
	Very Light Snow, Snow Grains or Snow Pellets4,5
	Light 
Snow, Snow Grains or Snow Pellets4,5
	Moderate Snow, Snow Grains or Snow Pellets4,5
	Freezing 
Drizzle6
	Light 
Freezing Rain
	Moderate
Snow mixed with Rain7,8
	Rain on 
Cold‑Soaked Wing8
	Other9

	-3 °C and above
(27 °F and above)
	100/0
	3:20 - 4:00
	0:45 - 1:25
	3:00 - 3:00
	1:55 - 3:00
	1:00 - 1:55
	1:25 - 2:00
	1:00 - 1:25
	0:08 - 0:08
	0:10 - 1:55
	 

	
	75/25
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	 

	
	50/50
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	CAUTION: 
No holdover time 
guidelines exist

	below -3 to -8 °C
(below 27 to 18 °F)
	100/0
	0:20 - 1:35
	0:35 - 1:05
	2:55 - 3:00
	1:30 - 2:55
	0:45 - 1:30
	0:25 - 1:25
	0:20 - 0:25
	

	
	75/25
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	

	below -8 to -14 °C
(below 18 to 7 °F)
	100/0
	0:20 - 1:35
	0:30 - 0:55
	2:25 - 3:00
	1:15 - 2:25
	0:40 - 1:15
	0:25 - 1:2510
	0:20 - 0:2510
	

	
	75/25
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	

	below -14 to -18 °C
(below 7 to 0 °F)
	100/0
	0:25 - 0:40
	0:01 - 0:06
	0:30 - 0:45
	0:09 - 0:30
	0:02 - 0:09
	
	

	below -18 to -25 °C
(below 0 to -13 °F)
	100/0
	0:25 - 0:40
	0:00 - 0:02
	0:10 - 0:20
	0:03 - 0:10
	0:01 - 0:03
	
	

	below -25 to -26 °C
(below -13 to -15 °F)
	100/0
	0:25 - 0:40
	0:00 - 0:01
	0:07 - 0:10
	0:02 - 0:07
	0:00 - 0:02
	
	


NOTES
1. Ensure that the lowest operational use temperature (LOUT) is respected. Consider use of Type I fluid when Type IV fluid cannot be used.
Freezing mist is best confirmed by observation. It is never reported by METAR; however, it can occur when mist is present at 0 °C (32 °F) and below. 
Use freezing fog holdover times in conditions of ice crystals mixed with freezing fog or freezing mist.
To determine snowfall intensity, the Snowfall Intensities as a Function of Prevailing Visibility table (Table 57) is required. No holdover times exist if the reported visibility correlates to a “heavy” precipitation intensity. 
Use snow holdover times in conditions of very light, light, or moderate snow mixed with ice crystals.
Includes light, moderate and heavy freezing drizzle. Use light freezing rain holdover times if positive identification of freezing drizzle is not possible.
These holdover times apply to conditions of “moderate” precipitation intensity. In cases of very light or light snow mixed with light rain or drizzle, use light freezing rain holdover times. The Snowfall Intensities as a Function of Prevailing Visibility table (Table 57) is required to confirm the precipitation intensity. No holdover times exist if the reported visibility correlates to a “heavy” precipitation intensity.
No holdover time guidelines exist for this condition for 0 °C (32 °F) and below.
Heavy snow, ice pellets, moderate and heavy freezing rain, small hail and hail (Table 56 provides allowance times for Type IV PG fluids in ice pellets and small hail).
No holdover time guidelines exist for this condition below -10 °C (14 °F).
CAUTIONS
The cautions that apply to the holdover times in the table above can be found on page 32.


[bookmark: _Toc234306062]Table 22: Type IV Holdover Times for AFLRUS LLC Green Flo Type 4
	Outside Air 
Temperature1
	Fluid 
Concentration 
Fluid/Water 
By % Volume
	Freezing Fog, Freezing Mist2, or Ice Crystals3
	Snow 
mixed with 
Freezing Fog4
	Very Light Snow, Snow Grains or Snow Pellets4,5
	Light 
Snow, Snow Grains or Snow Pellets4,5
	Moderate Snow, Snow Grains or Snow Pellets4,5
	Freezing 
Drizzle6
	Light 
Freezing Rain
	Moderate
Snow mixed with Rain7,8
	Rain on 
Cold‑Soaked Wing8
	Other9

	-3 °C and above
(27 °F and above)
	100/0
	1:15 - 2:30
	0:20 - 0:40
	1:50 - 2:15
	0:55 - 1:50
	0:25 - 0:55
	0:35 - 1:10
	0:15 - 0:30
	0:06 - 0:06
	0:08 - 1:10
	 

	
	75/25
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	 

	
	50/50
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	CAUTION: 
No holdover time 
guidelines exist

	below -3 to -8 °C
(below 27 to 18 °F)
	100/0
	0:50 - 2:35
	0:20 - 0:35
	1:35 - 2:00
	0:45 - 1:35
	0:25 - 0:45
	0:35 - 1:00
	0:20 - 0:30
	

	
	75/25
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	

	below -8 to -14 °C
(below 18 to 7 °F)
	100/0
	0:50 - 2:35
	0:15 - 0:30
	1:25 - 1:50
	0:45 - 1:25
	0:20 - 0:45
	0:35 - 1:0010
	0:20 - 0:3010
	

	
	75/25
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	

	below -14 to -18 °C
(below 7 to 0 °F)
	100/0
	0:35 - 1:10
	0:10 - 0:25
	1:20 - 1:45
	0:35 - 1:20
	0:15 - 0:35
	
	

	below -18 to -25 °C
(below 0 to -13 °F)
	100/0
	0:35 - 1:10
	0:10 - 0:25
	1:10 - 1:30
	0:30 - 1:10
	0:15 - 0:30
	
	

	below -25 to -30 °C
(below -13 to -22 °F)
	100/0
	0:25 - 1:00
	0:04 - 0:10
	0:35 - 0:40
	0:15 - 0:35
	0:06 - 0:15
	
	


NOTES
1. Ensure that the lowest operational use temperature (LOUT) is respected. Consider use of Type I fluid when Type IV fluid cannot be used.
Freezing mist is best confirmed by observation. It is never reported by METAR; however, it can occur when mist is present at 0 °C (32 °F) and below. 
Use freezing fog holdover times in conditions of ice crystals mixed with freezing fog or freezing mist.
To determine snowfall intensity, the Snowfall Intensities as a Function of Prevailing Visibility table (Table 57) is required. No holdover times exist if the reported visibility correlates to a “heavy” precipitation intensity. 
Use snow holdover times in conditions of very light, light, or moderate snow mixed with ice crystals.
Includes light, moderate and heavy freezing drizzle. Use light freezing rain holdover times if positive identification of freezing drizzle is not possible.
These holdover times apply to conditions of “moderate” precipitation intensity. In cases of very light or light snow mixed with light rain or drizzle, use light freezing rain holdover times. The Snowfall Intensities as a Function of Prevailing Visibility table (Table 57) is required to confirm the precipitation intensity. No holdover times exist if the reported visibility correlates to a “heavy” precipitation intensity.
No holdover time guidelines exist for this condition for 0 °C (32 °F) and below.
Heavy snow, ice pellets, moderate and heavy freezing rain, small hail and hail.
No holdover time guidelines exist for this condition below -10 °C (14 °F).
CAUTIONS
The cautions that apply to the holdover times in the table above can be found on page 32.


[bookmark: _TABLE_4B._TYPE][bookmark: _Toc234306063][bookmark: _Toc43986171][bookmark: _Toc508704823][bookmark: _Toc436349437]Table 23: Type IV Holdover Times for ALAB International PROFLIGHT EG4
	Outside Air 
Temperature1
	Fluid 
Concentration 
Fluid/Water 
By % Volume
	Freezing Fog, Freezing Mist2, or Ice Crystals3
	Snow 
mixed with 
Freezing Fog4
	Very Light Snow, Snow Grains or Snow Pellets4,5
	Light 
Snow, Snow Grains or Snow Pellets4,5
	Moderate Snow, Snow Grains or Snow Pellets4,5
	Freezing 
Drizzle6
	Light 
Freezing Rain
	Moderate
Snow mixed with Rain7,8
	Rain on 
Cold‑Soaked Wing8
	Other9

	-3 °C and above
(27 °F and above)
	100/0
	3:05 - 4:00
	0:40 - 1:15
	3:00 - 3:00
	1:35 - 3:00
	0:50 - 1:35
	1:25 - 2:00
	0:40 - 1:00
	0:08 - 0:08
	0:10 - 2:00
	 

	
	75/25
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	 

	
	50/50
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	CAUTION: 
No holdover time 
guidelines exist

	below -3 to -8 °C
(below 27 to 18 °F)
	100/0
	2:30 - 3:55
	0:40 - 1:15
	3:00 - 3:00
	1:35 - 3:00
	0:50 - 1:35
	1:05 - 2:00
	0:50 - 1:35
	

	
	75/25
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	

	below -8 to -14 °C
(below 18 to 7 °F)
	100/0
	2:30 - 3:55
	0:40 - 1:15
	3:00 - 3:00
	1:35 - 3:00
	0:50 - 1:35
	1:05 - 2:0010
	0:50 - 1:3510
	

	
	75/25
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	

	below -14 to -18 °C
(below 7 to 0 °F)
	100/0
	0:35 - 1:35
	0:30 - 1:00
	2:45 - 3:00
	1:20 - 2:45
	0:40 - 1:20
	
	

	below -18 to -25 °C
(below 0 to -13 °F)
	100/0
	0:35 - 1:35
	0:15 - 0:35
	1:30 - 1:55
	0:45 - 1:30
	0:20 - 0:45
	
	

	below -25 to -26 °C
(below -13 to -15 °F)
	100/0
	0:35 - 1:35
	0:15 - 0:30
	1:25 - 1:45
	0:40 - 1:25
	0:20 - 0:40
	
	


NOTES
1. Ensure that the lowest operational use temperature (LOUT) is respected. Consider use of Type I fluid when Type IV fluid cannot be used.
Freezing mist is best confirmed by observation. It is never reported by METAR; however, it can occur when mist is present at 0 °C (32 °F) and below. 
Use freezing fog holdover times in conditions of ice crystals mixed with freezing fog or freezing mist.
To determine snowfall intensity, the Snowfall Intensities as a Function of Prevailing Visibility table (Table 57) is required. No holdover times exist if the reported visibility correlates to a “heavy” precipitation intensity. 
Use snow holdover times in conditions of very light, light, or moderate snow mixed with ice crystals.
Includes light, moderate and heavy freezing drizzle. Use light freezing rain holdover times if positive identification of freezing drizzle is not possible.
These holdover times apply to conditions of “moderate” precipitation intensity. In cases of very light or light snow mixed with light rain or drizzle, use light freezing rain holdover times. The Snowfall Intensities as a Function of Prevailing Visibility table (Table 57) is required to confirm the precipitation intensity. No holdover times exist if the reported visibility correlates to a “heavy” precipitation intensity.
No holdover time guidelines exist for this condition for 0 °C (32 °F) and below.
Heavy snow, ice pellets, moderate and heavy freezing rain, small hail and hail.
No holdover time guidelines exist for this condition below -10 °C (14 °F).
CAUTIONS
The cautions that apply to the holdover times in the table above can be found on page 32.


[bookmark: _Toc234306064]Table 24: Type IV Holdover Times for ALAB International PROFLIGHT PG4
	Outside Air 
Temperature1
	Fluid 
Concentration 
Fluid/Water 
By % Volume
	Freezing Fog, Freezing Mist2, or Ice Crystals3
	Snow 
mixed with 
Freezing Fog4
	Very Light Snow, Snow Grains or Snow Pellets4,5
	Light 
Snow, Snow Grains or Snow Pellets4,5
	Moderate Snow, Snow Grains or Snow Pellets4,5
	Freezing 
Drizzle6
	Light 
Freezing Rain
	Moderate
Snow mixed with Rain7,8
	Rain on 
Cold‑Soaked Wing8
	Other9

	-3 °C and above
(27 °F and above)
	100/0
	1:25 - 2:15
	0:30 - 1:00
	2:40 - 3:00
	1:20 - 2:40
	0:40 - 1:20
	1:05 - 1:25
	0:40 - 0:50
	0:10 - 0:10
	0:15 - 1:20
	 

	
	75/25
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	 

	
	50/50
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	CAUTION: 
No holdover time 
guidelines exist

	below -3 to -8 °C
(below 27 to 18 °F)
	100/0
	1:05 - 2:20
	0:25 - 0:50
	2:20 - 2:55
	1:10 - 2:20
	0:35 - 1:10
	0:45 - 1:10
	0:35 - 0:45
	

	
	75/25
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	

	below -8 to -14 °C
(below 18 to 7 °F)
	100/0
	1:05 - 2:20
	0:20 - 0:45
	2:05 - 2:35
	1:00 - 2:05
	0:30 - 1:00
	0:45 - 1:1010
	0:35 - 0:4510
	

	
	75/25
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	

	below -14 to -18 °C
(below 7 to 0 °F)
	100/0
	0:35 - 0:50
	0:10 - 0:25
	1:15 - 1:40
	0:35 - 1:15
	0:15 - 0:35
	
	

	below -18 to -25 °C
(below 0 to -13 °F)
	100/0
	0:35 - 0:50
	0:07 - 0:15
	0:50 - 1:00
	0:20 - 0:50
	0:09 - 0:20
	
	

	below -25 to -29 °C
(below -13 to -20 °F)
	100/0
	0:35 - 0:50
	0:05 - 0:15
	0:40 - 0:50
	0:15 - 0:40
	0:07 - 0:15
	
	


NOTES
1. Ensure that the lowest operational use temperature (LOUT) is respected. Consider use of Type I fluid when Type IV fluid cannot be used.
Freezing mist is best confirmed by observation. It is never reported by METAR; however, it can occur when mist is present at 0 °C (32 °F) and below. 
Use freezing fog holdover times in conditions of ice crystals mixed with freezing fog or freezing mist.
To determine snowfall intensity, the Snowfall Intensities as a Function of Prevailing Visibility table (Table 57) is required. No holdover times exist if the reported visibility correlates to a “heavy” precipitation intensity. 
Use snow holdover times in conditions of very light, light, or moderate snow mixed with ice crystals.
Includes light, moderate and heavy freezing drizzle. Use light freezing rain holdover times if positive identification of freezing drizzle is not possible.
These holdover times apply to conditions of “moderate” precipitation intensity. In cases of very light or light snow mixed with light rain or drizzle, use light freezing rain holdover times. The Snowfall Intensities as a Function of Prevailing Visibility table (Table 57) is required to confirm the precipitation intensity. No holdover times exist if the reported visibility correlates to a “heavy” precipitation intensity.
No holdover time guidelines exist for this condition for 0 °C (32 °F) and below.
Heavy snow, ice pellets, moderate and heavy freezing rain, small hail and hail.
No holdover time guidelines exist for this condition below -10 °C (14 °F).
CAUTIONS
The cautions that apply to the holdover times in the table above can be found on page 32.


[bookmark: _Toc234306065]Table 25: Type IV Holdover Times for AllClear Clear IV Flight
	Outside Air 
Temperature1
	Fluid 
Concentration 
Fluid/Water 
By % Volume
	Freezing Fog, Freezing Mist2, or Ice Crystals3
	Snow 
mixed with 
Freezing Fog4
	Very Light Snow, Snow Grains or Snow Pellets4,5
	Light 
Snow, Snow Grains or Snow Pellets4,5
	Moderate Snow, Snow Grains or Snow Pellets4,5
	Freezing 
Drizzle6
	Light 
Freezing Rain
	Moderate
Snow mixed with Rain7,8
	Rain on 
Cold‑Soaked Wing8
	Other9

	-3 °C and above
(27 °F and above)
	100/0
	1:35 - 2:50
	0:30 - 1:00
	2:30 - 3:00
	1:20 - 2:30
	0:40 - 1:20
	1:05 - 1:45
	0:50 - 1:10
	0:15 - 0:15
	0:20 - 1:15
	 

	
	75/25
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	 

	
	50/50
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	CAUTION: 
No holdover time 
guidelines exist

	below -3 to -8 °C
(below 27 to 18 °F)
	100/0
	0:50 - 1:55
	0:25 - 0:45
	1:55 - 2:25
	1:00 - 1:55
	0:30 - 1:00
	0:50 - 1:25
	0:40 - 0:50
	

	
	75/25
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	

	below -8 to -14 °C
(below 18 to 7 °F)
	100/0
	0:50 - 1:55
	0:20 - 0:40
	1:40 - 2:00
	0:50 - 1:40
	0:25 - 0:50
	0:50 - 1:2510
	0:40 - 0:5010
	

	
	75/25
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	

	below -14 to -18 °C
(below 7 to 0 °F)
	100/0
	0:25 - 0:45
	0:10 - 0:20
	1:00 - 1:10
	0:30 - 1:00
	0:15 - 0:30
	
	

	below -18 to -23 °C
(below 0 to -9 °F)
	100/0
	0:25 - 0:45
	0:08 - 0:15
	0:40 - 0:50
	0:20 - 0:40
	0:10 - 0:20
	
	


NOTES
1. Ensure that the lowest operational use temperature (LOUT) is respected. Consider use of Type I fluid when Type IV fluid cannot be used.
Freezing mist is best confirmed by observation. It is never reported by METAR; however, it can occur when mist is present at 0 °C (32 °F) and below. 
Use freezing fog holdover times in conditions of ice crystals mixed with freezing fog or freezing mist.
To determine snowfall intensity, the Snowfall Intensities as a Function of Prevailing Visibility table (Table 57) is required. No holdover times exist if the reported visibility correlates to a “heavy” precipitation intensity. 
Use snow holdover times in conditions of very light, light, or moderate snow mixed with ice crystals.
Includes light, moderate and heavy freezing drizzle. Use light freezing rain holdover times if positive identification of freezing drizzle is not possible.
These holdover times apply to conditions of “moderate” precipitation intensity. In cases of very light or light snow mixed with light rain or drizzle, use light freezing rain holdover times. The Snowfall Intensities as a Function of Prevailing Visibility table (Table 57) is required to confirm the precipitation intensity. No holdover times exist if the reported visibility correlates to a “heavy” precipitation intensity.
No holdover time guidelines exist for this condition for 0 °C (32 °F) and below.
Heavy snow, ice pellets, moderate and heavy freezing rain, small hail and hail.
No holdover time guidelines exist for this condition below -10 °C (14 °F).
CAUTIONS
The cautions that apply to the holdover times in the table above can be found on page 32.


[bookmark: _Toc234306066]Table 26: Type IV Holdover Times for AllClear ClearWing EG
	Outside Air 
Temperature1
	Fluid 
Concentration 
Fluid/Water 
By % Volume
	Freezing Fog, Freezing Mist2, or Ice Crystals3
	Snow 
mixed with 
Freezing Fog4
	Very Light Snow, Snow Grains or Snow Pellets4,5
	Light 
Snow, Snow Grains or Snow Pellets4,5
	Moderate Snow, Snow Grains or Snow Pellets4,5
	Freezing 
Drizzle6
	Light 
Freezing Rain
	Moderate
Snow mixed with Rain7,8
	Rain on 
Cold‑Soaked Wing8
	Other9

	-3 °C and above
(27 °F and above)
	100/0
	1:50 - 3:15
	0:30 - 1:00
	2:40 - 3:00
	1:20 - 2:40
	0:40 - 1:20
	1:10 - 1:35
	0:30 - 1:00
	0:08 - 0:08
	0:10 - 1:30
	 

	
	75/25
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	 

	
	50/50
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	CAUTION: 
No holdover time 
guidelines exist

	below -3 to -8 °C
(below 27 to 18 °F)
	100/0
	1:35 - 3:45
	0:25 - 0:55
	2:25 - 3:00
	1:10 - 2:25
	0:35 - 1:10
	1:05 - 1:30
	0:30 - 1:00
	

	
	75/25
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	

	below -8 to -14 °C
(below 18 to 7 °F)
	100/0
	1:35 - 3:45
	0:25 - 0:50
	2:15 - 2:45
	1:05 - 2:15
	0:30 - 1:05
	1:05 - 1:3010
	0:30 - 1:0010
	

	
	75/25
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	

	below -14 to -18 °C
(below 7 to 0 °F)
	100/0
	0:55 - 2:00
	0:15 - 0:35
	1:35 - 2:05
	0:45 - 1:35
	0:20 - 0:45
	
	

	below -18 to -25 °C
(below 0 to -13 °F)
	100/0
	0:55 - 2:00
	0:09 - 0:20
	0:55 - 1:10
	0:25 - 0:55
	0:15 - 0:25
	
	

	below -25 to -29 °C
(below -13 to -20 °F)
	100/0
	0:55 - 2:00
	0:07 - 0:15
	0:45 - 0:55
	0:20 - 0:45
	0:10 - 0:20
	
	


NOTES
1. Ensure that the lowest operational use temperature (LOUT) is respected. Consider use of Type I fluid when Type IV fluid cannot be used.
Freezing mist is best confirmed by observation. It is never reported by METAR; however, it can occur when mist is present at 0 °C (32 °F) and below. 
Use freezing fog holdover times in conditions of ice crystals mixed with freezing fog or freezing mist.
To determine snowfall intensity, the Snowfall Intensities as a Function of Prevailing Visibility table (Table 57) is required. No holdover times exist if the reported visibility correlates to a “heavy” precipitation intensity. 
Use snow holdover times in conditions of very light, light, or moderate snow mixed with ice crystals.
Includes light, moderate and heavy freezing drizzle. Use light freezing rain holdover times if positive identification of freezing drizzle is not possible.
These holdover times apply to conditions of “moderate” precipitation intensity. In cases of very light or light snow mixed with light rain or drizzle, use light freezing rain holdover times. The Snowfall Intensities as a Function of Prevailing Visibility table (Table 57) is required to confirm the precipitation intensity. No holdover times exist if the reported visibility correlates to a “heavy” precipitation intensity.
No holdover time guidelines exist for this condition for 0 °C (32 °F) and below.
Heavy snow, ice pellets, moderate and heavy freezing rain, small hail and hail (Table 55 provides allowance times for Type IV EG fluids in ice pellets and small hail).
No holdover time guidelines exist for this condition below -10 °C (14 °F).
CAUTIONS
The cautions that apply to the holdover times in the table above can be found on page 32.


[bookmark: _Toc234306067][bookmark: _Toc43986172]Table 27: Type IV Holdover Times for ASGlobal 4Flite EG
	Outside Air 
Temperature1
	Fluid 
Concentration 
Fluid/Water 
By % Volume
	Freezing Fog, Freezing Mist2, or Ice Crystals3
	Snow 
mixed with 
Freezing Fog4
	Very Light Snow, Snow Grains or Snow Pellets4,5
	Light 
Snow, Snow Grains or Snow Pellets4,5
	Moderate Snow, Snow Grains or Snow Pellets4,5
	Freezing 
Drizzle6
	Light 
Freezing Rain
	Moderate
Snow mixed with Rain7,8
	Rain on 
Cold‑Soaked Wing8
	Other9

	-3 °C and above
(27 °F and above)
	100/0
	1:35 - 3:15
	0:25 - 0:45
	2:05 - 2:35
	1:00 - 2:05
	0:30 - 1:00
	0:40 - 1:10
	0:20 - 0:35
	0:06 - 0:06
	0:08 - 1:05
	 

	
	75/25
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	 

	
	50/50
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	CAUTION: 
No holdover time 
guidelines exist

	below -3 to -8 °C
(below 27 to 18 °F)
	100/0
	1:25 - 2:45
	0:20 - 0:40
	1:50 - 2:15
	0:55 - 1:50
	0:25 - 0:55
	0:40 - 1:10
	0:20 - 0:35
	

	
	75/25
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	

	below -8 to -14 °C
(below 18 to 7 °F)
	100/0
	1:25 - 2:45
	0:20 - 0:35
	1:35 - 2:00
	0:50 - 1:35
	0:25 - 0:50
	0:40 - 1:1010
	0:20 - 0:3510
	

	
	75/25
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	

	below -14 to -18 °C
(below 7 to 0 °F)
	100/0
	0:50 - 1:25
	0:15 - 0:35
	1:35 - 2:00
	0:45 - 1:35
	0:20 - 0:45
	
	

	below -18 to -25 °C
(below 0 to -13 °F)
	100/0
	0:50 - 1:25
	0:15 - 0:30
	1:20 - 1:40
	0:35 - 1:20
	0:20 - 0:35
	
	

	below -25 to -30 °C
(below -13 to -22 °F)
	100/0
	0:30 - 1:05
	0:09 - 0:20
	0:55 - 1:05
	0:25 - 0:55
	0:10 - 0:25
	
	


NOTES
1. Ensure that the lowest operational use temperature (LOUT) is respected. Consider use of Type I fluid when Type IV fluid cannot be used.
Freezing mist is best confirmed by observation. It is never reported by METAR; however, it can occur when mist is present at 0 °C (32 °F) and below. 
Use freezing fog holdover times in conditions of ice crystals mixed with freezing fog or freezing mist.
To determine snowfall intensity, the Snowfall Intensities as a Function of Prevailing Visibility table (Table 57) is required. No holdover times exist if the reported visibility correlates to a “heavy” precipitation intensity. 
Use snow holdover times in conditions of very light, light, or moderate snow mixed with ice crystals.
Includes light, moderate and heavy freezing drizzle. Use light freezing rain holdover times if positive identification of freezing drizzle is not possible.
These holdover times apply to conditions of “moderate” precipitation intensity. In cases of very light or light snow mixed with light rain or drizzle, use light freezing rain holdover times. The Snowfall Intensities as a Function of Prevailing Visibility table (Table 57) is required to confirm the precipitation intensity. No holdover times exist if the reported visibility correlates to a “heavy” precipitation intensity.
No holdover time guidelines exist for this condition for 0 °C (32 °F) and below.
Heavy snow, ice pellets, moderate and heavy freezing rain, small hail and hail.
No holdover time guidelines exist for this condition below -10 °C (14 °F).
CAUTIONS
The cautions that apply to the holdover times in the table above can be found on page 32.


[bookmark: _Toc234306068]Table 28: Type IV Holdover Times for ASGlobal 4Flite PG
	Outside Air 
Temperature1
	Fluid 
Concentration 
Fluid/Water 
By % Volume
	Freezing Fog, Freezing Mist2, or Ice Crystals3
	Snow 
mixed with 
Freezing Fog4
	Very Light Snow, Snow Grains or Snow Pellets4,5
	Light 
Snow, Snow Grains or Snow Pellets4,5
	Moderate Snow, Snow Grains or Snow Pellets4,5
	Freezing 
Drizzle6
	Light 
Freezing Rain
	Moderate
Snow mixed with Rain7,8
	Rain on 
Cold‑Soaked Wing8
	Other9

	-3 °C and above
(27 °F and above)
	100/0
	1:50 - 3:15
	0:40 - 1:10
	2:50 - 3:00
	1:35 - 2:50
	0:50 - 1:35
	1:10 - 1:35
	0:45 - 1:05
	0:15 - 0:15
	0:15 - 1:20
	 

	
	75/25
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	 

	
	50/50
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	CAUTION: 
No holdover time 
guidelines exist

	below -3 to -8 °C
(below 27 to 18 °F)
	100/0
	1:05 - 1:55
	0:30 - 0:50
	2:05 - 2:30
	1:10 - 2:05
	0:35 - 1:10
	0:55 - 1:10
	0:35 - 0:55
	

	
	75/25
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	

	below -8 to -14 °C
(below 18 to 7 °F)
	100/0
	1:05 - 1:55
	0:20 - 0:40
	1:40 - 2:00
	0:55 - 1:40
	0:30 - 0:55
	0:55 - 1:1010
	0:35 - 0:5510
	

	
	75/25
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	

	below -14 to -18 °C
(below 7 to 0 °F)
	100/0
	0:30 - 0:45
	0:15 - 0:25
	1:05 - 1:20
	0:35 - 1:05
	0:15 - 0:35
	
	

	below -18 to -25 °C
(below 0 to -13 °F)
	100/0
	0:30 - 0:45
	0:07 - 0:15
	0:35 - 0:45
	0:20 - 0:35
	0:09 - 0:20
	
	

	below -25 to -26 °C
(below -13 to -15 °F)
	100/0
	0:30 - 0:45
	0:06 - 0:15
	0:35 - 0:45
	0:20 - 0:35
	0:08 - 0:20
	
	


NOTES
1. Ensure that the lowest operational use temperature (LOUT) is respected. Consider use of Type I fluid when Type IV fluid cannot be used.
Freezing mist is best confirmed by observation. It is never reported by METAR; however, it can occur when mist is present at 0 °C (32 °F) and below. 
Use freezing fog holdover times in conditions of ice crystals mixed with freezing fog or freezing mist.
To determine snowfall intensity, the Snowfall Intensities as a Function of Prevailing Visibility table (Table 57) is required. No holdover times exist if the reported visibility correlates to a “heavy” precipitation intensity. 
Use snow holdover times in conditions of very light, light, or moderate snow mixed with ice crystals.
Includes light, moderate and heavy freezing drizzle. Use light freezing rain holdover times if positive identification of freezing drizzle is not possible.
These holdover times apply to conditions of “moderate” precipitation intensity. In cases of very light or light snow mixed with light rain or drizzle, use light freezing rain holdover times. The Snowfall Intensities as a Function of Prevailing Visibility table (Table 57) is required to confirm the precipitation intensity. No holdover times exist if the reported visibility correlates to a “heavy” precipitation intensity.
No holdover time guidelines exist for this condition for 0 °C (32 °F) and below.
Heavy snow, ice pellets, moderate and heavy freezing rain, small hail and hail (Table 56 provides allowance times for Type IV PG fluids in ice pellets and small hail).
No holdover time guidelines exist for this condition below -10 °C (14 °F).
CAUTIONS
The cautions that apply to the holdover times in the table above can be found on page 32.


[bookmark: _Toc234306069]Table 29: Type IV Holdover Times for AVIAFLUID AVIAFlight PG
	Outside Air 
Temperature1
	Fluid 
Concentration 
Fluid/Water 
By % Volume
	Freezing Fog, Freezing Mist2, or Ice Crystals3
	Snow 
mixed with 
Freezing Fog4
	Very Light Snow, Snow Grains or Snow Pellets4,5
	Light 
Snow, Snow Grains or Snow Pellets4,5
	Moderate Snow, Snow Grains or Snow Pellets4,5
	Freezing 
Drizzle6
	Light 
Freezing Rain
	Moderate
Snow mixed with Rain7,8
	Rain on 
Cold‑Soaked Wing8
	Other9

	-3 °C and above
(27 °F and above)
	100/0
	2:15 - 4:00
	0:40 - 1:15
	3:00 - 3:00
	1:40 - 3:00
	0:55 - 1:40
	2:00 - 2:00
	1:10 - 1:55
	0:15 - 0:15
	0:20 - 2:00
	 

	
	75/25
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	 

	
	50/50
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	CAUTION: 
No holdover time 
guidelines exist

	below -3 to -8 °C
(below 27 to 18 °F)
	100/0
	1:05 - 2:10
	0:25 - 0:50
	2:00 - 2:25
	1:05 - 2:00
	0:35 - 1:05
	0:35 - 1:55
	0:45 - 1:05
	

	
	75/25
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	

	below -8 to -14 °C
(below 18 to 7 °F)
	100/0
	1:05 - 2:10
	0:20 - 0:35
	1:30 - 1:50
	0:50 - 1:30
	0:25 - 0:50
	0:35 - 1:5510
	0:45 - 1:0510
	

	
	75/25
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	

	below -14 to -18 °C
(below 7 to 0 °F)
	100/0
	0:20 - 0:35
	0:10 - 0:20
	0:50 - 1:00
	0:25 - 0:50
	0:15 - 0:25
	
	

	below -18 to -25 °C
(below 0 to -13 °F)
	100/0
	0:20 - 0:35
	0:05 - 0:09
	0:25 - 0:30
	0:15 - 0:25
	0:06 - 0:15
	
	

	below -25 to -25.5 °C
(below -13 to -14 °F)
	100/0
	0:20 - 0:35
	0:05 - 0:09
	0:25 - 0:30
	0:10 - 0:25
	0:06 - 0:10
	
	


NOTES
1. Ensure that the lowest operational use temperature (LOUT) is respected. Consider use of Type I fluid when Type IV fluid cannot be used.
1. Freezing mist is best confirmed by observation. It is never reported by METAR; however, it can occur when mist is present at 0 °C (32 °F) and below. 
1. Use freezing fog holdover times in conditions of ice crystals mixed with freezing fog or freezing mist.
1. To determine snowfall intensity, the Snowfall Intensities as a Function of Prevailing Visibility table (Table 57) is required. No holdover times exist if the reported visibility correlates to a “heavy” precipitation intensity. 
Use snow holdover times in conditions of very light, light, or moderate snow mixed with ice crystals.
Includes light, moderate and heavy freezing drizzle. Use light freezing rain holdover times if positive identification of freezing drizzle is not possible.
These holdover times apply to conditions of “moderate” precipitation intensity. In cases of very light or light snow mixed with light rain or drizzle, use light freezing rain holdover times. The Snowfall Intensities as a Function of Prevailing Visibility table (Table 57) is required to confirm the precipitation intensity. No holdover times exist if the reported visibility correlates to a “heavy” precipitation intensity.
No holdover time guidelines exist for this condition for 0 °C (32 °F) and below.
Heavy snow, ice pellets, moderate and heavy freezing rain, small hail and hail (Table 56 provides allowance times for Type IV PG fluids in ice pellets and small hail).
No holdover time guidelines exist for this condition below -10 °C (14 °F).
CAUTIONS
The cautions that apply to the holdover times in the table above can be found on page 32.


[bookmark: _Toc234306070]Table 30: Type IV Holdover Times for CHEMCO ChemR EG IV
	Outside Air 
Temperature1
	Fluid 
Concentration 
Fluid/Water 
By % Volume
	Freezing Fog, Freezing Mist2, or Ice Crystals3
	Snow 
mixed with 
Freezing Fog4
	Very Light Snow, Snow Grains or Snow Pellets4,5
	Light 
Snow, Snow Grains or Snow Pellets4,5
	Moderate Snow, Snow Grains or Snow Pellets4,5
	Freezing 
Drizzle6
	Light 
Freezing Rain
	Moderate
Snow mixed with Rain7,8
	Rain on 
Cold‑Soaked Wing8
	Other9

	-3 °C and above
(27 °F and above)
	100/0
	2:05 - 3:35
	0:20 - 0:50
	2:25 - 3:00
	1:05 - 2:25
	0:30 - 1:05
	0:45 - 1:40
	0:25 - 0:40
	0:07 - 0:07
	0:09 - 1:45
	 

	
	75/25
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	 

	
	50/50
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	CAUTION: 
No holdover time 
guidelines exist

	below -3 to -8 °C
(below 27 to 18 °F)
	100/0
	1:25 - 3:40
	0:20 - 0:50
	2:25 - 3:00
	1:05 - 2:25
	0:30 - 1:05
	1:00 - 1:35
	0:35 - 0:50
	

	
	75/25
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	

	below -8 to -14 °C
(below 18 to 7 °F)
	100/0
	1:25 - 3:40
	0:20 - 0:50
	2:25 - 3:00
	1:05 - 2:25
	0:30 - 1:05
	1:00 - 1:3510
	0:35 - 0:5010
	

	
	75/25
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	

	below -14 to -18 °C
(below 7 to 0 °F)
	100/0
	0:40 - 1:25
	0:10 - 0:25
	1:05 - 1:25
	0:35 - 1:05
	0:15 - 0:35
	
	

	below -18 to -25 °C
(below 0 to -13 °F)
	100/0
	0:40 - 1:25
	0:10 - 0:25
	1:05 - 1:25
	0:35 - 1:05
	0:15 - 0:35
	
	

	below -25 to -27 °C
(below -13 to -17 °F)
	100/0
	0:40 - 1:25
	0:10 - 0:25
	1:05 - 1:25
	0:35 - 1:05
	0:15 - 0:35
	
	


NOTES
1. Ensure that the lowest operational use temperature (LOUT) is respected. Consider use of Type I fluid when Type IV fluid cannot be used.
1. Freezing mist is best confirmed by observation. It is never reported by METAR; however, it can occur when mist is present at 0 °C (32 °F) and below. 
1. Use freezing fog holdover times in conditions of ice crystals mixed with freezing fog or freezing mist.
1. To determine snowfall intensity, the Snowfall Intensities as a Function of Prevailing Visibility table (Table 57) is required. No holdover times exist if the reported visibility correlates to a “heavy” precipitation intensity. 
Use snow holdover times in conditions of very light, light, or moderate snow mixed with ice crystals.
Includes light, moderate and heavy freezing drizzle. Use light freezing rain holdover times if positive identification of freezing drizzle is not possible.,
These holdover times apply to conditions of “moderate” precipitation intensity. In cases of very light or light snow mixed with light rain or drizzle, use light freezing rain holdover times. The Snowfall Intensities as a Function of Prevailing Visibility table (Table 57) is required to confirm the precipitation intensity. No holdover times exist if the reported visibility correlates to a “heavy” precipitation intensity.
No holdover time guidelines exist for this condition for 0 °C (32 °F) and below.
Heavy snow, ice pellets, moderate and heavy freezing rain, small hail and hail (Table 55 provides allowance times for Type IV EG fluids in ice pellets and small hail).
No holdover time guidelines exist for this condition below -10 °C (14 °F).
CAUTIONS
The cautions that apply to the holdover times in the table above can be found on page 32.


[bookmark: _TABLE_4C._TYPE][bookmark: _Toc234306071][bookmark: _Toc508704824][bookmark: _Toc14867854][bookmark: _Toc508704825][bookmark: _Toc43986173][bookmark: _Toc436349438]Table 31: Type IV Holdover Times for CHEMCO ChemR Nordik IV
	Outside Air 
Temperature1
	Fluid 
Concentration 
Fluid/Water 
By % Volume
	Freezing Fog, Freezing Mist2, or Ice Crystals3
	Snow 
mixed with 
Freezing Fog4
	Very Light Snow, Snow Grains or Snow Pellets4,5
	Light 
Snow, Snow Grains or Snow Pellets4,5
	Moderate Snow, Snow Grains or Snow Pellets4,5
	Freezing 
Drizzle6
	Light 
Freezing Rain
	Moderate
Snow mixed with Rain7,8
	Rain on 
Cold‑Soaked Wing8
	Other9

	-3 °C and above
(27 °F and above)
	100/0
	2:15 - 4:00
	0:35 - 1:10
	2:50 - 3:00
	1:30 - 2:50
	0:50 - 1:30
	1:20 - 2:00
	0:55 - 1:20
	0:15 - 0:15
	0:25 - 2:00
	 

	
	75/25
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	 

	
	50/50
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	CAUTION: 
No holdover time 
guidelines exist

	below -3 to -8 °C
(below 27 to 18 °F)
	100/0
	1:50 - 4:00
	0:35 - 1:10
	2:50 - 3:00
	1:30 - 2:50
	0:50 - 1:30
	1:15 - 2:00
	0:45 - 1:20
	

	
	75/25
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	

	below -8 to -14 °C
(below 18 to 7 °F)
	100/0
	1:50 - 4:00
	0:35 - 1:10
	2:50 - 3:00
	1:30 - 2:50
	0:50 - 1:30
	1:15 - 2:0010
	0:45 - 1:2010
	

	
	75/25
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	

	below -14 to -18 °C
(below 7 to 0 °F)
	100/0
	0:40 - 1:30
	0:35 - 1:10
	3:00 - 3:00
	1:35 - 3:00
	0:50 - 1:35
	
	

	below -18 to -25 °C
(below 0 to -13 °F)
	100/0
	0:40 - 1:30
	0:25 - 0:50
	2:10 - 2:40
	1:05 - 2:10
	0:35 - 1:05
	
	

	below -25 to -29 °C
(below -13 to -20 °F)
	100/0
	0:40 - 1:30
	0:20 - 0:40
	1:50 - 2:15
	0:55 - 1:50
	0:30 - 0:55
	
	


NOTES
1. Ensure that the lowest operational use temperature (LOUT) is respected. Consider use of Type I fluid when Type IV fluid cannot be used.
1. Freezing mist is best confirmed by observation. It is never reported by METAR; however, it can occur when mist is present at 0 °C (32 °F) and below. 
1. Use freezing fog holdover times in conditions of ice crystals mixed with freezing fog or freezing mist.
1. To determine snowfall intensity, the Snowfall Intensities as a Function of Prevailing Visibility table (Table 57) is required. No holdover times exist if the reported visibility correlates to a “heavy” precipitation intensity. 
Use snow holdover times in conditions of very light, light, or moderate snow mixed with ice crystals.
Includes light, moderate and heavy freezing drizzle. Use light freezing rain holdover times if positive identification of freezing drizzle is not possible.
These holdover times apply to conditions of “moderate” precipitation intensity. In cases of very light or light snow mixed with light rain or drizzle, use light freezing rain holdover times. The Snowfall Intensities as a Function of Prevailing Visibility table (Table 57) is required to confirm the precipitation intensity. No holdover times exist if the reported visibility correlates to a “heavy” precipitation intensity.
No holdover time guidelines exist for this condition for 0 °C (32 °F) and below.
Heavy snow, ice pellets, moderate and heavy freezing rain, small hail and hail (Table 55 provides allowance times for Type IV EG fluids in ice pellets and small hail).
No holdover time guidelines exist for this condition below -10 °C (14 °F).
CAUTIONS
The cautions that apply to the holdover times in the table above can be found on page 32.


[bookmark: _Toc234306072]Table 32: Type IV Holdover Times for Chongqing Joba Chemical FW-IV
	Outside Air 
Temperature1
	Fluid 
Concentration 
Fluid/Water 
By % Volume
	Freezing Fog, Freezing Mist2, or Ice Crystals3
	Snow 
mixed with 
Freezing Fog4
	Very Light Snow, Snow Grains or Snow Pellets4,5
	Light 
Snow, Snow Grains or Snow Pellets4,5
	Moderate Snow, Snow Grains or Snow Pellets4,5
	Freezing 
Drizzle6
	Light 
Freezing Rain
	Moderate
Snow mixed with Rain7,8
	Rain on 
Cold‑Soaked Wing8
	Other9

	-3 °C and above
(27 °F and above)
	100/0
	3:15 - 4:00
	0:35 - 1:15
	3:00 - 3:00
	1:40 - 3:00
	0:50 - 1:40
	1:30 - 2:00
	0:45 - 1:05
	0:10 - 0:10
	0:15 - 2:00
	 

	
	75/25
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	 

	
	50/50
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	CAUTION: 
No holdover time 
guidelines exist

	below -3 to -8 °C
(below 27 to 18 °F)
	100/0
	2:30 - 4:00
	0:30 - 1:00
	2:45 - 3:00
	1:25 - 2:45
	0:40 - 1:25
	0:50 - 2:00
	0:35 - 1:10
	

	
	75/25
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	

	below -8 to -14 °C
(below 18 to 7 °F)
	100/0
	2:30 - 4:00
	0:30 - 0:55
	2:25 - 3:00
	1:15 - 2:25
	0:35 - 1:15
	0:50 - 2:0010
	0:35 - 1:1010
	

	
	75/25
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	

	below -14 to -18 °C
(below 7 to 0 °F)
	100/0
	0:35 - 1:40
	0:20 - 0:40
	2:00 - 2:35
	0:55 - 2:00
	0:25 - 0:55
	
	

	below -18 to -25 °C
(below 0 to -13 °F)
	100/0
	0:35 - 1:40
	0:15 - 0:30
	1:20 - 1:45
	0:35 - 1:20
	0:15 - 0:35
	
	

	below -25 to -29 °C
(below -13 to -20 °F)
	100/0
	0:35 - 1:40
	0:10 - 0:25
	1:10 - 1:30
	0:30 - 1:10
	0:15 - 0:30
	
	


NOTES
1. Ensure that the lowest operational use temperature (LOUT) is respected. Consider use of Type I fluid when Type IV fluid cannot be used.
Freezing mist is best confirmed by observation. It is never reported by METAR; however, it can occur when mist is present at 0 °C (32 °F) and below. 
Use freezing fog holdover times in conditions of ice crystals mixed with freezing fog or freezing mist.
To determine snowfall intensity, the Snowfall Intensities as a Function of Prevailing Visibility table (Table 57) is required. No holdover times exist if the reported visibility correlates to a “heavy” precipitation intensity. 
Use snow holdover times in conditions of very light, light, or moderate snow mixed with ice crystals.
Includes light, moderate and heavy freezing drizzle. Use light freezing rain holdover times if positive identification of freezing drizzle is not possible.
These holdover times apply to conditions of “moderate” precipitation intensity. In cases of very light or light snow mixed with light rain or drizzle, use light freezing rain holdover times. The Snowfall Intensities as a Function of Prevailing Visibility table (Table 57) is required to confirm the precipitation intensity. No holdover times exist if the reported visibility correlates to a “heavy” precipitation intensity.
No holdover time guidelines exist for this condition for 0 °C (32 °F) and below.
Heavy snow, ice pellets, moderate and heavy freezing rain, small hail and hail (Table 55 provides allowance times for Type IV EG fluids in ice pellets and small hail).
No holdover time guidelines exist for this condition below -10 °C (14 °F).
CAUTIONS
The cautions that apply to the holdover times in the table above can be found on page 32.


[bookmark: _TABLE_4D._TYPE_1][bookmark: _TABLE_4D._TYPE][bookmark: _TABLE_4F._TYPE_1][bookmark: _Toc436349439][bookmark: _Toc508704828][bookmark: _Toc43986176][bookmark: _Toc234306073]Table 33: Type IV Holdover Times for Clariant Safewing MP IV LAUNCH
	Outside Air 
Temperature1
	Fluid 
Concentration 
Fluid/Water 
By % Volume
	Freezing Fog, Freezing Mist2, or Ice Crystals3
	Snow 
mixed with 
Freezing Fog4
	Very Light Snow, Snow Grains or Snow Pellets4,5
	Light 
Snow, Snow Grains or Snow Pellets4,5
	Moderate Snow, Snow Grains or Snow Pellets4,5
	Freezing 
Drizzle6
	Light 
Freezing Rain
	Moderate
Snow mixed with Rain7,8
	Rain on 
Cold‑Soaked Wing8
	Other9

	-3 °C and above
(27 °F and above)
	100/0
	4:00 - 4:00
	0:50 - 1:20
	2:50 - 3:00
	1:45 - 2:50
	1:05 - 1:45
	1:30 - 2:00
	1:00 - 1:40
	0:10 - 0:10
	0:15 - 1:40
	 

	
	75/25
	3:40 - 4:00
	0:45 - 1:20
	3:00 - 3:00
	1:45 - 3:00
	1:00 - 1:45
	1:40 - 2:00
	0:45 - 1:15
	0:08 - 0:08
	0:10 - 1:45
	 

	
	50/50
	1:25 - 2:45
	0:20 - 0:35
	1:25 - 1:40
	0:45 - 1:25
	0:25 - 0:45
	0:30 - 0:50
	0:20 - 0:25
	CAUTION: 
No holdover time 
guidelines exist

	below -3 to -8 °C
(below 27 to 18 °F)
	100/0
	1:00 - 1:55
	0:40 - 1:05
	2:25 - 2:50
	1:30 - 2:25
	0:55 - 1:30
	0:35 - 1:40
	0:25 - 0:45
	

	
	75/25
	0:40 - 1:20
	0:40 - 1:10
	2:40 - 3:00
	1:30 - 2:40
	0:50 - 1:30
	0:25 - 1:10
	0:25 - 0:45
	

	below -8 to -14 °C
(below 18 to 7 °F)
	100/0
	1:00 - 1:55
	0:35 - 1:00
	2:10 - 2:30
	1:20 - 2:10
	0:50 - 1:20
	0:35 - 1:4010
	0:25 - 0:4510
	

	
	75/25
	0:40 - 1:20
	0:35 - 1:00
	2:25 - 2:55
	1:25 - 2:25
	0:45 - 1:25
	0:25 - 1:1010
	0:25 - 0:4510
	

	below -14 to -18 °C
(below 7 to 0 °F)
	100/0
	0:30 - 0:50
	0:05 - 0:15
	1:15 - 1:45
	0:20 - 1:15
	0:06 - 0:20
	
	

	below -18 to -25 °C
(below 0 to -13 °F)
	100/0
	0:30 - 0:50
	0:02 - 0:06
	0:30 - 0:45
	0:09 - 0:30
	0:02 - 0:09
	
	

	below -25 to -28.5 °C
(below -13 to -19 °F)
	100/0
	0:30 - 0:50
	0:01 - 0:04
	0:20 - 0:30
	0:06 - 0:20
	0:01 - 0:06
	
	


NOTES
1. Ensure that the lowest operational use temperature (LOUT) is respected. Consider use of Type I fluid when Type IV fluid cannot be used.
1. Freezing mist is best confirmed by observation. It is never reported by METAR; however, it can occur when mist is present at 0 °C (32 °F) and below. 
1. Use freezing fog holdover times in conditions of ice crystals mixed with freezing fog or freezing mist.
1. To determine snowfall intensity, the Snowfall Intensities as a Function of Prevailing Visibility table (Table 57) is required. No holdover times exist if the reported visibility correlates to a “heavy” precipitation intensity. 
Use snow holdover times in conditions of very light, light, or moderate snow mixed with ice crystals.
Includes light, moderate and heavy freezing drizzle. Use light freezing rain holdover times if positive identification of freezing drizzle is not possible.
These holdover times apply to conditions of “moderate” precipitation intensity. In cases of very light or light snow mixed with light rain or drizzle, use light freezing rain holdover times. The Snowfall Intensities as a Function of Prevailing Visibility table (Table 57) is required to confirm the precipitation intensity. No holdover times exist if the reported visibility correlates to a “heavy” precipitation intensity.
No holdover time guidelines exist for this condition for 0 °C (32 °F) and below.
Heavy snow, ice pellets, moderate and heavy freezing rain, small hail and hail (Table 56 provides allowance times for Type IV PG fluids in ice pellets and small hail).
No holdover time guidelines exist for this condition below -10 °C (14 °F).
CAUTIONS
The cautions that apply to the holdover times in the table above can be found on page 32.


[bookmark: _Table_4E._Type][bookmark: _Toc425184881][bookmark: _Toc436349440][bookmark: _Toc508704829][bookmark: _Toc43986177][bookmark: _Toc234306074]Table 34: Type IV Holdover Times for Clariant Safewing MP IV LAUNCH PLUS
	Outside Air 
Temperature1
	Fluid 
Concentration 
Fluid/Water 
By % Volume
	Freezing Fog, Freezing Mist2, or Ice Crystals3
	Snow 
mixed with 
Freezing Fog4
	Very Light Snow, Snow Grains or Snow Pellets4,5
	Light 
Snow, Snow Grains or Snow Pellets4,5
	Moderate Snow, Snow Grains or Snow Pellets4,5
	Freezing 
Drizzle6
	Light 
Freezing Rain
	Moderate
Snow mixed with Rain7,8
	Rain on 
Cold‑Soaked Wing8
	Other9

	-3 °C and above
(27 °F and above)
	100/0
	3:55 - 4:00
	0:40 - 1:35
	3:00 - 3:00
	2:05 - 3:00
	0:55 - 2:05
	2:00 - 2:00
	1:00 - 2:00
	0:15 - 0:15
	0:20 - 2:00
	 

	
	75/25
	3:55 - 4:00
	0:35 - 1:25
	3:00 - 3:00
	1:55 - 3:00
	0:50 - 1:55
	2:00 - 2:00
	1:20 - 1:25
	0:15 - 0:15
	0:20 - 1:50
	 

	
	50/50
	1:15 - 1:50
	0:15 - 0:35
	1:35 - 2:00
	0:45 - 1:35
	0:20 - 0:45
	0:25 - 1:00
	0:15 - 0:20
	CAUTION: 
No holdover time 
guidelines exist

	below -3 to -8 °C
(below 27 to 18 °F)
	100/0
	0:55 - 2:15
	0:35 - 1:15
	3:00 - 3:00
	1:40 - 3:00
	0:45 - 1:40
	0:25 - 1:35
	0:25 - 0:40
	

	
	75/25
	0:40 - 2:00
	0:30 - 1:05
	3:00 - 3:00
	1:30 - 3:00
	0:35 - 1:30
	0:20 - 1:05
	0:20 - 0:30
	

	below -8 to -14 °C
(below 18 to 7 °F)
	100/0
	0:55 - 2:15
	0:30 - 1:05
	3:00 - 3:00
	1:25 - 3:00
	0:40 - 1:25
	0:25 - 1:3510
	0:25 - 0:4010
	

	
	75/25
	0:40 - 2:00
	0:25 - 0:55
	2:55 - 3:00
	1:15 - 2:55
	0:30 - 1:15
	0:20 - 1:0510
	0:20 - 0:3010
	

	below -14 to -18 °C
(below 7 to 0 °F)
	100/0
	0:25 - 0:50
	0:05 - 0:20
	1:15 - 1:50
	0:25 - 1:15
	0:07 - 0:25
	
	

	below -18 to -25 °C
(below 0 to -13 °F)
	100/0
	0:25 - 0:50
	0:02 - 0:07
	0:30 - 0:45
	0:09 - 0:30
	0:03 - 0:09
	
	

	below -25 to -29 °C
(below -13 to -20 °F)
	100/0
	0:25 - 0:50
	0:01 - 0:04
	0:20 - 0:30
	0:06 - 0:20
	0:02 - 0:06
	
	


NOTES
1. Ensure that the lowest operational use temperature (LOUT) is respected. Consider use of Type I fluid when Type IV fluid cannot be used.
1. Freezing mist is best confirmed by observation. It is never reported by METAR; however, it can occur when mist is present at 0 °C (32 °F) and below. 
1. Use freezing fog holdover times in conditions of ice crystals mixed with freezing fog or freezing mist.
1. To determine snowfall intensity, the Snowfall Intensities as a Function of Prevailing Visibility table (Table 57) is required. No holdover times exist if the reported visibility correlates to a “heavy” precipitation intensity. 
Use snow holdover times in conditions of very light, light, or moderate snow mixed with ice crystals.
Includes light, moderate and heavy freezing drizzle. Use light freezing rain holdover times if positive identification of freezing drizzle is not possible.
These holdover times apply to conditions of “moderate” precipitation intensity. In cases of very light or light snow mixed with light rain or drizzle, use light freezing rain holdover times. The Snowfall Intensities as a Function of Prevailing Visibility table (Table 57) is required to confirm the precipitation intensity. No holdover times exist if the reported visibility correlates to a “heavy” precipitation intensity.
No holdover time guidelines exist for this condition for 0 °C (32 °F) and below.
Heavy snow, ice pellets, moderate and heavy freezing rain, small hail and hail (Table 56 provides allowance times for Type IV PG fluids in ice pellets and small hail).
No holdover time guidelines exist for this condition below -10 °C (14 °F).
CAUTIONS
The cautions that apply to the holdover times in the table above can be found on page 32.
[bookmark: _TABLE_4F._TYPE][bookmark: _TABLE_4G._TYPE][bookmark: _TABLE_4H._TYPE][bookmark: _Toc436349442][bookmark: _Toc436349443]

[bookmark: _Toc508704830][bookmark: _Toc43986178][bookmark: _Toc234306075]Table 35: Type IV Holdover Times for Cryotech Polar Guard® Advance
	Outside Air 
Temperature1
	Fluid 
Concentration 
Fluid/Water 
By % Volume
	Freezing Fog, Freezing Mist2, or Ice Crystals3
	Snow 
mixed with 
Freezing Fog4
	Very Light Snow, Snow Grains or Snow Pellets4,5
	Light 
Snow, Snow Grains or Snow Pellets4,5
	Moderate Snow, Snow Grains or Snow Pellets4,5
	Freezing 
Drizzle6
	Light 
Freezing Rain
	Moderate
Snow mixed with Rain7,8
	Rain on 
Cold‑Soaked Wing8
	Other9

	-3 °C and above
(27 °F and above)
	100/0
	2:50 - 4:00
	0:50 - 1:25
	3:00 - 3:00
	1:55 - 3:00
	1:05 - 1:55
	1:35 - 2:00
	1:15 - 1:30
	0:10 - 0:10
	0:15 - 2:00
	 

	
	75/25
	2:30 - 4:00
	0:30 - 1:05
	3:00 - 3:00
	1:25 - 3:00
	0:40 - 1:25
	1:40 - 2:00
	0:40 - 1:10
	0:07 - 0:07
	0:09 - 1:40
	 

	
	50/50
	0:50 - 1:25
	0:07 - 0:20
	1:10 - 1:35
	0:25 - 1:10
	0:10 - 0:25
	0:20 - 0:45
	0:09 - 0:20
	CAUTION: 
No holdover time 
guidelines exist

	below -3 to -8 °C
(below 27 to 18 °F)
	100/0
	0:55 - 2:30
	0:35 - 1:05
	2:25 - 2:50
	1:25 - 2:25
	0:50 - 1:25
	0:35 - 1:35
	0:35 - 0:45
	

	
	75/25
	0:40 - 1:30
	0:25 - 0:50
	2:20 - 3:00
	1:05 - 2:20
	0:30 - 1:05
	0:25 - 1:05
	0:35 - 0:45
	

	below -8 to -14 °C
(below 18 to 7 °F)
	100/0
	0:55 - 2:30
	0:30 - 0:50
	2:00 - 2:20
	1:10 - 2:00
	0:40 - 1:10
	0:35 - 1:3510
	0:35 - 0:4510
	

	
	75/25
	0:40 - 1:30
	0:20 - 0:45
	2:00 - 2:30
	0:55 - 2:00
	0:25 - 0:55
	0:25 - 1:0510
	0:35 - 0:4510
	

	below -14 to -18 °C
(below 7 to 0 °F)
	100/0
	0:25 - 0:50
	0:08 - 0:25
	1:35 - 2:15
	0:35 - 1:35
	0:10 - 0:35
	
	

	below -18 to -25 °C
(below 0 to -13 °F)
	100/0
	0:25 - 0:50
	0:03 - 0:10
	0:40 - 0:55
	0:15 - 0:40
	0:04 - 0:15
	
	

	below -25 to -30.5 °C
(below -13 to -23 °F)
	100/0
	0:25 - 0:50
	0:02 - 0:05
	0:25 - 0:30
	0:07 - 0:25
	0:02 - 0:07
	
	


NOTES
1. Ensure that the lowest operational use temperature (LOUT) is respected. Consider use of Type I fluid when Type IV fluid cannot be used.
1. Freezing mist is best confirmed by observation. It is never reported by METAR; however, it can occur when mist is present at 0 °C (32 °F) and below. 
1. Use freezing fog holdover times in conditions of ice crystals mixed with freezing fog or freezing mist.
1. To determine snowfall intensity, the Snowfall Intensities as a Function of Prevailing Visibility table (Table 57) is required. No holdover times exist if the reported visibility correlates to a “heavy” precipitation intensity. 
Use snow holdover times in conditions of very light, light, or moderate snow mixed with ice crystals.
Includes light, moderate and heavy freezing drizzle. Use light freezing rain holdover times if positive identification of freezing drizzle is not possible.
These holdover times apply to conditions of “moderate” precipitation intensity. In cases of very light or light snow mixed with light rain or drizzle, use light freezing rain holdover times. The Snowfall Intensities as a Function of Prevailing Visibility table (Table 57) is required to confirm the precipitation intensity. No holdover times exist if the reported visibility correlates to a “heavy” precipitation intensity.
No holdover time guidelines exist for this condition for 0 °C (32 °F) and below.
Heavy snow, ice pellets, moderate and heavy freezing rain, small hail and hail (Table 56 provides allowance times for Type IV PG fluids in ice pellets and small hail).
No holdover time guidelines exist for this condition below -10 °C (14 °F).
CAUTIONS
The cautions that apply to the holdover times in the table above can be found on page 32.
[bookmark: _TABLE_4I._TYPE_1]

[bookmark: _Toc43986179][bookmark: _Toc234306076][bookmark: _Toc436349444][bookmark: _Toc508704831]Table 36: Type IV Holdover Times for Cryotech Polar Guard® Xtend
	Outside Air 
Temperature1
	Fluid 
Concentration 
Fluid/Water 
By % Volume
	Freezing Fog, Freezing Mist2, or Ice Crystals3
	Snow 
mixed with 
Freezing Fog4
	Very Light Snow, Snow Grains or Snow Pellets4,5
	Light 
Snow, Snow Grains or Snow Pellets4,5
	Moderate Snow, Snow Grains or Snow Pellets4,5
	Freezing 
Drizzle6
	Light 
Freezing Rain
	Moderate
Snow mixed with Rain7,8
	Rain on 
Cold‑Soaked Wing8
	Other9

	-3 °C and above
(27 °F and above)
	100/0
	2:30 - 4:00
	0:50 - 1:30
	3:00 - 3:00
	2:00 - 3:00
	1:05 - 2:00
	2:00 - 2:00
	1:00 - 1:50
	0:15 - 0:15
	0:20 - 1:45
	 

	
	75/25
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	 

	
	50/50
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	CAUTION: 
No holdover time 
guidelines exist

	below -3 to -8 °C
(below 27 to 18 °F)
	100/0
	1:00 - 1:50
	0:40 - 1:10
	2:50 - 3:00
	1:35 - 2:50
	0:50 - 1:35
	0:35 - 1:40
	0:50 - 0:55
	

	
	75/25
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	

	below -8 to -14 °C
(below 18 to 7 °F)
	100/0
	1:00 - 1:50
	0:35 - 1:00
	2:25 - 2:55
	1:20 - 2:25
	0:45 - 1:20
	0:35 - 1:4010
	0:50 - 0:5510
	

	
	75/25
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	

	below -14 to -18 °C
(below 7 to 0 °F)
	100/0
	0:25 - 0:40
	0:15 - 0:30
	1:20 - 1:40
	0:40 - 1:20
	0:20 - 0:40
	
	

	below -18 to -25 °C
(below 0 to -13 °F)
	100/0
	0:25 - 0:40
	0:05 - 0:10
	0:30 - 0:40
	0:15 - 0:30
	0:06 - 0:15
	
	

	below -25 to -29 °C
(below -13 to -20 °F)
	100/0
	0:25 - 0:40
	0:03 - 0:06
	0:20 - 0:25
	0:09 - 0:20
	0:04 - 0:09
	
	


NOTES
1. Ensure that the lowest operational use temperature (LOUT) is respected. Consider use of Type I fluid when Type IV fluid cannot be used.
1. Freezing mist is best confirmed by observation. It is never reported by METAR; however, it can occur when mist is present at 0 °C (32 °F) and below. 
1. Use freezing fog holdover times in conditions of ice crystals mixed with freezing fog or freezing mist.
1. To determine snowfall intensity, the Snowfall Intensities as a Function of Prevailing Visibility table (Table 57) is required. No holdover times exist if the reported visibility correlates to a “heavy” precipitation intensity. 
Use snow holdover times in conditions of very light, light, or moderate snow mixed with ice crystals.
Includes light, moderate and heavy freezing drizzle. Use light freezing rain holdover times if positive identification of freezing drizzle is not possible.
These holdover times apply to conditions of “moderate” precipitation intensity. In cases of very light or light snow mixed with light rain or drizzle, use light freezing rain holdover times. The Snowfall Intensities as a Function of Prevailing Visibility table (Table 57) is required to confirm the precipitation intensity. No holdover times exist if the reported visibility correlates to a “heavy” precipitation intensity.
No holdover time guidelines exist for this condition for 0 °C (32 °F) and below.
Heavy snow, ice pellets, moderate and heavy freezing rain, small hail and hail (Table 56 provides allowance times for Type IV PG fluids in ice pellets and small hail).
No holdover time guidelines exist for this condition below -10 °C (14 °F).
CAUTIONS
The cautions that apply to the holdover times in the table above can be found on page 32.


[bookmark: _Toc43986180][bookmark: _Toc234306077]Table 37: Type IV Holdover Times for Dow Inc. UCAR Endurance™ EG106 ADF/AAF
	Outside Air 
Temperature1
	Fluid 
Concentration 
Fluid/Water 
By % Volume
	Freezing Fog, Freezing Mist2, or Ice Crystals3
	Snow 
mixed with 
Freezing Fog4
	Very Light Snow, Snow Grains or Snow Pellets4,5
	Light 
Snow, Snow Grains or Snow Pellets4,5
	Moderate Snow, Snow Grains or Snow Pellets4,5
	Freezing 
Drizzle6
	Light 
Freezing Rain
	Moderate
Snow mixed with Rain7,8
	Rain on 
Cold‑Soaked Wing8
	Other9

	-3 °C and above
(27 °F and above)
	100/0
	2:05 - 3:10
	0:30 - 1:00
	2:45 - 3:00
	1:20 - 2:45
	0:40 - 1:20
	1:10 - 2:00
	0:50 - 1:15
	0:15 - 0:15
	0:20 - 2:00
	 

	
	75/25
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	 

	
	50/50
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	CAUTION: 
No holdover time 
guidelines exist

	below -3 to -8 °C
(below 27 to 18 °F)
	100/0
	1:50 - 3:20
	0:25 - 0:50
	2:25 - 3:00
	1:10 - 2:25
	0:35 - 1:10
	0:55 - 1:50
	0:45 - 1:10
	

	
	75/25
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	

	below -8 to -14 °C
(below 18 to 7 °F)
	100/0
	1:50 - 3:20
	0:25 - 0:45
	2:10 - 2:45
	1:05 - 2:10
	0:30 - 1:05
	0:55 - 1:5010
	0:45 - 1:1010
	

	
	75/25
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	

	below -14 to -18 °C
(below 7 to 0 °F)
	100/0
	0:30 - 1:05
	0:15 - 0:35
	1:45 - 2:15
	0:50 - 1:45
	0:25 - 0:50
	
	

	below -18 to -25 °C
(below 0 to -13 °F)
	100/0
	0:30 - 1:05
	0:15 - 0:30
	1:30 - 1:55
	0:40 - 1:30
	0:20 - 0:40
	
	

	below -25 to -29 °C
(below -13 to -20 °F)
	100/0
	0:30 - 1:05
	0:15 - 0:30
	1:20 - 1:45
	0:40 - 1:20
	0:20 - 0:40
	
	


NOTES
1. Ensure that the lowest operational use temperature (LOUT) is respected. Consider use of Type I fluid when Type IV fluid cannot be used.
1. Freezing mist is best confirmed by observation. It is never reported by METAR; however, it can occur when mist is present at 0 °C (32 °F) and below. 
1. Use freezing fog holdover times in conditions of ice crystals mixed with freezing fog or freezing mist.
1. To determine snowfall intensity, the Snowfall Intensities as a Function of Prevailing Visibility table (Table 57) is required. No holdover times exist if the reported visibility correlates to a “heavy” precipitation intensity. 
Use snow holdover times in conditions of very light, light, or moderate snow mixed with ice crystals.
Includes light, moderate and heavy freezing drizzle. Use light freezing rain holdover times if positive identification of freezing drizzle is not possible.
These holdover times apply to conditions of “moderate” precipitation intensity. In cases of very light or light snow mixed with light rain or drizzle, use light freezing rain holdover times. The Snowfall Intensities as a Function of Prevailing Visibility table (Table 57) is required to confirm the precipitation intensity. No holdover times exist if the reported visibility correlates to a “heavy” precipitation intensity.
No holdover time guidelines exist for this condition for 0 °C (32 °F) and below.
Heavy snow, ice pellets, moderate and heavy freezing rain, small hail and hail (Table 55 provides allowance times for Type IV EG fluids in ice pellets and small hail).
No holdover time guidelines exist for this condition below -10 °C (14 °F).
CAUTIONS
The cautions that apply to the holdover times in the table above can be found on page 32.
[bookmark: _Table_4J._Type][bookmark: _TABLE_4K._TYPE][bookmark: _Toc436349446]

[bookmark: _Toc508704832][bookmark: _Toc43986181][bookmark: _Toc234306078]Table 38: Type IV Holdover Times for Dow Inc. UCAR™ FLIGHTGUARD™ AD-49
	Outside Air 
Temperature1
	Fluid 
Concentration 
Fluid/Water 
By % Volume
	Freezing Fog, Freezing Mist2, or Ice Crystals3
	Snow 
mixed with 
Freezing Fog4
	Very Light Snow, Snow Grains or Snow Pellets4,5
	Light 
Snow, Snow Grains or Snow Pellets4,5
	Moderate Snow, Snow Grains or Snow Pellets4,5
	Freezing 
Drizzle6
	Light 
Freezing Rain
	Moderate
Snow mixed with Rain7,8
	Rain on 
Cold‑Soaked Wing8
	Other9

	-3 °C and above
(27 °F and above)
	100/0
	3:20 - 4:00
	0:45 - 1:25
	3:00 - 3:00
	1:55 - 3:00
	1:00 - 1:55
	1:25 - 2:00
	1:00 - 1:25
	0:08 - 0:08
	0:10 - 1:55
	 

	
	75/25
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	 

	
	50/50
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	CAUTION: 
No holdover time 
guidelines exist

	below -3 to -8 °C
(below 27 to 18 °F)
	100/0
	0:20 - 1:35
	0:35 - 1:05
	2:55 - 3:00
	1:30 - 2:55
	0:45 - 1:30
	0:25 - 1:25
	0:20 - 0:25
	

	
	75/25
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	

	below -8 to -14 °C
(below 18 to 7 °F)
	100/0
	0:20 - 1:35
	0:30 - 0:55
	2:25 - 3:00
	1:15 - 2:25
	0:40 - 1:15
	0:25 - 1:2510
	0:20 - 0:2510
	

	
	75/25
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	

	below -14 to -18 °C
(below 7 to 0 °F)
	100/0
	0:25 - 0:40
	0:01 - 0:06
	0:30 - 0:45
	0:09 - 0:30
	0:02 - 0:09
	
	

	below -18 to -25 °C
(below 0 to -13 °F)
	100/0
	0:25 - 0:40
	0:00 - 0:02
	0:10 - 0:20
	0:03 - 0:10
	0:01 - 0:03
	
	

	below -25 to -26 °C
(below -13 to -15 °F)
	100/0
	0:25 - 0:40
	0:00 - 0:01
	0:07 - 0:10
	0:02 - 0:07
	0:00 - 0:02
	
	


NOTES
1. Ensure that the lowest operational use temperature (LOUT) is respected. Consider use of Type I fluid when Type IV fluid cannot be used.
1. Freezing mist is best confirmed by observation. It is never reported by METAR; however, it can occur when mist is present at 0 °C (32 °F) and below. 
1. Use freezing fog holdover times in conditions of ice crystals mixed with freezing fog or freezing mist.
1. To determine snowfall intensity, the Snowfall Intensities as a Function of Prevailing Visibility table (Table 57) is required. No holdover times exist if the reported visibility correlates to a “heavy” precipitation intensity. 
Use snow holdover times in conditions of very light, light, or moderate snow mixed with ice crystals.
Includes light, moderate and heavy freezing drizzle. Use light freezing rain holdover times if positive identification of freezing drizzle is not possible.
These holdover times apply to conditions of “moderate” precipitation intensity. In cases of very light or light snow mixed with light rain or drizzle, use light freezing rain holdover times. The Snowfall Intensities as a Function of Prevailing Visibility table (Table 57) is required to confirm the precipitation intensity. No holdover times exist if the reported visibility correlates to a “heavy” precipitation intensity.
No holdover time guidelines exist for this condition for 0 °C (32 °F) and below.
Heavy snow, ice pellets, moderate and heavy freezing rain, small hail and hail (Table 56 provides allowance times for Type IV PG fluids in ice pellets and small hail).
No holdover time guidelines exist for this condition below -10 °C (14 °F).
CAUTIONS
The cautions that apply to the holdover times in the table above can be found on page 32.
[bookmark: _TABLE_4L._TYPE][bookmark: _Toc436349447]

[bookmark: _Toc234306079]Table 39: Type IV Holdover Times for ESSPO CHEMICALS D.O.O Nordwing PG4
	Outside Air 
Temperature1
	Fluid 
Concentration 
Fluid/Water 
By % Volume
	Freezing Fog, Freezing Mist2, or Ice Crystals3
	Snow 
mixed with 
Freezing Fog4
	Very Light Snow, Snow Grains or Snow Pellets4,5
	Light 
Snow, Snow Grains or Snow Pellets4,5
	Moderate Snow, Snow Grains or Snow Pellets4,5
	Freezing 
Drizzle6
	Light 
Freezing Rain
	Moderate
Snow mixed with Rain7,8
	Rain on 
Cold‑Soaked Wing8
	Other9

	-3 °C and above
(27 °F and above)
	100/0
	1:35 - 3:10
	0:30 - 0:55
	2:35 - 3:00
	1:15 - 2:35
	0:35 - 1:15
	1:05 - 1:45
	0:50 - 1:00
	0:15 - 0:15
	0:20 - 1:45
	 

	
	75/25
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	 

	
	50/50
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	CAUTION: 
No holdover time 
guidelines exist

	below -3 to -8 °C
(below 27 to 18 °F)
	100/0
	0:55 - 2:25
	0:25 - 0:50
	2:10 - 2:40
	1:05 - 2:10
	0:30 - 1:05
	0:55 - 1:30
	0:35 - 0:50
	

	
	75/25
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	

	below -8 to -14 °C
(below 18 to 7 °F)
	100/0
	0:55 - 2:25
	0:20 - 0:45
	1:55 - 2:25
	0:55 - 1:55
	0:30 - 0:55
	0:55 - 1:3010
	0:35 - 0:5010
	

	
	75/25
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	

	below -14 to -18 °C
(below 7 to 0 °F)
	100/0
	0:30 - 0:45
	0:10 - 0:25
	1:20 - 1:45
	0:35 - 1:20
	0:15 - 0:35
	
	

	below -18 to -25 °C
(below 0 to -13 °F)
	100/0
	0:30 - 0:45
	0:06 - 0:15
	0:50 - 1:10
	0:20 - 0:50
	0:09 - 0:20
	
	

	below -25 to -30 °C
(below -13 to -22 °F)
	100/0
	0:20 - 0:35
	0:04 - 0:09
	0:30 - 0:40
	0:15 - 0:30
	0:05 - 0:15
	
	


NOTES
1. Ensure that the lowest operational use temperature (LOUT) is respected. Consider use of Type I fluid when Type IV fluid cannot be used.
1. Freezing mist is best confirmed by observation. It is never reported by METAR; however, it can occur when mist is present at 0 °C (32 °F) and below. 
1. Use freezing fog holdover times in conditions of ice crystals mixed with freezing fog or freezing mist.
1. To determine snowfall intensity, the Snowfall Intensities as a Function of Prevailing Visibility table (Table 57) is required. No holdover times exist if the reported visibility correlates to a “heavy” precipitation intensity. 
Use snow holdover times in conditions of very light, light, or moderate snow mixed with ice crystals.
Includes light, moderate and heavy freezing drizzle. Use light freezing rain holdover times if positive identification of freezing drizzle is not possible.
These holdover times apply to conditions of “moderate” precipitation intensity. In cases of very light or light snow mixed with light rain or drizzle, use light freezing rain holdover times. The Snowfall Intensities as a Function of Prevailing Visibility table (Table 57) is required to confirm the precipitation intensity. No holdover times exist if the reported visibility correlates to a “heavy” precipitation intensity.
No holdover time guidelines exist for this condition for 0 °C (32 °F) and below.
Heavy snow, ice pellets, moderate and heavy freezing rain, small hail and hail.
No holdover time guidelines exist for this condition below -10 °C (14 °F).
CAUTIONS
The cautions that apply to the holdover times in the table above can be found on page 32.


[bookmark: _Toc508704833][bookmark: _Toc43986182][bookmark: _Toc234306080]Table 40: Type IV Holdover Times for Inland Technologies ECO-SHIELD®
	Outside Air 
Temperature1
	Fluid 
Concentration 
Fluid/Water 
By % Volume
	Freezing Fog, Freezing Mist2, or Ice Crystals3
	Snow 
mixed with 
Freezing Fog4
	Very Light Snow, Snow Grains or Snow Pellets4,5
	Light 
Snow, Snow Grains or Snow Pellets4,5
	Moderate Snow, Snow Grains or Snow Pellets4,5
	Freezing 
Drizzle6
	Light 
Freezing Rain
	Moderate
Snow mixed with Rain7,8
	Rain on 
Cold‑Soaked Wing8
	Other9

	-3 °C and above
(27 °F and above)
	100/0
	1:15 - 2:40
	0:35 - 1:00
	2:25 - 2:50
	1:20 - 2:25
	0:45 - 1:20
	0:40 - 1:30
	0:35 - 0:40
	0:09 - 0:09
	0:15 - 1:35
	 

	
	75/25
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	 

	
	50/50
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	CAUTION: 
No holdover time 
guidelines exist

	below -3 to -8 °C
(below 27 to 18 °F)
	100/0
	1:10 - 2:35
	0:30 - 0:55
	2:05 - 2:30
	1:10 - 2:05
	0:40 - 1:10
	0:50 - 1:25
	0:30 - 0:40
	

	
	75/25
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	

	below -8 to -14 °C
(below 18 to 7 °F)
	100/0
	1:10 - 2:35
	0:25 - 0:50
	1:55 - 2:15
	1:05 - 1:55
	0:35 - 1:05
	0:50 - 1:2510
	0:30 - 0:4010
	

	
	75/25
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	

	below -14 to -18 °C
(below 7 to 0 °F)
	100/0
	0:30 - 1:00
	0:01 - 0:06
	0:30 - 0:45
	0:09 - 0:30
	0:02 - 0:09
	
	

	below -18 to -25 °C
(below 0 to -13 °F)
	100/0
	0:30 - 1:00
	0:00 - 0:02
	0:10 - 0:20
	0:03 - 0:10
	0:01 - 0:03
	
	

	below -25 to -25.5 °C
(below -13 to -14 °F)
	100/0
	0:30 - 1:00
	0:00 - 0:01
	0:07 - 0:10
	0:02 - 0:07
	0:00 - 0:02
	
	


NOTES
1. Ensure that the lowest operational use temperature (LOUT) is respected. Consider use of Type I fluid when Type IV fluid cannot be used.
1. Freezing mist is best confirmed by observation. It is never reported by METAR; however, it can occur when mist is present at 0 °C (32 °F) and below. 
1. Use freezing fog holdover times in conditions of ice crystals mixed with freezing fog or freezing mist.
1. To determine snowfall intensity, the Snowfall Intensities as a Function of Prevailing Visibility table (Table 57) is required. No holdover times exist if the reported visibility correlates to a “heavy” precipitation intensity. 
Use snow holdover times in conditions of very light, light, or moderate snow mixed with ice crystals.
Includes light, moderate and heavy freezing drizzle. Use light freezing rain holdover times if positive identification of freezing drizzle is not possible.
These holdover times apply to conditions of “moderate” precipitation intensity. In cases of very light or light snow mixed with light rain or drizzle, use light freezing rain holdover times. The Snowfall Intensities as a Function of Prevailing Visibility table (Table 57) is required to confirm the precipitation intensity. No holdover times exist if the reported visibility correlates to a “heavy” precipitation intensity.
No holdover time guidelines exist for this condition for 0 °C (32 °F) and below.
Heavy snow, ice pellets, moderate and heavy freezing rain, small hail and hail.
No holdover time guidelines exist for this condition below -10 °C (14 °F).
CAUTIONS
The cautions that apply to the holdover times in the table above can be found on page 32.
[bookmark: _TABLE_4I._TYPE]

[bookmark: _Toc43986183][bookmark: _Toc234306081][bookmark: _Toc508704834]Table 41: Type IV Holdover Times for JSC RCP Nordix Defrost ECO 4
	Outside Air 
Temperature1
	Fluid 
Concentration 
Fluid/Water 
By % Volume
	Freezing Fog, Freezing Mist2, or Ice Crystals3
	Snow 
mixed with 
Freezing Fog4
	Very Light Snow, Snow Grains or Snow Pellets4,5
	Light 
Snow, Snow Grains or Snow Pellets4,5
	Moderate Snow, Snow Grains or Snow Pellets4,5
	Freezing 
Drizzle6
	Light 
Freezing Rain
	Moderate
Snow mixed with Rain7,8
	Rain on 
Cold‑Soaked Wing8
	Other9

	-3 °C and above
(27 °F and above)
	100/0
	1:30 - 2:40
	0:30 - 0:55
	2:30 - 3:00
	1:15 - 2:30
	0:35 - 1:15
	1:05 - 1:30
	0:40 - 1:05
	0:10 - 0:10
	0:15 - 1:10
	 

	
	75/25
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	 

	
	50/50
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	CAUTION: 
No holdover time 
guidelines exist

	below -3 to -8 °C
(below 27 to 18 °F)
	100/0
	0:55 - 2:35
	0:25 - 0:50
	2:15 - 2:45
	1:05 - 2:15
	0:35 - 1:05
	0:50 - 1:20
	0:35 - 0:50
	

	
	75/25
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	

	below -8 to -14 °C
(below 18 to 7 °F)
	100/0
	0:55 - 2:35
	0:25 - 0:45
	2:05 - 2:35
	1:00 - 2:05
	0:30 - 1:00
	0:50 - 1:2010
	0:35 - 0:5010
	

	
	75/25
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	

	below -14 to -18 °C
(below 7 to 0 °F)
	100/0
	0:30 - 0:50
	0:01 - 0:06
	0:30 - 0:45
	0:09 - 0:30
	0:02 - 0:09
	
	

	below -18 to -25 °C
(below 0 to -13 °F)
	100/0
	0:30 - 0:50
	0:00 - 0:02
	0:10 - 0:20
	0:03 - 0:10
	0:01 - 0:03
	
	

	below -25 to -25.5 °C
(below -13 to -14 °F)
	100/0
	0:30 - 0:50
	0:00 - 0:01
	0:07 - 0:10
	0:02 - 0:07
	0:00 - 0:02
	
	


NOTES
1. Ensure that the lowest operational use temperature (LOUT) is respected. Consider use of Type I fluid when Type IV fluid cannot be used.
1. Freezing mist is best confirmed by observation. It is never reported by METAR; however, it can occur when mist is present at 0 °C (32 °F) and below. 
1. Use freezing fog holdover times in conditions of ice crystals mixed with freezing fog or freezing mist.
1. To determine snowfall intensity, the Snowfall Intensities as a Function of Prevailing Visibility table (Table 57) is required. No holdover times exist if the reported visibility correlates to a “heavy” precipitation intensity. 
Use snow holdover times in conditions of very light, light, or moderate snow mixed with ice crystals.
Includes light, moderate and heavy freezing drizzle. Use light freezing rain holdover times if positive identification of freezing drizzle is not possible.
These holdover times apply to conditions of “moderate” precipitation intensity. In cases of very light or light snow mixed with light rain or drizzle, use light freezing rain holdover times. The Snowfall Intensities as a Function of Prevailing Visibility table (Table 57) is required to confirm the precipitation intensity. No holdover times exist if the reported visibility correlates to a “heavy” precipitation intensity.
No holdover time guidelines exist for this condition for 0 °C (32 °F) and below.
Heavy snow, ice pellets, moderate and heavy freezing rain, small hail and hail (Table 56 provides allowance times for Type IV PG fluids in ice pellets and small hail).
No holdover time guidelines exist for this condition below -10 °C (14 °F).
CAUTIONS
The cautions that apply to the holdover times in the table above can be found on page 32.


[bookmark: _Toc234306082][bookmark: _Toc43986185]Table 42: Type IV Holdover Times for JSC RCP Nordix Defrost NORTH 4
	Outside Air 
Temperature1
	Fluid 
Concentration 
Fluid/Water 
By % Volume
	Freezing Fog, Freezing Mist2, or Ice Crystals3
	Snow 
mixed with 
Freezing Fog4
	Very Light Snow, Snow Grains or Snow Pellets4,5
	Light 
Snow, Snow Grains or Snow Pellets4,5
	Moderate Snow, Snow Grains or Snow Pellets4,5
	Freezing 
Drizzle6
	Light 
Freezing Rain
	Moderate
Snow mixed with Rain7,8
	Rain on 
Cold‑Soaked Wing8
	Other9

	-3 °C and above
(27 °F and above)
	100/0
	2:10 - 4:00
	0:25 - 0:50
	2:25 - 3:00
	1:10 - 2:25
	0:30 - 1:10
	1:05 - 2:00
	0:30 - 0:50
	0:06 - 0:06
	0:09 - 1:55
	 

	
	75/25
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	 

	
	50/50
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	CAUTION: 
No holdover time 
guidelines exist

	below -3 to -8 °C
(below 27 to 18 °F)
	100/0
	2:40 - 4:00
	0:25 - 0:50
	2:25 - 3:00
	1:10 - 2:25
	0:30 - 1:10
	1:05 - 2:00
	0:40 - 1:00
	

	
	75/25
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	

	below -8 to -14 °C
(below 18 to 7 °F)
	100/0
	2:40 - 4:00
	0:25 - 0:50
	2:25 - 3:00
	1:10 - 2:25
	0:30 - 1:10
	1:05 - 2:0010
	0:40 - 1:0010
	

	
	75/25
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	

	below -14 to -18 °C
(below 7 to 0 °F)
	100/0
	0:45 - 1:55
	0:07 - 0:20
	0:50 - 1:05
	0:25 - 0:50
	0:10 - 0:25
	
	

	below -18 to -25 °C
(below 0 to -13 °F)
	100/0
	0:45 - 1:55
	0:03 - 0:10
	0:40 - 0:55
	0:15 - 0:40
	0:05 - 0:15
	
	

	below -25 to -26 °C
(below -13 to -15 °F)
	100/0
	0:45 - 1:55
	0:01 - 0:06
	0:25 - 0:35
	0:08 - 0:25
	0:02 - 0:08
	
	


NOTES
1. Ensure that the lowest operational use temperature (LOUT) is respected. Consider use of Type I fluid when Type IV fluid cannot be used.
1. Freezing mist is best confirmed by observation. It is never reported by METAR; however, it can occur when mist is present at 0 °C (32 °F) and below. 
1. Use freezing fog holdover times in conditions of ice crystals mixed with freezing fog or freezing mist.
1. To determine snowfall intensity, the Snowfall Intensities as a Function of Prevailing Visibility table (Table 57) is required. No holdover times exist if the reported visibility correlates to a “heavy” precipitation intensity. 
Use snow holdover times in conditions of very light, light, or moderate snow mixed with ice crystals.
Includes light, moderate and heavy freezing drizzle. Use light freezing rain holdover times if positive identification of freezing drizzle is not possible.
These holdover times apply to conditions of “moderate” precipitation intensity. In cases of very light or light snow mixed with light rain or drizzle, use light freezing rain holdover times. The Snowfall Intensities as a Function of Prevailing Visibility table (Table 57) is required to confirm the precipitation intensity. No holdover times exist if the reported visibility correlates to a “heavy” precipitation intensity.
No holdover time guidelines exist for this condition for 0 °C (32 °F) and below.
Heavy snow, ice pellets, moderate and heavy freezing rain, small hail and hail (Table 55 provides allowance times for Type IV EG fluids in ice pellets and small hail).
No holdover time guidelines exist for this condition below -10 °C (14 °F).
CAUTIONS
The cautions that apply to the holdover times in the table above can be found on page 32.


[bookmark: _Toc234306083]Table 43: Type IV Holdover Times for Kilfrost ABC-S Plus
	Outside Air 
Temperature1
	Fluid 
Concentration 
Fluid/Water 
By % Volume
	Freezing Fog, Freezing Mist2, or Ice Crystals3
	Snow 
mixed with 
Freezing Fog4
	Very Light Snow, Snow Grains or Snow Pellets4,5
	Light 
Snow, Snow Grains or Snow Pellets4,5
	Moderate Snow, Snow Grains or Snow Pellets4,5
	Freezing 
Drizzle6
	Light 
Freezing Rain
	Moderate
Snow mixed with Rain7,8
	Rain on 
Cold‑Soaked Wing8
	Other9

	-3 °C and above
(27 °F and above)
	100/0
	2:10 - 4:00
	0:55 - 1:35
	3:00 - 3:00
	2:05 - 3:00
	1:15 - 2:05
	1:50 - 2:00
	1:05 - 2:00
	0:15 - 0:15
	0:25 - 2:00
	 

	
	75/25
	1:25 - 2:40
	0:30 - 0:55
	2:05 - 2:25
	1:15 - 2:05
	0:45 - 1:15
	1:00 - 1:20
	0:30 - 0:50
	0:08 - 0:08
	0:10 - 1:20
	 

	
	50/50
	0:30 - 0:55
	0:15 - 0:25
	1:00 - 1:10
	0:30 - 1:00
	0:15 - 0:30
	0:15 - 0:40
	0:15 - 0:20
	CAUTION: 
No holdover time 
guidelines exist

	below -3 to -8 °C
(below 27 to 18 °F)
	100/0
	0:55 - 3:30
	0:50 - 1:25
	3:00 - 3:00
	1:50 - 3:00
	1:05 - 1:50
	0:25 - 1:35
	0:20 - 0:30
	

	
	75/25
	0:45 - 1:50
	0:30 - 0:50
	1:50 - 2:10
	1:05 - 1:50
	0:40 - 1:05
	0:20 - 1:10
	0:15 - 0:25
	

	below -8 to -14 °C
(below 18 to 7 °F)
	100/0
	0:55 - 3:30
	0:45 - 1:15
	2:55 - 3:00
	1:45 - 2:55
	1:00 - 1:45
	0:25 - 1:3510
	0:20 - 0:3010
	

	
	75/25
	0:45 - 1:50
	0:25 - 0:45
	1:45 - 2:00
	1:00 - 1:45
	0:35 - 1:00
	0:20 - 1:1010
	0:15 - 0:2510
	

	below -14 to -18 °C
(below 7 to 0 °F)
	100/0
	0:40 - 1:00
	0:01 - 0:06
	0:30 - 0:45
	0:09 - 0:30
	0:02 - 0:09
	
	

	below -18 to -25 °C
(below 0 to -13 °F)
	100/0
	0:40 - 1:00
	0:00 - 0:02
	0:10 - 0:20
	0:03 - 0:10
	0:01 - 0:03
	
	

	below -25 to -28 °C
(below -13 to -18 °F)
	100/0
	0:40 - 1:00
	0:00 - 0:01
	0:07 - 0:10
	0:02 - 0:07
	0:00 - 0:02
	
	


NOTES
1. Ensure that the lowest operational use temperature (LOUT) is respected. Consider use of Type I fluid when Type IV fluid cannot be used.
1. Freezing mist is best confirmed by observation. It is never reported by METAR; however, it can occur when mist is present at 0 °C (32 °F) and below. 
1. Use freezing fog holdover times in conditions of ice crystals mixed with freezing fog or freezing mist.
1. To determine snowfall intensity, the Snowfall Intensities as a Function of Prevailing Visibility table (Table 57) is required. No holdover times exist if the reported visibility correlates to a “heavy” precipitation intensity. 
Use snow holdover times in conditions of very light, light, or moderate snow mixed with ice crystals.
Includes light, moderate and heavy freezing drizzle. Use light freezing rain holdover times if positive identification of freezing drizzle is not possible.
These holdover times apply to conditions of “moderate” precipitation intensity. In cases of very light or light snow mixed with light rain or drizzle, use light freezing rain holdover times. The Snowfall Intensities as a Function of Prevailing Visibility table (Table 57) is required to confirm the precipitation intensity. No holdover times exist if the reported visibility correlates to a “heavy” precipitation intensity.
No holdover time guidelines exist for this condition for 0 °C (32 °F) and below.
Heavy snow, ice pellets, moderate and heavy freezing rain, small hail and hail (Table 56 provides allowance times for Type IV PG fluids in ice pellets and small hail).
No holdover time guidelines exist for this condition below -10 °C (14 °F).
CAUTIONS
The cautions that apply to the holdover times in the table above can be found on page 32.


[bookmark: _Toc234306084]Table 44: Type IV Holdover Times for LNT Solutions P450
	Outside Air 
Temperature1
	Fluid 
Concentration 
Fluid/Water 
By % Volume
	Freezing Fog, Freezing Mist2, or Ice Crystals3
	Snow 
mixed with 
Freezing Fog4
	Very Light Snow, Snow Grains or Snow Pellets4,5
	Light 
Snow, Snow Grains or Snow Pellets4,5
	Moderate Snow, Snow Grains or Snow Pellets4,5
	Freezing 
Drizzle6
	Light 
Freezing Rain
	Moderate
Snow mixed with Rain7,8
	Rain on 
Cold‑Soaked Wing8
	Other9

	-3 °C and above
(27 °F and above)
	100/0
	3:10 - 4:00
	0:40 - 1:35
	3:00 - 3:00
	2:05 - 3:00
	0:55 - 2:05
	2:00 - 2:00
	1:05 - 1:40
	0:20 - 0:20
	0:30 - 1:55
	 

	
	75/25
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	 

	
	50/50
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	CAUTION: 
No holdover time 
guidelines exist

	below -3 to -8 °C
(below 27 to 18 °F)
	100/0
	1:10 - 2:55
	0:35 - 1:15
	3:00 - 3:00
	1:35 - 3:00
	0:45 - 1:35
	0:35 - 1:50
	0:25 - 0:50
	

	
	75/25
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	

	below -8 to -14 °C
(below 18 to 7 °F)
	100/0
	1:10 - 2:55
	0:30 - 1:00
	3:00 - 3:00
	1:20 - 3:00
	0:35 - 1:20
	0:35 - 1:5010
	0:25 - 0:5010
	

	
	75/25
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	

	below -14 to -18 °C
(below 7 to 0 °F)
	100/0
	0:15 - 0:25
	0:01 - 0:06
	0:30 - 0:45
	0:09 - 0:30
	0:02 - 0:09
	
	

	below -18 to -25 °C
(below 0 to -13 °F)
	100/0
	0:15 - 0:25
	0:00 - 0:02
	0:10 - 0:20
	0:03 - 0:10
	0:01 - 0:03
	
	

	below -25 to -29 °C
(below -13 to -20 °F)
	100/0
	0:15 - 0:25
	0:00 - 0:01
	0:07 - 0:10
	0:02 - 0:07
	0:00 - 0:02
	
	


NOTES
1. Ensure that the lowest operational use temperature (LOUT) is respected. Consider use of Type I fluid when Type IV fluid cannot be used.
1. Freezing mist is best confirmed by observation. It is never reported by METAR; however, it can occur when mist is present at 0 °C (32 °F) and below. 
1. Use freezing fog holdover times in conditions of ice crystals mixed with freezing fog or freezing mist.
1. To determine snowfall intensity, the Snowfall Intensities as a Function of Prevailing Visibility table (Table 57) is required. No holdover times exist if the reported visibility correlates to a “heavy” precipitation intensity. 
Use snow holdover times in conditions of very light, light, or moderate snow mixed with ice crystals.
Includes light, moderate and heavy freezing drizzle. Use light freezing rain holdover times if positive identification of freezing drizzle is not possible.
These holdover times apply to conditions of “moderate” precipitation intensity. In cases of very light or light snow mixed with light rain or drizzle, use light freezing rain holdover times. The Snowfall Intensities as a Function of Prevailing Visibility table (Table 57) is required to confirm the precipitation intensity. No holdover times exist if the reported visibility correlates to a “heavy” precipitation intensity.
No holdover time guidelines exist for this condition for 0 °C (32 °F) and below.
Heavy snow, ice pellets, moderate and heavy freezing rain, small hail and hail.
No holdover time guidelines exist for this condition below -10 °C (14 °F).
CAUTIONS
The cautions that apply to the holdover times in the table above can be found on page 32.


[bookmark: _Toc234306085]Table 45: Type IV Holdover Times for MAX TECH LLC MTL 4-EG
	Outside Air 
Temperature1
	Fluid 
Concentration 
Fluid/Water 
By % Volume
	Freezing Fog, Freezing Mist2, or Ice Crystals3
	Snow 
mixed with 
Freezing Fog4
	Very Light Snow, Snow Grains or Snow Pellets4,5
	Light 
Snow, Snow Grains or Snow Pellets4,5
	Moderate Snow, Snow Grains or Snow Pellets4,5
	Freezing 
Drizzle6
	Light 
Freezing Rain
	Moderate
Snow mixed with Rain7,8
	Rain on 
Cold‑Soaked Wing8
	Other9

	-3 °C and above
(27 °F and above)
	100/0
	2:40 - 4:00
	0:55 - 2:05
	3:00 - 3:00
	2:50 - 3:00
	1:10 - 2:50
	1:15 - 2:00
	0:45 - 1:15
	0:10 - 0:10
	0:15 - 1:50
	 

	
	75/25
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	 

	
	50/50
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	CAUTION: 
No holdover time 
guidelines exist

	below -3 to -8 °C
(below 27 to 18 °F)
	100/0
	2:35 - 3:55
	0:35 - 1:25
	3:00 - 3:00
	1:55 - 3:00
	0:50 - 1:55
	1:00 - 2:00
	0:50 - 1:15
	

	
	75/25
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	

	below -8 to -14 °C
(below 18 to 7 °F)
	100/0
	1:25 - 4:00
	0:30 - 1:10
	3:00 - 3:00
	1:30 - 3:00
	0:40 - 1:30
	0:50 - 2:0010
	0:45 - 1:2010
	

	
	75/25
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	

	below -14 to -18 °C
(below 7 to 0 °F)
	100/0
	0:50 - 4:00
	0:20 - 0:45
	2:15 - 2:50
	1:00 - 2:15
	0:30 - 1:00
	
	

	below -18 to -25 °C
(below 0 to -13 °F)
	100/0
	0:25 - 1:00
	0:15 - 0:30
	1:30 - 2:00
	0:40 - 1:30
	0:20 - 0:40
	
	

	below -25 to -26.5 °C
(below -13 to -16 °F)
	100/0
	0:25 - 1:00
	0:15 - 0:30
	1:25 - 1:50
	0:40 - 1:25
	0:20 - 0:40
	
	


NOTES
1. Ensure that the lowest operational use temperature (LOUT) is respected. Consider use of Type I fluid when Type IV fluid cannot be used.
1. Freezing mist is best confirmed by observation. It is never reported by METAR; however, it can occur when mist is present at 0 °C (32 °F) and below. 
1. Use freezing fog holdover times in conditions of ice crystals mixed with freezing fog or freezing mist.
1. To determine snowfall intensity, the Snowfall Intensities as a Function of Prevailing Visibility table (Table 57) is required. No holdover times exist if the reported visibility correlates to a “heavy” precipitation intensity. 
Use snow holdover times in conditions of very light, light, or moderate snow mixed with ice crystals.
Includes light, moderate and heavy freezing drizzle. Use light freezing rain holdover times if positive identification of freezing drizzle is not possible.
These holdover times apply to conditions of “moderate” precipitation intensity. In cases of very light or light snow mixed with light rain or drizzle, use light freezing rain holdover times. The Snowfall Intensities as a Function of Prevailing Visibility table (Table 57) is required to confirm the precipitation intensity. No holdover times exist if the reported visibility correlates to a “heavy” precipitation intensity.
No holdover time guidelines exist for this condition for 0 °C (32 °F) and below.
Heavy snow, ice pellets, moderate and heavy freezing rain, small hail and hail.
No holdover time guidelines exist for this condition below -10 °C (14 °F).
CAUTIONS
The cautions that apply to the holdover times in the table above can be found on page 32.



[bookmark: _Toc234306086]Table 46: Type IV Holdover Times for MAX TECH LLC MTL 4-PG
	Outside Air 
Temperature1
	Fluid 
Concentration 
Fluid/Water 
By % Volume
	Freezing Fog, Freezing Mist2, or Ice Crystals3
	Snow 
mixed with 
Freezing Fog4
	Very Light Snow, Snow Grains or Snow Pellets4,5
	Light 
Snow, Snow Grains or Snow Pellets4,5
	Moderate Snow, Snow Grains or Snow Pellets4,5
	Freezing 
Drizzle6
	Light 
Freezing Rain
	Moderate
Snow mixed with Rain7,8
	Rain on 
Cold‑Soaked Wing8
	Other9

	-3 °C and above
(27 °F and above)
	100/0
	2:25 - 4:00
	0:35 - 1:15
	3:00 - 3:00
	1:40 - 3:00
	0:45 - 1:40
	1:15 - 2:00
	0:55 - 1:10
	0:15 - 0:15
	0:20 - 1:30
	 

	
	75/25
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	 

	
	50/50
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	CAUTION: 
No holdover time 
guidelines exist

	below -3 to -8 °C
(below 27 to 18 °F)
	100/0
	1:35 - 3:55
	0:20 - 0:50
	2:35 - 3:00
	1:10 - 2:35
	0:30 - 1:10
	0:30 - 1:50
	0:20 - 0:35
	

	
	75/25
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	

	below -8 to -14 °C
(below 18 to 7 °F)
	100/0
	0:40 - 2:10
	0:15 - 0:40
	2:00 - 2:35
	0:50 - 2:00
	0:25 - 0:50
	0:25 - 1:3010
	0:15 - 0:3010
	

	
	75/25
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	

	below -14 to -18 °C
(below 7 to 0 °F)
	100/0
	0:30 - 1:30
	0:10 - 0:25
	1:00 - 1:15
	0:30 - 1:00
	0:15 - 0:30
	
	

	below -18 to -25 °C
(below 0 to -13 °F)
	100/0
	0:25 - 0:40
	0:07 - 0:15
	0:40 - 0:45
	0:20 - 0:40
	0:10 - 0:20
	
	

	below -25 to -27 °C
(below -13 to -17 °F)
	100/0
	0:25 - 0:40
	0:06 - 0:15
	0:35 - 0:40
	0:15 - 0:35
	0:08 - 0:15
	
	


NOTES
1. Ensure that the lowest operational use temperature (LOUT) is respected. Consider use of Type I fluid when Type IV fluid cannot be used.
1. Freezing mist is best confirmed by observation. It is never reported by METAR; however, it can occur when mist is present at 0 °C (32 °F) and below. 
1. Use freezing fog holdover times in conditions of ice crystals mixed with freezing fog or freezing mist.
1. To determine snowfall intensity, the Snowfall Intensities as a Function of Prevailing Visibility table (Table 57) is required. No holdover times exist if the reported visibility correlates to a “heavy” precipitation intensity. 
Use snow holdover times in conditions of very light, light, or moderate snow mixed with ice crystals.
Includes light, moderate and heavy freezing drizzle. Use light freezing rain holdover times if positive identification of freezing drizzle is not possible.
These holdover times apply to conditions of “moderate” precipitation intensity. In cases of very light or light snow mixed with light rain or drizzle, use light freezing rain holdover times. The Snowfall Intensities as a Function of Prevailing Visibility table (Table 57) is required to confirm the precipitation intensity. No holdover times exist if the reported visibility correlates to a “heavy” precipitation intensity.
No holdover time guidelines exist for this condition for 0 °C (32 °F) and below.
Heavy snow, ice pellets, moderate and heavy freezing rain, small hail and hail.
No holdover time guidelines exist for this condition below -10 °C (14 °F).
CAUTIONS
The cautions that apply to the holdover times in the table above can be found on page 32.


[bookmark: _TABLE_4M._TYPE][bookmark: _TABLE_4N._TYPE][bookmark: _Toc234306087][bookmark: _Toc436349449][bookmark: _Toc508704836][bookmark: _Toc43986187]Table 47: Type IV Holdover Times for MKS DevO Chemicals COREICEPHOB TYPE-IV PG
	Outside Air 
Temperature1
	Fluid 
Concentration 
Fluid/Water 
By % Volume
	Freezing Fog, Freezing Mist2, or Ice Crystals3
	Snow 
mixed with 
Freezing Fog4
	Very Light Snow, Snow Grains or Snow Pellets4,5
	Light 
Snow, Snow Grains or Snow Pellets4,5
	Moderate Snow, Snow Grains or Snow Pellets4,5
	Freezing 
Drizzle6
	Light 
Freezing Rain
	Moderate
Snow mixed with Rain7,8
	Rain on 
Cold‑Soaked Wing8
	Other9

	-3 °C and above
(27 °F and above)
	100/0
	2:20 - 3:50
	0:35 - 1:15
	3:00 - 3:00
	1:40 - 3:00
	0:45 - 1:40
	1:25 - 2:00
	0:50 - 1:20
	0:09 - 0:09
	0:10 - 1:40
	 

	
	75/25
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	 

	
	50/50
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	CAUTION: 
No holdover time 
guidelines exist

	below -3 to -8 °C
(below 27 to 18 °F)
	100/0
	0:15 - 0:35
	0:25 - 0:55
	2:35 - 3:00
	1:10 - 2:35
	0:35 - 1:10
	0:40 - 1:30
	0:20 - 0:35
	

	
	75/25
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	

	below -8 to -14 °C
(below 18 to 7 °F)
	100/0
	0:15 - 0:35
	0:20 - 0:45
	2:05 - 2:40
	0:55 - 2:05
	0:25 - 0:55
	0:40 - 1:3010
	0:20 - 0:3510
	

	
	75/25
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	

	below -14 to -18 °C
(below 7 to 0 °F)
	100/0
	0:15 - 0:30
	0:01 - 0:06
	0:30 - 0:45
	0:09 - 0:30
	0:02 - 0:09
	
	

	below -18 to -25 °C
(below 0 to -13 °F)
	100/0
	0:15 - 0:30
	0:00 - 0:02
	0:10 - 0:20
	0:03 - 0:10
	0:01 - 0:03
	
	

	below -25 to -29 °C
(below -13 to -20 °F)
	100/0
	0:15 - 0:30
	0:00 - 0:01
	0:07 - 0:10
	0:02 - 0:07
	0:00 - 0:02
	
	


NOTES
1. Ensure that the lowest operational use temperature (LOUT) is respected. Consider use of Type I fluid when Type IV fluid cannot be used.
1. Freezing mist is best confirmed by observation. It is never reported by METAR; however, it can occur when mist is present at 0 °C (32 °F) and below. 
1. Use freezing fog holdover times in conditions of ice crystals mixed with freezing fog or freezing mist.
1. To determine snowfall intensity, the Snowfall Intensities as a Function of Prevailing Visibility table (Table 57) is required. No holdover times exist if the reported visibility correlates to a “heavy” precipitation intensity. 
Use snow holdover times in conditions of very light, light, or moderate snow mixed with ice crystals.
Includes light, moderate and heavy freezing drizzle. Use light freezing rain holdover times if positive identification of freezing drizzle is not possible.
These holdover times apply to conditions of “moderate” precipitation intensity. In cases of very light or light snow mixed with light rain or drizzle, use light freezing rain holdover times. The Snowfall Intensities as a Function of Prevailing Visibility table (Table 57) is required to confirm the precipitation intensity. No holdover times exist if the reported visibility correlates to a “heavy” precipitation intensity.
No holdover time guidelines exist for this condition for 0 °C (32 °F) and below.
Heavy snow, ice pellets, moderate and heavy freezing rain, small hail and hail. 
No holdover time guidelines exist for this condition below -10 °C (14 °F).
CAUTIONS
The cautions that apply to the holdover times in the table above can be found on page 32.


[bookmark: _Toc234306088]Table 48: Type IV Holdover Times for Newave Aerochemical FCY 9311
	Outside Air 
Temperature1
	Fluid 
Concentration 
Fluid/Water 
By % Volume
	Freezing Fog, Freezing Mist2, or Ice Crystals3
	Snow 
mixed with 
Freezing Fog4
	Very Light Snow, Snow Grains or Snow Pellets4,5
	Light 
Snow, Snow Grains or Snow Pellets4,5
	Moderate Snow, Snow Grains or Snow Pellets4,5
	Freezing 
Drizzle6
	Light 
Freezing Rain
	Moderate
Snow mixed with Rain7,8
	Rain on 
Cold‑Soaked Wing8
	Other9

	-3 °C and above
(27 °F and above)
	100/0
	1:55 - 4:00
	0:25 - 0:55
	2:20 - 2:55
	1:10 - 2:20
	0:35 - 1:10
	1:10 - 2:00
	0:40 - 1:05
	0:09 - 0:09
	0:15 - 1:25
	 

	
	75/25
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	 

	
	50/50
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	CAUTION: 
No holdover time 
guidelines exist

	below -3 to -8 °C
(below 27 to 18 °F)
	100/0
	0:35 - 2:05
	0:20 - 0:40
	1:50 - 2:20
	0:55 - 1:50
	0:30 - 0:55
	0:35 - 1:20
	0:20 - 0:35
	

	
	75/25
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	

	below -8 to -14 °C
(below 18 to 7 °F)
	100/0
	0:35 - 2:05
	0:20 - 0:35
	1:35 - 2:00
	0:50 - 1:35
	0:25 - 0:50
	0:35 - 1:2010
	0:20 - 0:3510
	

	
	75/25
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	

	below -14 to -18 °C
(below 7 to 0 °F)
	100/0
	0:30 - 0:55
	0:10 - 0:20
	1:00 - 1:15
	0:30 - 1:00
	0:15 - 0:30
	
	

	below -18 to -25 °C
(below 0 to -13 °F)
	100/0
	0:30 - 0:55
	0:05 - 0:10
	0:35 - 0:40
	0:15 - 0:35
	0:07 - 0:15
	
	

	below -25 to -29.5 °C
(below -13 to -21 °F)
	100/0
	0:30 - 0:55
	0:05 - 0:10
	0:30 - 0:40
	0:15 - 0:30
	0:06 - 0:15
	
	


NOTES
1. Ensure that the lowest operational use temperature (LOUT) is respected. Consider use of Type I fluid when Type IV fluid cannot be used.
1. Freezing mist is best confirmed by observation. It is never reported by METAR; however, it can occur when mist is present at 0 °C (32 °F) and below. 
1. Use freezing fog holdover times in conditions of ice crystals mixed with freezing fog or freezing mist.
1. To determine snowfall intensity, the Snowfall Intensities as a Function of Prevailing Visibility table (Table 57) is required. No holdover times exist if the reported visibility correlates to a “heavy” precipitation intensity. 
Use snow holdover times in conditions of very light, light, or moderate snow mixed with ice crystals.
Includes light, moderate and heavy freezing drizzle. Use light freezing rain holdover times if positive identification of freezing drizzle is not possible.
These holdover times apply to conditions of “moderate” precipitation intensity. In cases of very light or light snow mixed with light rain or drizzle, use light freezing rain holdover times. The Snowfall Intensities as a Function of Prevailing Visibility table (Table 57) is required to confirm the precipitation intensity. No holdover times exist if the reported visibility correlates to a “heavy” precipitation intensity.
No holdover time guidelines exist for this condition for 0 °C (32 °F) and below.
Heavy snow, ice pellets, moderate and heavy freezing rain, small hail and hail (Table 56 provides allowance times for Type IV PG fluids in ice pellets and small hail).
No holdover time guidelines exist for this condition below -10 °C (14 °F).
CAUTIONS
The cautions that apply to the holdover times in the table above can be found on page 32.


[bookmark: _TABLE_5._SNOWFALL][bookmark: _TABLE_4O._TYPE][bookmark: _Toc234306089][bookmark: _Toc508704838][bookmark: _Toc43986188][bookmark: _Toc436349450]Table 49: Type IV Holdover Times for Newave Aerochemical FCY-EGIV
	Outside Air 
Temperature1
	Fluid 
Concentration 
Fluid/Water 
By % Volume
	Freezing Fog, Freezing Mist2, or Ice Crystals3
	Snow 
mixed with 
Freezing Fog4
	Very Light Snow, Snow Grains or Snow Pellets4,5
	Light 
Snow, Snow Grains or Snow Pellets4,5
	Moderate Snow, Snow Grains or Snow Pellets4,5
	Freezing 
Drizzle6
	Light 
Freezing Rain
	Moderate
Snow mixed with Rain7,8
	Rain on 
Cold‑Soaked Wing8
	Other9

	-3 °C and above
(27 °F and above)
	100/0
	2:35 - 4:00
	0:25 - 0:55
	2:35 - 3:00
	1:10 - 2:35
	0:35 - 1:10
	1:20 - 2:00
	0:40 - 1:05
	0:10 - 0:10
	0:15 - 2:00
	 

	
	75/25
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	 

	
	50/50
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	CAUTION: 
No holdover time 
guidelines exist

	below -3 to -8 °C
(below 27 to 18 °F)
	100/0
	1:25 - 3:25
	0:20 - 0:45
	2:10 - 2:45
	1:00 - 2:10
	0:25 - 1:00
	0:50 - 2:00
	0:45 - 1:05
	

	
	75/25
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	

	below -8 to -14 °C
(below 18 to 7 °F)
	100/0
	1:25 - 3:25
	0:20 - 0:40
	1:55 - 2:25
	0:50 - 1:55
	0:25 - 0:50
	0:50 - 2:0010
	0:45 - 1:0510
	

	
	75/25
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	

	below -14 to -18 °C
(below 7 to 0 °F)
	100/0
	0:35 - 1:55
	0:15 - 0:30
	1:35 - 2:05
	0:40 - 1:35
	0:15 - 0:40
	
	

	below -18 to -25 °C
(below 0 to -13 °F)
	100/0
	0:35 - 1:55
	0:09 - 0:20
	1:10 - 1:35
	0:30 - 1:10
	0:15 - 0:30
	
	

	below -25 to -29 °C
(below -13 to -20 °F)
	100/0
	0:35 - 1:55
	0:08 - 0:20
	1:00 - 1:20
	0:25 - 1:00
	0:10 - 0:25
	
	


NOTES
1. Ensure that the lowest operational use temperature (LOUT) is respected. Consider use of Type I fluid when Type IV fluid cannot be used.
1. Freezing mist is best confirmed by observation. It is never reported by METAR; however, it can occur when mist is present at 0 °C (32 °F) and below. 
1. Use freezing fog holdover times in conditions of ice crystals mixed with freezing fog or freezing mist.
1. To determine snowfall intensity, the Snowfall Intensities as a Function of Prevailing Visibility table (Table 57) is required. No holdover times exist if the reported visibility correlates to a “heavy” precipitation intensity. 
Use snow holdover times in conditions of very light, light, or moderate snow mixed with ice crystals.
Includes light, moderate and heavy freezing drizzle. Use light freezing rain holdover times if positive identification of freezing drizzle is not possible.
These holdover times apply to conditions of “moderate” precipitation intensity. In cases of very light or light snow mixed with light rain or drizzle, use light freezing rain holdover times. The Snowfall Intensities as a Function of Prevailing Visibility table (Table 57) is required to confirm the precipitation intensity. No holdover times exist if the reported visibility correlates to a “heavy” precipitation intensity.
No holdover time guidelines exist for this condition for 0 °C (32 °F) and below.
Heavy snow, ice pellets, moderate and heavy freezing rain, small hail and hail (Table 55 provides allowance times for Type IV EG fluids in ice pellets and small hail).
No holdover time guidelines exist for this condition below -10 °C (14 °F).
CAUTIONS
The cautions that apply to the holdover times in the table above can be found on page 32.


[bookmark: _Toc234306090]Table 50: Type IV Holdover Times for Newave Aerochemical FCY-EGIV PLUS
	Outside Air 
Temperature1
	Fluid 
Concentration 
Fluid/Water 
By % Volume
	Freezing Fog, Freezing Mist2, or Ice Crystals3
	Snow 
mixed with 
Freezing Fog4
	Very Light Snow, Snow Grains or Snow Pellets4,5
	Light 
Snow, Snow Grains or Snow Pellets4,5
	Moderate Snow, Snow Grains or Snow Pellets4,5
	Freezing 
Drizzle6
	Light 
Freezing Rain
	Moderate
Snow mixed with Rain7,8
	Rain on 
Cold‑Soaked Wing8
	Other9

	-3 °C and above
(27 °F and above)
	100/0
	3:05 - 4:00
	0:30 - 1:00
	2:50 - 3:00
	1:20 - 2:50
	0:40 - 1:20
	1:15 - 2:00
	0:40 - 0:55
	0:10 - 0:10
	0:15 - 2:00
	 

	
	75/25
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	 

	
	50/50
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	CAUTION: 
No holdover time 
guidelines exist

	below -3 to -8 °C
(below 27 to 18 °F)
	100/0
	1:35 - 3:15
	0:25 - 0:50
	2:15 - 2:55
	1:05 - 2:15
	0:30 - 1:05
	1:15 - 2:00
	0:30 - 0:45
	

	
	75/25
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	

	below -8 to -14 °C
(below 18 to 7 °F)
	100/0
	1:35 - 3:15
	0:20 - 0:40
	2:00 - 2:30
	0:55 - 2:00
	0:25 - 0:55
	1:15 - 2:0010
	0:30 - 0:4510
	

	
	75/25
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	

	below -14 to -18 °C
(below 7 to 0 °F)
	100/0
	0:30 - 1:10
	0:15 - 0:30
	1:30 - 1:55
	0:40 - 1:30
	0:20 - 0:40
	
	

	below -18 to -25 °C
(below 0 to -13 °F)
	100/0
	0:30 - 1:10
	0:09 - 0:20
	1:05 - 1:25
	0:30 - 1:05
	0:15 - 0:30
	
	

	below -25 to -29 °C
(below -13 to -20 °F)
	100/0
	0:30 - 1:10
	0:08 - 0:20
	1:00 - 1:15
	0:25 - 1:00
	0:10 - 0:25
	
	


NOTES
1. Ensure that the lowest operational use temperature (LOUT) is respected. Consider use of Type I fluid when Type IV fluid cannot be used.
1. Freezing mist is best confirmed by observation. It is never reported by METAR; however, it can occur when mist is present at 0 °C (32 °F) and below. 
1. Use freezing fog holdover times in conditions of ice crystals mixed with freezing fog or freezing mist.
1. To determine snowfall intensity, the Snowfall Intensities as a Function of Prevailing Visibility table (Table 57) is required. No holdover times exist if the reported visibility correlates to a “heavy” precipitation intensity. 
Use snow holdover times in conditions of very light, light, or moderate snow mixed with ice crystals.
Includes light, moderate and heavy freezing drizzle. Use light freezing rain holdover times if positive identification of freezing drizzle is not possible.
These holdover times apply to conditions of “moderate” precipitation intensity. In cases of very light or light snow mixed with light rain or drizzle, use light freezing rain holdover times. The Snowfall Intensities as a Function of Prevailing Visibility table (Table 57) is required to confirm the precipitation intensity. No holdover times exist if the reported visibility correlates to a “heavy” precipitation intensity.
No holdover time guidelines exist for this condition for 0 °C (32 °F) and below.
Heavy snow, ice pellets, moderate and heavy freezing rain, small hail and hail.
No holdover time guidelines exist for this condition below -10 °C (14 °F).
CAUTIONS
The cautions that apply to the holdover times in the table above can be found on page 32.


[bookmark: _Toc234306091]Table 51: Type IV Holdover Times for Shaanxi Cleanway Cleansurface IV
	Outside Air 
Temperature1
	Fluid 
Concentration 
Fluid/Water 
By % Volume
	Freezing Fog, Freezing Mist2, or Ice Crystals3
	Snow 
mixed with 
Freezing Fog4
	Very Light Snow, Snow Grains or Snow Pellets4,5
	Light 
Snow, Snow Grains or Snow Pellets4,5
	Moderate Snow, Snow Grains or Snow Pellets4,5
	Freezing 
Drizzle6
	Light 
Freezing Rain
	Moderate
Snow mixed with Rain7,8
	Rain on 
Cold‑Soaked Wing8
	Other9

	-3 °C and above
(27 °F and above)
	100/0
	2:30 - 4:00
	0:30 - 1:15
	3:00 - 3:00
	1:40 - 3:00
	0:40 - 1:40
	1:20 - 2:00
	0:40 - 1:10
	0:09 - 0:09
	0:15 - 1:50
	 

	
	75/25
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	 

	
	50/50
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	CAUTION: 
No holdover time 
guidelines exist

	below -3 to -8 °C
(below 27 to 18 °F)
	100/0
	0:55 - 2:05
	0:20 - 0:45
	2:25 - 3:00
	1:00 - 2:25
	0:25 - 1:00
	0:30 - 1:30
	0:25 - 0:35
	

	
	75/25
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	

	below -8 to -14 °C
(below 18 to 7 °F)
	100/0
	0:55 - 2:05
	0:15 - 0:35
	1:45 - 2:15
	0:45 - 1:45
	0:20 - 0:45
	0:30 - 1:3010
	0:25 - 0:3510
	

	
	75/25
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	

	below -14 to -18 °C
(below 7 to 0 °F)
	100/0
	0:25 - 0:35
	0:10 - 0:20
	1:05 - 1:20
	0:30 - 1:05
	0:15 - 0:30
	
	

	below -18 to -25 °C
(below 0 to -13 °F)
	100/0
	0:25 - 0:35
	0:05 - 0:10
	0:35 - 0:45
	0:15 - 0:35
	0:07 - 0:15
	
	

	below -25 to -30 °C
(below -13 to -22 °F)
	100/0
	0:20 - 0:30
	0:04 - 0:09
	0:30 - 0:35
	0:15 - 0:30
	0:06 - 0:15
	
	


NOTES
1. Ensure that the lowest operational use temperature (LOUT) is respected. Consider use of Type I fluid when Type IV fluid cannot be used.
1. Freezing mist is best confirmed by observation. It is never reported by METAR; however, it can occur when mist is present at 0 °C (32 °F) and below. 
1. Use freezing fog holdover times in conditions of ice crystals mixed with freezing fog or freezing mist.
1. To determine snowfall intensity, the Snowfall Intensities as a Function of Prevailing Visibility table (Table 57) is required. No holdover times exist if the reported visibility correlates to a “heavy” precipitation intensity. 
Use snow holdover times in conditions of very light, light, or moderate snow mixed with ice crystals.
Includes light, moderate and heavy freezing drizzle. Use light freezing rain holdover times if positive identification of freezing drizzle is not possible.
These holdover times apply to conditions of “moderate” precipitation intensity. In cases of very light or light snow mixed with light rain or drizzle, use light freezing rain holdover times. The Snowfall Intensities as a Function of Prevailing Visibility table (Table 57) is required to confirm the precipitation intensity. No holdover times exist if the reported visibility correlates to a “heavy” precipitation intensity.
No holdover time guidelines exist for this condition for 0 °C (32 °F) and below.
Heavy snow, ice pellets, moderate and heavy freezing rain, small hail and hail.
No holdover time guidelines exist for this condition below -10 °C (14 °F).
CAUTIONS
The cautions that apply to the holdover times in the table above can be found on page 32.


[bookmark: _Toc234306092]Table 52: Type IV Holdover Times for Xinjiang Zhongtian Liyang Aviation Clearice-IV
	Outside Air 
Temperature1
	Fluid 
Concentration 
Fluid/Water 
By % Volume
	Freezing Fog, Freezing Mist2, or Ice Crystals3
	Snow 
mixed with 
Freezing Fog4
	Very Light Snow, Snow Grains or Snow Pellets4,5
	Light 
Snow, Snow Grains or Snow Pellets4,5
	Moderate Snow, Snow Grains or Snow Pellets4,5
	Freezing 
Drizzle6
	Light 
Freezing Rain
	Moderate
Snow mixed with Rain7,8
	Rain on 
Cold‑Soaked Wing8
	Other9

	-3 °C and above
(27 °F and above)
	100/0
	2:25 - 4:00
	0:25 - 0:50
	2:15 - 2:50
	1:05 - 2:15
	0:30 - 1:05
	1:05 - 1:55
	0:35 - 0:55
	0:09 - 0:09
	0:15 - 1:30
	 

	
	75/25
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	 

	
	50/50
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	CAUTION: 
No holdover time 
guidelines exist

	below -3 to -8 °C
(below 27 to 18 °F)
	100/0
	1:20 - 2:10
	0:20 - 0:40
	1:50 - 2:20
	0:55 - 1:50
	0:25 - 0:55
	0:55 - 1:35
	0:35 - 0:50
	

	
	75/25
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	

	below -8 to -14 °C
(below 18 to 7 °F)
	100/0
	1:20 - 2:10
	0:15 - 0:35
	1:35 - 2:00
	0:45 - 1:35
	0:20 - 0:45
	0:55 - 1:3510
	0:35 - 0:5010
	

	
	75/25
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	

	below -14 to -18 °C
(below 7 to 0 °F)
	100/0
	0:30 - 1:00
	0:15 - 0:30
	1:15 - 1:35
	0:40 - 1:15
	0:20 - 0:40
	
	

	below -18 to -25 °C
(below 0 to -13 °F)
	100/0
	0:30 - 1:00
	0:15 - 0:25
	1:10 - 1:25
	0:35 - 1:10
	0:15 - 0:35
	
	

	below -25 to -29 °C
(below -13 to -20 °F)
	100/0
	0:30 - 1:00
	0:10 - 0:25
	1:05 - 1:20
	0:30 - 1:05
	0:15 - 0:30
	
	


NOTES
1. Ensure that the lowest operational use temperature (LOUT) is respected. Consider use of Type I fluid when Type IV fluid cannot be used.
1. Freezing mist is best confirmed by observation. It is never reported by METAR; however, it can occur when mist is present at 0 °C (32 °F) and below. 
1. Use freezing fog holdover times in conditions of ice crystals mixed with freezing fog or freezing mist.
1. To determine snowfall intensity, the Snowfall Intensities as a Function of Prevailing Visibility table (Table 57) is required. No holdover times exist if the reported visibility correlates to a “heavy” precipitation intensity. 
Use snow holdover times in conditions of very light, light, or moderate snow mixed with ice crystals.
Includes light, moderate and heavy freezing drizzle. Use light freezing rain holdover times if positive identification of freezing drizzle is not possible.
These holdover times apply to conditions of “moderate” precipitation intensity. In cases of very light or light snow mixed with light rain or drizzle, use light freezing rain holdover times. The Snowfall Intensities as a Function of Prevailing Visibility table (Table 57) is required to confirm the precipitation intensity. No holdover times exist if the reported visibility correlates to a “heavy” precipitation intensity.
No holdover time guidelines exist for this condition for 0 °C (32 °F) and below.
Heavy snow, ice pellets, moderate and heavy freezing rain, small hail and hail.
No holdover time guidelines exist for this condition below -10 °C (14 °F).
CAUTIONS
The cautions that apply to the holdover times in the table above can be found on page 32.
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[bookmark: _TABLE_6._ICE][bookmark: SnowZFogCautions][bookmark: _Toc485747174][bookmark: _Toc508704839][bookmark: _Toc43986189][bookmark: _Toc234306093][bookmark: _Toc436349451]Allowance Times Tables for Winter 2026-2027

The HOT Guidelines are provided for information and guidance purposes. The HOT Guidelines on their own do not change, create, amend or permit deviations from regulatory requirements.

The HOT Guidelines may use mandatory terms such as “must”, “shall” and “is/are required” so as to convey the intent of meeting regulatory requirements and SAE Standards, where applicable. The term “should” is to be understood, unless an alternative method of achieving safety is implemented that would meet or exceed the intent of the recommendation.



[bookmark: AllowanceTimesCautions][bookmark: _Ref198818909]CAUTIONS
The responsibility for the application of these data remains with the user.
Fluids used during ground de/anti-icing do not provide in-flight icing protection. 
This table is for departure planning only and should be used in conjunction with pre-takeoff check procedures.
Allowance time cannot be extended by an inspection of the aircraft critical surfaces. 
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[bookmark: _TABLE_7._ICE][bookmark: _Ref167965228][bookmark: _Toc168404652][bookmark: _Toc234306094][bookmark: _Ref137462890][bookmark: _Toc140477237][bookmark: _Toc140480375]Table 53: Validation Status of fluids for use with Allowance Times1
	Manufacturer
	Fluid Name
	Applicable 
Allowance Times (ATs)

	Type III Fluids

	AllClear Systems LLC
	AeroClear MAX
	ATs for Type III Fluids

	Type IV EG Fluids

	AFLRUS LLC
	Green Flo Type 4
	Fluid has not been validated2

	ALAB International
	PROFLIGHT EG4 
	Fluid has not been validated2

	AllClear Systems LLC
	ClearWing EG
	ATs for Type IV EG Fluids

	ASGlobal
	4Flite EG
	Fluid has not been validated2

	AVIAFLUID International Ltd
	AVIAFlight EG
	ATs for Type IV EG Fluids

	CHEMCO Inc.
	ChemR EG IV
	ATs for Type IV EG Fluids

	CHEMCO Inc.
	ChemR Nordik IV
	ATs for Type IV EG Fluids

	Chongqing Joba Chemical Co,.Ltd
	FW-IV
	ATs for Type IV EG Fluids

	Dow Inc.
	UCAR ENDURANCE™ EG106 ADF/AAF
	ATs for Type IV EG Fluids

	JSC RCP Nordix
	Defrost NORTH 4
	ATs for Type IV EG Fluids

	MAX TECH LLC
	MTL 4-EG
	Fluid has not been validated2

	Newave Aerochemical Co. Ltd.
	FCY-EGIV
	ATs for Type IV EG Fluids

	Newave Aerochemical Co. Ltd.
	FCY-EGIV PLUS
	Fluid has not been validated2

	Xinjiang Zhongtian Liyang Aviation
	Clearice-IV
	Fluid has not been validated2

	Type IV PG Fluids

	ABAX Industries
	ECOWING AD-49
	ATs for Type IV PG Fluids

	ALAB International
	PROFLIGHT PG4 
	Fluid has not been validated2

	AllClear Systems LLC
	Clear IV Flight
	Fluid has not been validated2

	ASGlobal
	4Flite PG
	ATs for Type IV PG Fluids

	AVIAFLUID International Ltd
	AVIAFlight PG
	ATs for Type IV PG Fluids

	Clariant Produkte (Deutschland) GmbH
	Safewing MP IV LAUNCH
	ATs for Type IV PG Fluids

	Clariant Produkte (Deutschland) GmbH
	Safewing MP IV LAUNCH PLUS
	ATs for Type IV PG Fluids

	Cryotech Deicing Technology
	Polar Guard® Advance
	ATs for Type IV PG Fluids

	Cryotech Deicing Technology
	Polar Guard® Xtend
	ATs for Type IV PG Fluids

	Dow Inc.
	UCAR™ FLIGHTGUARD™ AD-49
	ATs for Type IV PG Fluids

	ESSPO CHEMICALS D.O.O
	Nordwing PG4
	Fluid has not been validated2

	Inland Technologies Inc.
	ECO-SHIELD®
	Fluid has not been validated2

	JSC RCP Nordix
	Defrost ECO 4
	ATs for Type IV PG Fluids

	Kilfrost Limited
	ABC-S Plus
	ATs for Type IV PG Fluids

	LNT Solutions
	P450
	Fluid has not been validated2

	MAX TECH LLC
	MTL 4-PG
	Fluid has not been validated2

	MKS DevO Chemicals
	COREICEPHOB TYPE-IV PG
	Fluid has not been validated2

	Newave Aerochemical Co. Ltd.
	FCY 9311
	ATs for Type IV PG Fluids

	Shaanxi Cleanway Aviation Chemical Co., Ltd
	Cleansurface IV
	Fluid has not been validated2


NOTES
1 Allowance times are for use with undiluted (100/0) Type III, Type IV EG, and Type IV PG fluids only. No allowance times exist for Type II fluids.
2 No allowance times exist for this fluid at the time of publication as the allowance times have not yet been validated.
[bookmark: _Ref172009805][bookmark: _Toc234306095]
Table 54: Allowance Times for SAE Type III Fluids1,2
	Precipitation Types or Combinations
and Applicable METAR Codes4
	Outside Air Temperature3

	
	Above 0 °C
(Above 32 °F)
	0 to -5 °C
(32 to 23 °F)
	Below -5
 to -10 °C
(Below 23 to 14 °F)
	Below -10 °C
(Below 14 °F)

	Light Ice Pellets (or Small Hail5,6)
-PL
	10 minutes 
	10 minutes 
	10 minutes 
	Caution: 
No allowance times currently exist

	Light Ice Pellets (or Small Hail5,6) Mixed with Light Snow 
-PLSN, -SNPL
	10 minutes 
	10 minutes 
	10 minutes
	

	Light Ice Pellets (or Small Hail5,6) Mixed with Light Freezing Drizzle 
-PLFZDZ, -FZDZPL
	
	7 minutes 
	5 minutes 
	

	Light Ice Pellets (or Small Hail5,6) Mixed with Light Drizzle
-PLDZ, -DZPL
	7 minutes
	
	

	Light Ice Pellets (or Small Hail5,6) Mixed with Light Freezing Rain 
-PLFZRA, -FZRAPL
	
	7 minutes
	5 minutes 
	

	Light Ice Pellets (or Small Hail5,6) Mixed with Light Rain 
-PLRA, -RAPL
	7 minutes
	
	

	Moderate Ice Pellets (or Small Hail5,6) 
PL
	5 minutes 
	5 minutes 
	5 minutes 
	


NOTES
1. These allowance times are for use with undiluted (100/0) fluids applied unheated on aircraft with rotation speeds of 100 knots or greater. To use the allowance times in this table, ensure the fluid being used is listed in the Validation Status of Fluids for Use with Allowance Times (Table 53).
Takeoff is allowed up to 90 minutes after start of fluid application if the precipitation stops at or before the allowance time expires and does not restart. Takeoff is not permitted if the OAT decreases during the 90 minutes in conditions of light ice pellets mixed with either: light freezing drizzle; light drizzle; light freezing rain; or light rain.
Ensure that the lowest operational use temperature (LOUT) is respected. 
Applicable METAR codes include only Ice Pellet conditions (i.e., PL). While allowance times can be used when Small Hail is reported instead of Ice Pellets, the corresponding METAR codes for Small Hail are not listed in the table.
The reporting of Small Hail by METAR varies by country, which can result in different HOTs or allowance times when the same METAR code is used in different regions. For details, refer to the METAR Codes and Holdover or Allowance Times Used by Country table in the FAA Ground Deicing Program General Information Document.
If the METAR does not report an intensity for small hail, use the “moderate ice pellets or small hail” allowance times. If the METAR reports an intensity with small hail, the condition with the equivalent intensity can be used, e.g., if light small hail is reported, the “light ice pellets” allowance times can be used. This also applies in mixed conditions, e.g., if light small hail mixed with light snow is reported, use the “light ice pellets mixed with light snow” allowance times.
CAUTIONS
The cautions that apply to the allowance times in the table above can be found on page 66.


[bookmark: _Ref137464359][bookmark: _Toc140477238][bookmark: _Toc140480376][bookmark: _Toc234306096]Table 55: Allowance Times for SAE Type IV
Ethylene Glycol (EG) Fluids1,2
	Precipitation Types or Combinations 
and Applicable METAR Codes5
	Outside Air Temperature3

	
	Above 0 °C4
(Above 32 °F)
	0 to -5 °C4
(32 to 23 °F)
	Below -5 
to -10 °C4
(Below 23 to 14 °F)
	Below -10 
to -16 °C4
(Below 14 to 3 °F)
	Below -16 
to -22 °C4
(Below 3 to -8 °F)

	Light Ice Pellets (or Small Hail6,7)
-PL
	70 minutes
	70 minutes
	70 minutes
	50 minutes
	30 minutes

	Light Ice Pellets (or Small Hail6,7) Mixed with Light Snow 
-PLSN, -SNPL
	50 minutes
	50 minutes
	30 minutes
	25 minutes
	

	Light Ice Pellets (or Small Hail6,7) Mixed with Light Freezing Drizzle 
-PLFZDZ, -FZDZPL
	
	40 minutes
	30 minutes
	Caution: 
No allowance times 
currently exist

	Light Ice Pellets (or Small Hail6,7) Mixed with Light Drizzle
-PLDZ, -DZPL
	40 minutes
	
	

	Light Ice Pellets (or Small Hail6,7) Mixed with Light Freezing Rain 
-PLFZRA, -FZRAPL
	
	40 minutes
	30 minutes
	

	Light Ice Pellets (or Small Hail6,7) Mixed with Light Rain 
-PLRA, -RAPL
	40 minutes
	
	

	Light Ice Pellets (or Small Hail6,7) Mixed with Light Freezing Rain and Light Snow
-PLFZRASN, -PLSNFZRA, -FZRAPLSN, 
-FZRASNPL, -SNPLFZRA, -SNFZRAPL 
	
	20 minutes
	
	

	Light Ice Pellets (or Small Hail6,7) Mixed with Light Rain and Light Snow
-PLRASN, -PLSNRA, -RAPLSN, -RASNPL, 
-SNPLRA, -SNRAPL
	20 minutes
	
	

	Moderate Ice Pellets (or Small Hail6,7) 
PL
	35 minutes
	35 minutes
	35 minutes
	15 minutes
	10 minutes

	Moderate Ice Pellets (or Small Hail6,7)
Mixed with Moderate Snow
PLSN, SNPL
	25 minutes
	25 minutes
	15 minutes
	10 minutes
	

	Moderate Ice Pellets (or Small Hail6,7) Mixed with Light or Moderate Freezing Drizzle 
PLFZDZ, FZDZPL
	
	20 minutes
	10 minutes
	
	

	Moderate Ice Pellets (or Small Hail6,7) Mixed with Light or Moderate Drizzle
PLDZ, DZPL
	20 minutes
	Caution: 
No allowance times 
currently exist 

	Moderate Ice Pellets (or Small Hail6,7) Mixed with Moderate Rain 
PLRA, RAPL
	15 minutes
	


NOTES
The notes that apply to the allowance times in the table above can be found on page 70.
CAUTIONS
The cautions that apply to the allowance times in the table above can be found on page 66.


Table 55 (CONT’D): ALLOWANCE TIMES FOR SAE TYPE IV
ETHYLENE GLYCOL (EG) FLUIDS
NOTES
1. These allowance times are for use with undiluted (100/0) EG-based fluids. To use the allowance times in this table, ensure the fluid being used is listed in the Validation Status of Fluids for Use with Allowance Times (Table 53).
[bookmark: _Hlk170966960]Takeoff is allowed up to 90 minutes after start of fluid application if the precipitation stops at or before the allowance time expires and does not restart. Takeoff is not permitted if the OAT decreases during the 90 minutes in conditions of light ice pellets mixed with either: light freezing drizzle; light drizzle; light freezing rain; light rain; light rain and light snow; or light freezing rain and light snow, as well as in conditions of moderate ice pellets mixed with either: light or moderate freezing drizzle; light or moderate drizzle; or moderate rain.
171 Ensure that the lowest operational use temperature (LOUT) is respected. 
172 No allowance times exist for EG-based fluids when used on aircraft with rotation speeds less than 100 knots. 
Applicable METAR codes include only Ice Pellet conditions (i.e., PL). While allowance times can be used when Small Hail is reported instead of Ice Pellets, the corresponding METAR codes for Small Hail are not listed in the table.
The reporting of Small Hail by METAR varies by country, which can result in different HOTs or allowance times when the same METAR code is used in different regions. For details, refer to the METAR Codes and Holdover or Allowance Times Used by Country table in the FAA Ground Deicing Program General Information Document.
If the METAR does not report an intensity for small hail, use the “moderate ice pellets or small hail” allowance times. If the METAR reports an intensity with small hail, the condition with the equivalent intensity can be used, e.g., if light small hail is reported, the “light ice pellets” allowance times can be used. This also applies in mixed conditions, e.g., if light small hail mixed with light snow is reported, use the “light ice pellets mixed with light snow” allowance times.



[bookmark: _Ref137464407][bookmark: _Toc140477239][bookmark: _Toc140480377][bookmark: _Toc234306097]Table 56: Allowance Times for SAE Type IV
Propylene Glycol (PG) Fluids1,2
	Precipitation Types or Combinations
and Applicable METAR Codes6
	Outside Air Temperature3

	
	Above 0 °C4
(Above 32 °F)
	0 to -5 °C4
(32 to 23 °F)
	Below -5 
to -10 °C4
(Below 23 to 14 °F)
	Below -10 
to -16 °C5
(Below 14 to 3 °F)
	Below -16 
to -22 °C5
(Below 3 to -8 °F)

	Light Ice Pellets (or Small Hail7,8)
-PL
	50 minutes
	50 minutes
	30 minutes
	30 minutes
	20 minutes

	Light Ice Pellets (or Small Hail7,8) Mixed with Light Snow
-PLSN, -SNPL
	40 minutes
	40 minutes
	15 minutes
	15 minutes
	

	Light Ice Pellets (or Small Hail7,8) Mixed with Light Freezing Drizzle 
-PLFZDZ, -FZDZPL
	
	25 minutes
	10 minutes
	Caution: 
No allowance times 
currently exist

	Light Ice Pellets (or Small Hail7,8) Mixed with Light Drizzle
-PLDZ, -DZPL
	25 minutes
	
	

	Light Ice Pellets (or Small Hail7,8) Mixed with Light Freezing Rain
-PLFZRA, -FZRAPL
	
	25 minutes
	10 minutes
	

	Light Ice Pellets (or Small Hail7,8) Mixed with Light Rain
-PLRA, -RAPL
	25 minutes
	
	

	Light Ice Pellets (or Small Hail7,8) Mixed with Light Freezing Rain and Light Snow
-PLFZRASN, -PLSNFZRA, -FZRAPLSN, 
-FZRASNPL, -SNPLFZRA, -SNFZRAPL
	
	20 minutes
	
	

	Light Ice Pellets (or Small Hail7,8) Mixed with Light Rain and Light Snow
-PLRASN, -PLSNRA, -RAPLSN, -RASNPL, 
-SNPLRA, -SNRAPL
	20 minutes
	
	

	Moderate Ice Pellets (or Small Hail7,8)
PL
	15 minutes
	15 minutes
	10 minutes
	10 minutes
	

	Moderate Ice Pellets (or Small Hail7,8)
Mixed with Moderate Snow
PLSN, SNPL
	15 minutes
	15 minutes
	5 minutes
	5 minutes
	

	Moderate Ice Pellets (or Small Hail7,8) Mixed with Light or Moderate Freezing Drizzle
PLFZDZ, FZDZPL
	
	10 minutes
	7 minutes
	
	

	Moderate Ice Pellets (or Small Hail7,8) Mixed with Light or Moderate Drizzle
PLDZ, DZPL
	10 minutes
	Caution: 
No allowance times 
currently exist 

	Moderate Ice Pellets (or Small Hail7,8) Mixed with Moderate Rain
PLRA, RAPL
	10 minutes
	


NOTES
The notes that apply to the allowance times in the table above can be found on page 72.
CAUTIONS
The cautions that apply to the allowance times in the table above can be found on page 66.


Table 56 (CONT’D): ALLOWANCE TIMES FOR SAE TYPE IV
PROPYLENE GLYCOL (PG) FLUIDS
NOTES
1. These allowance times are for use with undiluted (100/0) PG-based fluids applied on aircraft with rotation speeds of 100 knots or greater. To use the allowance times in this table, ensure the fluid being used is listed in the Validation Status of Fluids for Use with Allowance Times (Table 53).
Takeoff is allowed up to 90 minutes after start of fluid application if the precipitation stops at or before the allowance time expires and does not restart. Takeoff is not permitted if the OAT decreases during the 90 minutes in conditions of light ice pellets mixed with either: light freezing drizzle; light drizzle; light freezing rain; light rain; light rain and light snow; or light freezing rain and light snow, as well as in conditions of moderate ice pellets mixed with either: light or moderate freezing drizzle; light or moderate drizzle; or moderate rain.
Ensure that the lowest operational use temperature (LOUT) is respected.
No allowance times exist for PG-based fluids when used on aircraft with rotation speeds less than 100 knots. 
No allowance times exist for PG-based fluids when used on aircraft with rotation speeds less than 115 knots. 
Applicable METAR codes include only Ice Pellet conditions (i.e., PL). While allowance times can be used when Small Hail is reported instead of Ice Pellets, the corresponding METAR codes for Small Hail are not listed in the table.
The reporting of Small Hail by METAR varies by country, which can result in different HOTs or allowance times when the same METAR code is used in different regions. For details, refer to the METAR Codes and Holdover or Allowance Times Used by Country table in the FAA Ground Deicing Program General Information Document.
If the METAR does not report an intensity for small hail, use the “moderate ice pellets or small hail” allowance times. If the METAR reports an intensity with small hail, the condition with the equivalent intensity can be used, e.g., if light small hail is reported, the “light ice pellets” allowance times can be used. This also applies in mixed conditions, e.g., if light small hail mixed with light snow is reported, use the “light ice pellets mixed with light snow” allowance times.
FAA Holdover Time Guidelines	Winter 2026-2027

[bookmark: _TABLE_8-1._LIST][bookmark: _TABLE_7._SNOWFALL][bookmark: _Toc485747177][bookmark: _Toc508704842][bookmark: _Toc43986192][bookmark: _Toc234306098][bookmark: _Toc436349453]Supplemental Guidance for Winter 2026-2027

The HOT Guidelines are provided for information and guidance purposes. The HOT Guidelines on their own do not change, create, amend or permit deviations from regulatory requirements.

The HOT Guidelines may use mandatory terms such as “must”, “shall” and “is/are required” so as to convey the intent of meeting regulatory requirements and SAE Standards, where applicable. The term “should” is to be understood, unless an alternative method of achieving safety is implemented that would meet or exceed the intent of the recommendation.



[bookmark: _Ref107225632][bookmark: _Toc234306099][bookmark: _Ref485908996][bookmark: _Toc508704843][bookmark: _Toc43986193]Table 57: Snowfall Intensities as a Function of Prevailing Visibility
		Visibility
	Day
	Night

	Statute Miles
	Meters
	-1 °C and below
30 °F and below
	Above -1 °C
Above 30 °F
	-1 °C and Below
30 °F and below
	Above -1 °C
Above 30 °F

	≤1/4
	(≤3/8)
	≤400
	(≤600)
	Heavy
	Heavy
	Heavy
	Heavy

	1/2
	(>3/8 to ≤5/8)
	800
	(>600 to ≤1000)
	Moderate
	Heavy
	Heavy
	Heavy

	3/4
	(>5/8 to ≤7/8)
	1200
	(>1000 to ≤1400)
	Moderate
	Moderate
	Moderate
	Heavy

	1
	(>7/8 to ≤1 1/8 ) 
	1600
	(>1400 to ≤1800)
	Light
	Light
	Moderate
	Moderate

	1 ¼
	(>1 1/8 to ≤1 3/8) 
	2000
	(>1800 to ≤2200)
	Light
	Light
	Moderate
	Moderate

	1 ½
	(>1 3/8 to ≤1 5/8) 
	2400
	(>2200 to ≤2600)
	Light
	Light
	Moderate
	Moderate

	1 ¾
	(>1 5/8 to ≤1 7/8)
	2800
	(>2600 to ≤3000)
	Very Light
	Light
	Light
	Light

	2
	(>1 7/8 to ≤2 ¼)
	3200
	(>3000 to ≤3600)
	Very Light
	Very Light
	Light
	Light

	2 ½
	(>2 ¼ to ≤2 ¾)
	4000
	(>3600 to ≤4400)
	Very Light
	Very Light
	Light
	Light

	3
	(>2 ¾ to ≤3 ¼)
	4800
	(>4400 to ≤5200)
	Very Light
	Very Light
	Very Light
	Light

	≥3 ½
	(>3 ¼)
	≥5600
	(>5200)
	Very Light
	Very Light
	Very Light
	Very Light





NOTES
The METAR/SPECI reported visibility or flight crew observed visibility will be used with this visibility table to establish snowfall intensity for Type I, II, III and IV holdover time guidelines, during snow, snow grain, or snow pellet precipitation conditions. This visibility table will also be used when snow, snow grains, or snow pellets are accompanied by blowing or drifting snow, or when snow is mixed with ice crystals, freezing fog, rain or drizzle in the METAR/SPECI.
The use of Runway Visual Range (RVR) is not permitted for determining visibility used with the holdover tables.
Some METARs contain tower visibility as well as surface visibility. Whenever surface visibility is available from an official source, such as a METAR, in either the main body of the METAR or in the Remarks (“RMK”) section, the preferred action is to use the surface visibility value.
If the visibility is being reduced by snow along with form(s) of obscuration such as fog, haze, smoke, etc., use of the table above may overestimate the actual snowfall intensity. However, use of the snowfall intensity being reported by the weather observer or automated surface observing system (ASOS), from the FMH-1 Table, may underestimate the actual snowfall intensity as it does not directly correlate to the snowfall intensities used when determining holdover times. Use of the visibility table in all snow conditions with or without obscurations is recommended. 
[bookmark: _Hlk107319670]Example for how to read and use the table: CYVO 160200Z 15011G17KT 1SM -SN DRSN OVC009 M06/M08 A2948 
In the above METAR the snowfall intensity is reported as light. However, based upon the “Snowfall Intensities as a Function of Prevailing Visibility” table, with a visibility of 1 statute mile, at night and a temperature of -6 °C, the snowfall intensity is classified as moderate. The snowfall intensity of moderate - not the METAR reported intensity of light - will be used to determine which holdover time guideline value is appropriate for the fluid in use.
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[bookmark: _TABLE_8-1][bookmark: _TABLE_9._GUIDELINES][bookmark: _TABLE_9-I._GUIDELINES][bookmark: _Ref233887239][bookmark: _Toc508704844][bookmark: _Toc517253589][bookmark: _Toc45702524][bookmark: _Toc140480380][bookmark: _Toc234306100][bookmark: _Toc391757747][bookmark: _Toc425184898][bookmark: _Toc436349457]Table 58:
Type I Fluids Tested for Anti-Icing Performance and Aerodynamic Acceptance
(see cautions and notes on pages 87 and 88)
	Fluid Name
	Type 
of 
Glycol1
	Expiry2
(y-m-d)
	Lowest Operational Use Temperature3

	
	
	
	Dilution4,5
(fluid/water)
	low speed 
aerodynamic test6
	middle speed 
aerodynamic test6
	high speed 
aerodynamic test6

	
	
	
	
	°C
	°F
	°C
	°F
	°C
	°F

	ABAX Industries

	DE-950
	PG
	30-06-01
	71/29
	-26
	-15
	Not tested11
	-31 
	-24

	Aéro Mag 2000 SYR LLC

	DeiceX PG ADF Concentrate
(Multiple Location)
	PG
	Y-M-D12
	65/35
	-25
	-13
	Not tested11
	-31.5
	-25

	AFLRUS LLC

	Orange Flo Type 1
	EG
	26-11-15
	70/30
	-42
	-44
	Not tested11
	-40
	-40

	ALAB International

	PROFLIGHT EG1
	EG
	25-06-019
	70/30
	-43.5
	-46
	Not tested11
	-44
	-47

	AllClear Systems LLC

	Lift-Off E-188
	EG
	30-06-01
	70/30
	-40
	-40
	Not tested11
	-46
	-51

	Lift-Off P-88
	PG
	30-06-01
	70/30
	-24.5
	-12
	Not tested11
	-29.5
	-21

	ASGlobal

	Sky-Go EG
	EG
	26-09-23
	70/30
	-3114
	-2414
	Not tested11
	-44
	-47

	Sky-Go PG
	PG
	26-07-2713
	70/30
	-21.514
	-714
	Not tested11
	-30.5
	-23

	Sky-Go PG 80
	PG
	27-08-07
	70/30
	-2514
	-1314
	Not tested11
	-31.5
	-25

	AVIAFLUID International Ltd.

	AVIAFLO EG
	EG
	25-03-239
	70/30
	-40.5
	-41
	Not tested11
	-41
	-42

	Aviation Xi’an High-Tech Physical Chemical Co. Ltd.10

	Cleanwing E
	EG
	28-06-01
	75/25
	-37
	-35
	Not tested11
	-37
	-35

	Cleanwing I
	PG
	27-06-08
	75/25
	Not tested11
	Not tested11
	-39.5
	-39

	Cleanwing S-92
	EG
	28-06-01
	75/25
	-35
	-31
	Not tested11
	-40
	-40

	KHF-1
	PG
	27-06-08
	75/25
	Not tested11
	Not tested11
	-38.5
	-37

	Beijing Yadilite Aviation Advanced Materials Corporation10

	YD-101A Type I
	EG
	25-02-269
	70/30
	Not tested11
	Not tested11
	-38
	-36





Table 58 (CONT’D):
TYPE I FLUIDS TESTED FOR ANTI-ICING PERFORMANCE AND AERODYNAMIC ACCEPTANCE
(see cautions and notes on pages 87 and 88)
	Fluid Name
	Type 
of 
Glycol1
	Expiry2
(y-m-d)
	Lowest Operational Use Temperature3

	
	
	
	Dilution4,5
(fluid/water)
	low speed 
aerodynamic test6
	middle speed 
aerodynamic test6
	high speed 
aerodynamic test6

	
	
	
	
	°C
	°F
	°C
	°F
	°C
	°F

	CHEMCO Inc.

	CHEMR EG I
	EG
	28-06-01
	70/30
	-37
	-35
	Not tested11
	-43
	-45

	CHEMR REG I
	EG
	30-06-01
	75/25
	-36.5
	-34
	Not tested11
	-43.5
	-46

	Chongqing Joba Chemical Co.,Ltd

	FW-I
	EG
	30-06-01
	75/25
	-43
	-45
	Not tested11
	-46
	-51

	Clariant Produkte (Deutschland) GmbH

	Safewing EG I Arctic
	EG
	26-08-23
	70/30
	-43.5
	-46
	Not tested11
	-46
	-51

	Safewing MP I 1938 ECO (80)
	PG
	28-06-19
	71/29
	-25
	-13
	Not tested11
	-32.5
	-27

	Safewing MP I ECO PLUS (80)
	PG
	27-06-01
	71/29
	-25
	-13
	Not tested11
	-33
	-27

	Safewing MP I LFD 80
	PG
	29-06-01
	71/29
	-26
	-15
	Not tested11
	-33
	-27

	Safewing MP I LFD 80 Pre-Mix 55%
	PG
	29-06-01
	as supplied
	Not tested11
	Not tested11
	-17
	1

	Safewing MP I LFD 88
	PG
	27-06-01
	65/35
	-26
	-15
	Not tested11
	-33
	-27

	Safewing MP I LFD PLUS 88
	PG
	30-06-01
	65/35
	-25
	-13
	Not tested11
	-34
	-29

	Cryotech Deicing Technology

	Polar Plus® LT
	PG
	28-06-01
	63/37
	-27
	-17
	Not tested11
	-33
	-27

	Polar Plus® LT (80)
	PG
	28-06-01
	70/30
	-27
	-17
	Not tested11
	-33
	-27

	Dow Inc.

	UCAR™ ADF Concentrate
	EG
	27-06-01
	75/25
	-36
	-33
	Not tested11
	-45
	-49

	UCAR™ ADF XL5415
	EG
	27-06-01
	as supplied
	-33 
	-27
	Not tested11
	-33
	-27

	UCAR™ PG ADF Concentrate
	PG
	27-06-01
	65/35
	-25
	-13
	Not tested11
	-32
	-26

	UCAR™ PG ADF Dilute 55/4516
	PG
	27-06-01
	as supplied
	-24 
	-11
	Not tested11
	-25
	-13

	ESSPO CHEMICALS D.O.O.10

	Nordwing EG1
	EG
	27-06-01
	70/30
	-42
	-44
	Not tested11
	-48
	-54

	Nordwing PG1
	PG
	27-06-01
	70/30
	-25
	-13
	Not tested11
	-29
	-20





Table 58 (CONT’D):
TYPE I FLUIDS TESTED FOR ANTI-ICING PERFORMANCE AND AERODYNAMIC ACCEPTANCE
(see cautions and notes on pages 87 and 88)
	Fluid Name
	Type 
of 
Glycol1
	Expiry2
(y-m-d)
	Lowest Operational Use Temperature3

	
	
	
	Dilution4,5
(fluid/water)
	low speed 
aerodynamic test6
	middle speed 
aerodynamic test6
	high speed 
aerodynamic test6

	
	
	
	
	°C
	°F
	°C
	°F
	°C
	°F

	HOC Industries10

	SafeTemp® ES Plus
	PG
	28-07-04
	65/35
	-25.5
	-14
	Not tested11
	-29
	-20

	Inland Technologies Inc.

	DuraGly-E Type I ADF Concentrate
	EG
	23-02-089
	60/40
	-33
	-27
	Not tested11
	-33
	-27

	Inland ADF Concentrate
(Multiple Location)
	EG
	Y-M-D17
	75/25
	-36
	-33
	Not tested11
	-42.5
	-45

	SafeTemp® ES Plus 
(Multiple Location)
	PG
	Y-M-D18
	65/35
	-25.5
	-14
	Not tested11
	-31
	-24

	JSC RCP Nordix

	DEFROST EG 88.1
	EG
	25-04-139
	70/30
	-40.5
	-41
	Not tested11
	-44.5
	-48

	DEFROST PG 1
	PG
	23-11-219
	70/30
	-24.5
	-12
	Not tested11
	-31.5
	-25

	Kilfrost Limited

	Kilfrost DF Plus
	PG
	27-06-01
	69/31
	-25.5
	-14
	Not tested11
	-32
	-26

	Kilfrost DF Plus (80)
	PG
	24-07-149
	69/31
	-26
	-15
	Not tested11
	-31.5
	-25

	Kilfrost DF Plus (88)
	PG
	23-06-059
	63/37
	-25.5
	-14
	Not tested11
	-32
	-26

	Kilfrost Ice Clear I
	PG
	27-06-01
	70/30
	-26
	-15
	Not tested11
	-33
	-27

	LNT Solutions10

	LNT E188
	EG
	25-08-139
	70/30
	-30.5
	-23
	Not tested11
	-41
	-42

	LNT P180
	PG
	26-11-10
	69/31
	-26
	-15
	Not tested11
	-32
	-26

	MAX TECH AIRCRAFT MAINTENANCE AND REPAIR LLC

	MTL EG-1
	EG
	27-09-25
	70/30
	-42.5
	-45
	Not tested11
	-46
	-51

	MTL PG-1
	PG
	27-09-12
	70/30
	-24
	-11
	Not tested11
	-30.5
	-23

	MKS DevO Chemicals

	COREICEPHOB TYPE I EG BASED
	EG
	28-06-01
	70/30
	Not tested11
	Not tested11
	-47
	-53

	COREICEPHOB TYPE I
	PG
	30-06-01
	71/29
	Not tested11
	Not tested11
	-32.5
	-27





Table 58 (CONT’D):
TYPE I FLUIDS TESTED FOR ANTI-ICING PERFORMANCE AND AERODYNAMIC ACCEPTANCE
(see cautions and notes on pages 87 and 88)
	Fluid Name
	Type 
of 
Glycol1
	Expiry2
(y-m-d)
	Lowest Operational Use Temperature3

	
	
	
	Dilution4,5
(fluid/water)
	low speed 
aerodynamic test6
	middle speed 
aerodynamic test6
	high speed 
aerodynamic test6

	
	
	
	
	°C
	°F
	°C
	°F
	°C
	°F

	Newave Aerochemical Co. Ltd.

	FCY-1A
	EG
	27-06-01
	75/25
	-4014
	-4014
	Not tested11
	-40
	-40

	FCY-1Bio+
	EG
	29-06-01
	75/25
	-40.5
	-41
	Not tested11
	-40.5
	-41

	FCY-1Bio+ (R)
	EG
	30-06-01
	75/25
	Not tested11
	Not tested11
	-46
	-51

	ROMCHIM PROTECT SRL10

	ADD-PROTECT NG Type I
	EG
	26-06-019
	60/40
	-22
	-8
	Not tested11
	-22
	-8

	ADD-PROTECT Type I
	PG
	27-06-01
	70/30
	-25.5
	-14
	Not tested11
	-31
	-24

	Shaanxi Cleanway Aviation Chemical Co., Ltd10

	Cleansurface I
	EG
	25-06-079
	75/25
	Not tested11
	Not tested11
	-40.5
	-41

	Topan LLP10

	TOPAN TYPE I
	EG
	24-07-139
	75/25
	-35.5
	-32
	Not tested11
	-42
	-44

	Turbotect Slovakia, s.r.o.

	TURBOTECT DF I
	PG
	26-10-08
	as supplied
	-12.5
	9.5
	Not tested11
	-20
	-4

	Xinjiang Zhongtian Liyang Aviation Newmaterial Technology Co., Ltd.

	Clearice-I 
	EG
	29-06-01
	60/40
	Not tested11
	Not tested11
	-30
	-22

	Clearice-IB
	EG
	29-06-01
	75/25
	Not tested11
	Not tested11
	-43.5
	-46




[bookmark: _TABLE_8-2][bookmark: _Ref233887308][bookmark: _Toc140480381][bookmark: _Toc45702525][bookmark: _Toc517253590][bookmark: _Toc508704845][bookmark: _Toc234306101]Table 59:
Type II Fluids Tested for Anti-Icing Performance and Aerodynamic Acceptance
(see cautions and notes on pages 87 and 88)
	Fluid Name
	Type of Glycol1
	Expiry2
(y-m-d)
	Dilution
(fluid/water)
	Lowest Operational Use Temperature3
	AS 9968 Viscosity7 (mPa.s)

	
	
	
	
	middle speed 
aerodynamic test6
	high speed 
aerodynamic test6
	Lowest On-Wing Viscosity8
	Highest On-Wing Viscosity8

	
	
	
	
	
	
	Manufacturer Method
	Alternate 
Method
	Manufacturer Method
	Alternate 
Method

	
	
	
	
	°C
	°F
	°C
	°F
	
	
	
	

	ABAX Industries

	ECOWING AD-2
	PG
	27-06-01
	100/0
	Not tested11
	-27
	-17
	5 750 (a)
	Not Available19
	17 200 (a)
	14 000 (h)

	
	
	
	75/25
	Not tested11
	-15
	5
	12 000 (c)
	Not Available19
	30 200 (c)
	32 000 (h)

	
	
	
	50/509
	Not tested11
	-3
	27
	7 500 (a)
	Not Available19
	26 900 (c)
	36 800 (h)

	Aviation Xi’an High-Tech Physical Chemical Co. Ltd.10

	Cleanwing II
	PG
	27-06-01
	100/0
	Not tested11
	-25
	-13
	4 650 (e)
	4 500 (a)
	13 500 (a)
	11 100 (i)

	
	
	
	75/25
	Not tested11
	-15
	5
	9 450 (e)
	10 000 (a)
	14 600 (i)
	Not Available19

	
	
	
	50/50
	Not tested11
	-4.5
	24
	10 150 (e)
	10 200 (a)
	12 900 (i)
	Not Available19

	Clariant Produkte (Deutschland) GmbH

	Safewing MP II FLIGHT
	PG
	28-06-01
	100/0
	Not tested11
	-29
	-20
	3 340 (a)
	Not Available19
	20 500 (r)
	20 500 (c)

	
	
	
	75/25
	Not tested11
	-14
	7
	12 900 (c)
	Not Available19
	47 800 (r)
	47 800 (c)

	
	
	
	50/50
	Not tested11
	-3.5
	26
	11 500 (a)
	Not Available19
	63 000 (r)
	63 000 (c)

	Cryotech Deicing Technology

	Polar Guard® II
	PG
	27-06-01
	100/0
	Not tested11
	-30.5
	-23
	4 400 (f)
	4 050 (a)
	17 000 (f)
	16 200 (a)

	
	
	
	75/25
	Not tested11
	-14
	7
	11 600 (f)
	9 750 (a)
	38 000 (c)
	Not Available19

	
	
	
	50/50
	Not tested11
	-3.5
	26
	80 (a)
	Not Available19
	48 000 (c)
	Not Available19

	ESSPO CHEMICALS D.O.O.10

	Nordwing PG2
	PG
	27-06-01
	100/0
	Not tested11
	-30
	-22
	11 450 (a)
	9 500 (h)
	20 500 (c)
	18,100 (h)

	
	
	
	75/25
	Dilution Not Applicable
	Dilution Not Applicable

	
	
	
	50/50
	Dilution Not Applicable
	Dilution Not Applicable

	Kilfrost Limited

	ABC-K Plus
	PG
	27-07-24
	100/0
	Not tested11
	-29
	-20
	2 850 (e)
	2 640 (a)
	13 400 (a)
	Not Available19

	
	
	
	75/25
	Not tested11
	-14.5
	6
	12 650 (e)
	12 650 (c)
	29 000 (c)
	Not Available19

	
	
	
	50/50
	Not tested11
	-3.5
	26
	4 200 (e)
	5 260 (a)
	15 000 (a)
	Not Available19

	Ice Clear II
	PG
	28-06-01
	100/0
	Not tested11
	-28
	-18
	4 100 (a)
	18 000 (n)
	26 000 (c)
	Not Available19

	
	
	
	75/25
	Dilution Not Applicable
	Dilution Not Applicable

	
	
	
	50/50
	Dilution Not Applicable
	Dilution Not Applicable




Table 59 (CONT’D):
TYPE II FLUIDS TESTED FOR ANTI-ICING PERFORMANCE AND AERODYNAMIC ACCEPTANCE
(see cautions and notes on pages 87 and 88)
	Fluid Name
	Type of Glycol1
	Expiry2
(y-m-d)
	Dilution
(fluid/water)
	Lowest Operational Use Temperature3
	AS 9968 Viscosity7 (mPa.s)

	
	
	
	
	middle speed 
aerodynamic test6
	high speed 
aerodynamic test6
	Lowest On-Wing Viscosity8
	Highest On-Wing Viscosity8

	
	
	
	
	
	
	Manufacturer Method
	Alternate 
Method
	Manufacturer Method
	Alternate 
Method

	
	
	
	
	°C
	°F
	°C
	°F
	
	
	
	

	LNT Solutions

	P250
	PG
	28-06-01
	100/0
	Not tested11
	-29
	-20
	20 800 (l)
	Not Available19
	44 200 (h)
	Not Available19

	
	
	
	75/25
	Dilution Not Applicable
	Dilution Not Applicable

	
	
	
	50/50
	Dilution Not Applicable
	Dilution Not Applicable

	MKS DevO Chemicals

	COREICEPHOB 
TYPE II
	PG
	28-06-01
	100/0
	Not tested11
	-27
	-17
	34 400 (i)
	Not Available19
	50 200 (i)
	Not Available19

	
	
	
	75/25
	Dilution Not Applicable
	Dilution Not Applicable

	
	
	
	50/50
	Not tested11
	-3.5
	26
	20 700 (i)
	Not Available19
	30 700 (i)
	Not Available19

	Newave Aerochemical Co. Ltd.

	FCY-2
	PG
	27-06-01
	100/0
	Not tested11
	-28
	-18
	7 000 (e)
	8 920 (a)
	24 800 (c)
	Not Available19

	
	
	
	75/25
	Dilution Not Applicable 
	Dilution Not Applicable 

	
	
	
	50/50
	Dilution Not Applicable 
	Dilution Not Applicable 

	ROMCHIM PROTECT SRL10

	ADD-PROTECT
NG Type II
	PG
	25-06-019
	100/0
	Not tested11
	-28
	-18
	5 200 (a)
	Not Available19
	12 400 (a)
	Not Available19

	
	
	
	75/25
	Not tested11
	-14.5
	6
	8 250 (a)
	Not Available19
	43 800 (i)
	Not Available19

	
	
	
	50/50
	Not tested11
	-3
	27
	5 850 (a)
	Not Available19
	38 900 (i)
	Not Available19

	ADD-PROTECT
Type II
	PG
	25-06-019
	100/0
	Not tested11
	-28
	-18
	4 000 (a)
	Not Available19
	18 250 (a)
	12 900 (i)

	
	
	
	75/25
	Not tested11
	-14
	7
	7 700 (a)
	Not Available19
	23 300 (c)
	23 200 (i)

	
	
	
	50/50
	Not tested11
	-3
	27
	14 500 (a)
	Not Available19
	31 400 (c)
	22 600 (i)




[bookmark: _TABLE_8-3][bookmark: _Toc140480382][bookmark: _Toc45702526][bookmark: _Toc517253591][bookmark: _Toc508704846][bookmark: _Toc234306102]Table 60:
Type III Fluids Tested for Anti-Icing Performance and Aerodynamic Acceptance
(see cautions and notes on pages 87 and 88)
	Fluid Name
	Type of Glycol1
	Expiry2
(y-m-d)
	Dilution
(fluid/water)
	Lowest Operational Use Temperature3
	AS 9968 Viscosity7 (mPa.s)

	
	
	
	
	low speed 
aerodynamic test6
	middle speed 
aerodynamic test6
	high speed 
aerodynamic test6
	Lowest On-Wing Viscosity8
	Highest On-Wing Viscosity8

	
	
	
	
	
	
	
	Manufacturer Method
	Alternate 
Method
	Manufacturer Method
	Alternate 
Method

	
	
	
	
	°C
	°F
	°C
	°F
	°C
	°F
	
	
	
	

	AllClear Systems LLC

	AeroClear MAX
	EG
	27-06-01
	100/0
	-16
	3
	-20.5
	-5
	-35
	-31
	7 800 (p)
	Not Available19
	15 000 (p)
	Not Available19

	
	
	
	75/25
	Dilution Not Applicable
	Dilution Not Applicable

	
	
	
	50/50
	Dilution Not Applicable
	Dilution Not Applicable




[bookmark: _TABLE_8-4][bookmark: _Ref233887352][bookmark: _Toc140480383][bookmark: _Toc45702527][bookmark: _Toc517253592][bookmark: _Toc508704847][bookmark: _Toc234306103]Table 61:
Type IV Fluids Tested for Anti-Icing Performance and Aerodynamic Acceptance 
(see cautions and notes on pages 87 and 88)
	Fluid Name
	Type of Glycol1
	Expiry2
(y-m-d)
	Dilution
(fluid/water)
	Lowest Operational Use Temperature3
	AS 9968 Viscosity7 (mPa.s)

	
	
	
	
	middle speed 
aerodynamic test6
	high speed 
aerodynamic test6
	Lowest On-Wing Viscosity8
	Highest On-Wing Viscosity8

	
	
	
	
	
	
	Manufacturer Method
	Alternate 
Method
	Manufacturer Method
	Alternate 
Method

	
	
	
	
	°C
	°F
	°C
	°F
	
	
	
	

	ABAX Industries

	ECOWING AD-49
	PG
	28-06-01
	100/0
	Not tested11
	-26
	-15
	12 150 (h)
	11 000 (a)
	22 400 (h)
	25 900 (c)

	
	
	
	75/25
	Dilution Not Applicable
	Dilution Not Applicable

	
	
	
	50/50
	Dilution Not Applicable
	Dilution Not Applicable

	AFLRUS LLC

	Green Flo Type 4
	EG
	26-11-25
	100/0
	Not tested11
	-30
	-22
	6 550 (a)
	Not Available19
	13 400 (a)
	Not Available19

	
	
	
	75/25
	Dilution Not Applicable
	Dilution Not Applicable

	
	
	
	50/50
	Dilution Not Applicable
	Dilution Not Applicable

	ALAB International

	PROFLIGHT EG4
	EG
	28-06-01
	100/0
	Not tested11
	-26
	-15
	1 840 (a)
	Not Available19
	6 180 (a)
	Not Available19

	
	
	
	75/25
	Dilution Not Applicable
	Dilution Not Applicable

	
	
	
	50/50
	Dilution Not Applicable
	Dilution Not Applicable

	PROFLIGHT PG4
	PG
	26-06-019
	100/0
	Not tested11
	-29
	-20
	10 600 (a)
	Not Available19
	17 800 (h)
	Not Available19

	
	
	
	75/25
	Dilution Not Applicable
	Dilution Not Applicable

	
	
	
	50/50
	Dilution Not Applicable
	Dilution Not Applicable

	AllClear Systems LLC

	Clear IV Flight
	PG
	27-06-01
	100/0
	Not tested11
	-23
	-9
	22 300 (n)
	21 900 (m)
	31 700 (n)
	29 400 (i)

	
	
	
	75/25
	Dilution Not Applicable
	Dilution Not Applicable

	
	
	
	50/50
	Dilution Not Applicable
	Dilution Not Applicable

	ClearWing EG
	EG
	27-06-01
	100/0
	Not tested11
	-29
	-20
	35 500 (o)
	13 350 (a)
	51 800 (k)
	Not Available19

	
	
	
	75/25
	Dilution Not Applicable
	Dilution Not Applicable

	
	
	
	50/50
	Dilution Not Applicable
	Dilution Not Applicable

	ASGlobal

	[bookmark: _Hlk72933887]4Flite EG
	EG
	26-09-24
	100/0
	Not tested11
	-30
	-22
	6 600 (a)
	Not Available19
	17 300 (a)
	Not Available19

	
	
	
	75/25
	Dilution Not Applicable
	Dilution Not Applicable

	
	
	
	50/50
	Dilution Not Applicable
	Dilution Not Applicable

	4Flite PG
	PG
	27-07-24
	100/0
	Not tested11
	-26
	-15
	26 100 (c)
	Not Available19
	36 500 (c)
	Not Available19

	
	
	
	75/25
	Dilution Not Applicable
	Dilution Not Applicable

	
	
	
	50/50
	Dilution Not Applicable
	Dilution Not Applicable



Table 61 (CONT’D):
TYPE IV FLUIDS TESTED FOR ANTI-ICING PERFORMANCE AND AERODYNAMIC ACCEPTANCE
(see cautions and notes on pages 87 and 88)
	Fluid Name
	Type of Glycol1
	Expiry2
(y-m-d)
	Dilution
(fluid/water)
	Lowest Operational Use Temperature3
	AS 9968 Viscosity7 (mPa.s)

	
	
	
	
	middle speed 
aerodynamic test6
	high speed 
aerodynamic test6
	Lowest On-Wing Viscosity8
	Highest On-Wing Viscosity8

	
	
	
	
	
	
	Manufacturer Method
	Alternate 
Method
	Manufacturer Method
	Alternate 
Method

	
	
	
	
	°C
	°F
	°C
	°F
	
	
	
	

	AVIAFLUID International Ltd 

	AVIAFlight PG
	PG
	23-07-019
	100/0
	Not tested11
	-25.5
	-14
	28 600 (c)
	Not Available19
	35 900 (c)
	22 200 (i)

	
	
	
	75/25
	Dilution Not Applicable
	Dilution Not Applicable

	
	
	
	50/50
	Dilution Not Applicable
	Dilution Not Applicable

	CHEMCO Inc.

	ChemR EG IV
	EG
	23-04-079
	100/0
	Not tested11
	-27
	-17
	46 400 (n)
	19 450 (c)
	67 000 (n)
	Not Available19

	
	
	
	75/25
	Dilution Not Applicable
	Dilution Not Applicable

	
	
	
	50/50
	Dilution Not Applicable
	Dilution Not Applicable

	ChemR Nordik IV
	EG
	27-06-01
	100/0
	Not tested11
	-29
	-20
	60 800 (o)
	43 100 (c)
	87 100 (o)
	Not Available19

	
	
	
	75/25
	Dilution Not Applicable
	Dilution Not Applicable

	
	
	
	50/50
	Dilution Not Applicable
	Dilution Not Applicable

	Chongqing Joba Chemical Co.,Ltd

	FW-IV
	EG
	28-06-01
	100/0
	Not tested11
	-29
	-20
	32 600 (j)
	Not Available19
	66 200 (j)
	Not Available19

	
	
	
	75/25
	Dilution Not Applicable
	Dilution Not Applicable

	
	
	
	50/50
	Dilution Not Applicable
	Dilution Not Applicable

	Clariant Produkte (Deutschland) GmbH

	[bookmark: _Hlk126217657]Safewing MP IV 
LAUNCH
	PG
	28-06-01
	100/0
	Not tested11
	-28.5
	-19
	7 550 (a)
	Not Available19
	20 500 (r)
	20 500 (c)

	
	
	
	75/25
	Not tested11
	-14
	7
	18 000 (a)
	Not Available19
	47 800 (r)
	47 800 (c)

	
	
	
	50/50
	Not tested11
	-3.5
	26
	17 800 (a)
	Not Available19
	63 000 (r)
	63 000 (c)

	Safewing MP IV 
LAUNCH PLUS
	PG
	27-06-01
	100/0
	Not tested11
	-29
	-20
	8 700 (q)
	8 450 (a)
	21 000 (r)
	21 000 (c)

	
	
	
	75/25
	Not tested11
	-14
	7
	18 800 (r)
	17 200 (c)
	51 600 (r)
	51 600 (c)

	
	
	
	50/50
	Not tested11
	-3.5
	26
	9 700 (q)
	12 150 (a)
	65 700 (r)
	65 700 (c)

	Cryotech Deicing Technology

	Polar Guard® Advance
	PG
	27-06-01
	100/0
	Not tested11
	-30.5
	-23
	4 400 (f)
	4 050 (a)
	17 000 (f)
	16 200 (a)

	
	
	
	75/25
	Not tested11
	-14
	7
	11 600 (f)
	9 750 (a)
	38 000 (c)
	Not Available19

	
	
	
	50/50
	Not tested11
	-3.5
	26
	80 (a)
	Not Available19
	48 000 (c)
	Not Available19

	Polar Guard® Xtend
	PG
	27-06-01
	100/0
	Not tested11
	-29
	-20
	6 000 (f)
	6 350 (a)
	23 500 (f)
	23 200 (c)

	
	
	
	75/25
	Dilution Not Applicable
	Dilution Not Applicable

	
	
	
	50/50
	Dilution Not Applicable
	Dilution Not Applicable


Table 61 (CONT’D):
TYPE IV FLUIDS TESTED FOR ANTI-ICING PERFORMANCE AND AERODYNAMIC ACCEPTANCE
(see cautions and notes on pages 87 and 88)
	Fluid Name
	Type of Glycol1
	Expiry2
(y-m-d)
	Dilution
(fluid/water)
	Lowest Operational Use Temperature3
	AS9968 Viscosity7 (mPa.s)

	
	
	
	
	middle speed 
aerodynamic test6
	high speed 
aerodynamic test6
	Lowest On-Wing Viscosity8
	Highest On-Wing Viscosity8

	
	
	
	
	
	
	Manufacturer Method
	Alternate 
Method
	Manufacturer Method
	Alternate 
Method

	
	
	
	
	°C
	°F
	°C
	°F
	
	
	
	

	Dow Inc.

	UCAR ENDURANCE™ EG106 ADF/AAF
	EG
	27-06-01
	100/0
	Not tested11
	-29
	-20
	24 850 (j)
	2 230 (a)
	47 800 (j)
	5 900 (a)

	
	
	
	75/25
	Dilution Not Applicable
	Dilution Not Applicable

	
	
	
	50/50
	Dilution Not Applicable
	Dilution Not Applicable

	UCAR™ FLIGHTGUARD™ 
AD-49
	PG
	27-06-01
	100/0
	Not tested11
	-26
	-15
	12 150 (h)
	11 000 (a)
	22 400 (h)
	25 900 (c)

	
	
	
	75/25
	Dilution Not Applicable
	Dilution Not Applicable

	
	
	
	50/50
	Dilution Not Applicable
	Dilution Not Applicable

	ESSPO CHEMICALS D.O.O.10

	Nordwing PG4
	PG
	27-06-01
	100/0
	Not tested11
	-30
	-22
	11 550 (a)
	9 800 (h)
	20 000 (c)
	20 300 (h)

	
	
	
	75/25
	Dilution Not Applicable
	Dilution Not Applicable

	
	
	
	50/50
	Dilution Not Applicable
	Dilution Not Applicable

	Inland Technologies Inc.

	ECO-SHIELD®
	PG
	24-10-289
	100/0
	Not tested11
	-25.5
	-14
	11 050 (a)
	Not Available19
	25 800 (i)
	34 500 (c)

	
	
	
	75/25
	Dilution Not Applicable
	Dilution Not Applicable

	
	
	
	50/50
	Dilution Not Applicable
	Dilution Not Applicable

	JSC RCP Nordix

	Defrost ECO 4
	PG
	23-08-129
	100/0
	Not tested11
	-25.5
	-14
	9 800 (h)
	12 350 (a)
	14 800 (i)
	17 340 (a)

	
	
	
	75/25
	Dilution Not Applicable
	Dilution Not Applicable

	
	
	
	50/50
	Dilution Not Applicable
	Dilution Not Applicable

	Defrost NORTH 4
	EG
	23-06-019
	100/0
	Not tested11
	-26
	-15
	2 500 (a)
	Not Available19
	5 350 (a)
	Not Available19

	
	
	
	75/25
	Dilution Not Applicable
	Dilution Not Applicable

	
	
	
	50/50
	Dilution Not Applicable
	Dilution Not Applicable

	Kilfrost Limited

	ABC-S Plus
	PG
	27-08-28
	100/0
	Not tested11
	-28
	-18
	17 900 (e)
	17 900 (c)
	43 800 (c)
	Not Available19

	
	
	
	75/25
	Not tested11
	-14.5
	6
	18 300 (e)
	18 300 (c)
	58 000 (c)
	Not Available19

	
	
	
	50/50
	Not tested11
	-3.5
	26
	7 500 (e)
	7 500 (a)
	27 000 (c)
	Not Available19




Table 61 (CONT’D):
TYPE IV FLUIDS TESTED FOR ANTI-ICING PERFORMANCE AND AERODYNAMIC ACCEPTANCE
(see cautions and notes on pages 87 and 88)
	Fluid Name
	Type of Glycol1
	Expiry2
(y-m-d)
	Dilution
(fluid/water)
	Lowest Operational Use Temperature3
	AS9968 Viscosity7 (mPa.s)

	
	
	
	
	middle speed 
aerodynamic test6
	high speed 
aerodynamic test6
	Lowest On-Wing Viscosity8
	Highest On-Wing Viscosity8

	
	
	
	
	
	
	Manufacturer Method
	Alternate 
Method
	Manufacturer Method
	Alternate 
Method

	
	
	
	
	°C
	°F
	°C
	°F
	
	
	
	

	LNT Solutions

	P450
	PG
	28-06-01
	100/0
	Not tested11
	-29
	-20
	15 900 (l)
	Not Available19
	30 500 (h)
	Not Available19

	
	
	
	75/25
	Dilution Not Applicable
	Dilution Not Applicable

	
	
	
	50/50
	Dilution Not Applicable
	Dilution Not Applicable

	MAX TECH AIRCRAFT MAINTENANCE AND REPAIR LLC

	MTL 4-EG
	EG
	28-06-01
	100/0
	Not tested11
	-26.5
	-16
	3 200 (a)
	Not Available19
	29 200 (i)
	Not Available19

	
	
	
	75/25
	Dilution Not Applicable
	Dilution Not Applicable

	
	
	
	50/50
	Dilution Not Applicable
	Dilution Not Applicable

	MTL 4-PG
	PG
	27-10-23
	100/0
	Not tested11
	-27
	-17
	10 700 (a)
	Not Available19
	26 000 (c)
	Not Available19

	
	
	
	75/25
	Dilution Not Applicable
	Dilution Not Applicable

	
	
	
	50/50
	Dilution Not Applicable
	Dilution Not Applicable

	MKS DevO Chemicals

	COREICEPHOB 
TYPE-IV PG
	PG
	28-06-01
	100/0
	Not tested11
	-29
	-20
	50 200 (i)
	Not Available19
	60 900 (i)
	Not Available19

	
	
	
	75/25
	Dilution Not Applicable
	Dilution Not Applicable

	
	
	
	50/50
	Dilution Not Applicable
	Dilution Not Applicable

	Newave Aerochemical Co. Ltd.

	FCY 9311
	PG
	28-06-01
	100/0
	Not tested11
	-29.5
	-21
	14 100 (c)
	Not Available19
	27 600 (c)
	25 700 (i)

	
	
	
	75/25
	Dilution Not Applicable
	Dilution Not Applicable

	
	
	
	50/50
	Dilution Not Applicable
	Dilution Not Applicable

	FCY-EGIV
	EG
	28-06-01
	100/0
	Not tested11
	-29
	-20
	24 800 (g)
	6 300 (a)
	43 700 (k)
	78 000 (c)

	
	
	
	75/25
	Dilution Not Applicable
	Dilution Not Applicable

	
	
	
	50/50
	Dilution Not Applicable
	Dilution Not Applicable

	FCY-EGIV PLUS
	EG
	27-06-01
	100/0
	Not tested11
	-29
	-20
	27 400 (k)
	Not Available19
	66 900 (k)
	Not Available19

	
	
	
	75/25
	Dilution Not Applicable
	Dilution Not Applicable

	
	
	
	50/50
	Dilution Not Applicable
	Dilution Not Applicable





Table 61 (CONT’D):
TYPE IV FLUIDS TESTED FOR ANTI-ICING PERFORMANCE AND AERODYNAMIC ACCEPTANCE
(see cautions and notes on pages 87 and 88)
	Fluid Name
	Type of Glycol1
	Expiry2
(y-m-d)
	Dilution
(fluid/water)
	Lowest Operational Use Temperature3
	AS9968 Viscosity7 (mPa.s)

	
	
	
	
	middle speed 
aerodynamic test6
	high speed 
aerodynamic test6
	Lowest On-Wing Viscosity8
	Highest On-Wing Viscosity8

	
	
	
	
	
	
	Manufacturer Method
	Alternate 
Method
	Manufacturer Method
	Alternate 
Method

	
	
	
	
	°C
	°F
	°C
	°F
	
	
	
	

	Shaanxi Cleanway Aviation Chemical Co., Ltd10

	Cleansurface IV
	PG
	25-11-289
	100/0
	Not tested11
	-30
	-22
	16 750 (a)
	14 800 (h)
	29 700 (d)
	21 100 (i)

	
	
	
	75/25
	Dilution Not Applicable
	Dilution Not Applicable

	
	
	
	50/50
	Dilution Not Applicable
	Dilution Not Applicable

	Xinjiang Zhongtian Liyang Aviation Newmaterial Technology Co., Ltd.

	Clearice-IV
	EG
	26-11-11
	100/0
	Not tested11
	-29
	-20
	35 600 (d)
	Not Available19
	75 100 (d)
	Not Available19

	
	
	
	75/25
	Dilution Not Applicable
	Dilution Not Applicable

	
	
	
	50/50
	Dilution Not Applicable
	Dilution Not Applicable






[bookmark: _TABLE_9-I]CAUTIONS AND NOTES FOR TABLES 58, 59, 60, 61
CAUTIONS
· These tables list fluids that have been tested with respect to endurance time performance (Holdover Times), anti-icing performance (Water Spray Endurance Testing/High Humidity Endurance Testing) and aerodynamic acceptance (Type I: SAE ARP6207 §3.4.1, AMS1424 §3.5.2 and §3.5.3; Type II/ III/ IV: SAE ARP5718 §FOREWARD, AMS1428 §3.2.4 and §3.2.5) only. These tests were conducted by APS Aviation Inc. (www.apsaviation.ca) and Anti-icing Materials International Laboratory (AMIL) (https://lima.uqac.ca). The end user is responsible for contacting the fluid manufacturer to confirm all other SAE AMS1424/1428 technical requirement tests, such as fluid stability, toxicity, materials compatibility, etc. have been conducted. These technical requirement tests are typically conducted by Scientific Material International (SMI) (www.smiinc.com) and AMIL, or any acceptable source. 
· LOUT data provided in these tables is based strictly on the manufacturer’s data; the end user is responsible for verifying the validity of this data. 
· Type I fluids supplied in concentrated form must not be used in that form and must be diluted. 
NOTES
1	PG = conventional glycol (propylene glycol); EG = conventional glycol (ethylene glycol); DEG = conventional glycol (diethylene glycol); NCG = non-conventional glycol (organic non-ionic diols and triols, e.g. 1,3-propanediol, glycerine) and mixtures of non-conventional glycol and conventional glycol; NG = non-glycol (e.g. organic salts) and mixtures of non-glycol and glycol.
2	Expiry date is the earlier expiry date of the Aerodynamic Test(s) or Water Spray Endurance Test. Fluids that are tested after the issuance of this list will appear in a later update.
3	The values in this table were determined using test results from pre-production fluid samples when available. In some cases, the fluid manufacturer requested the publication of a more conservative value than the pre-production test value. The lowest operational use temperature (LOUT) for a given fluid is the higher (warmer) of: 
a) The lowest temperature at which the fluid meets the aerodynamic acceptance test for a given aircraft type; or
b) The actual freezing point of the fluid plus its freezing point buffer (Type I = 10 °C/18 °F; Type II/III/IV = 7 °C/13 °F).
Note: LOUTs are rounded to the nearest half degree Celsius and the values in degrees Fahrenheit are calculated to the nearest whole degree. 
4	The LOUT for Type I fluids that are intended to be diluted is derived from a dilution that provides the lowest operational use temperature. For other Type I dilutions, determine the freezing point of the fluid and add a 10 °C freezing point buffer, as a dilution will usually yield a higher and more restrictive operational use temperature. Consult the fluid manufacturer or fluid documentation for further clarification and guidance on establishing the appropriate operational use temperature of a diluted fluid.
5	Type I concentrate fluids have also been tested at 50/50 (glycol/water) dilution.
6	If uncertain as to what aerodynamic performance test information is applicable to a particular aircraft model, consult the aircraft manufacturer’s documentation or apply the most conservative values available.
7	The Alternate viscosity method should only be used for field verification and auditing purposes; when in doubt as to which method is appropriate, use the manufacturer method. Viscosity measurement methods are indicated as letters (in parentheses) beside each viscosity value. Details of each measurement method are shown in Table 62 on the following page. The exact measurement method (spindle, container, fluid volume, temperature, speed, duration) must be used to compare the viscosity of a sample to a viscosity given in this table.
8 	The lowest on-wing viscosity (LOWV), and highest on-wing viscosity (HOWV) values in this table are those of the fluids provided by the manufacturers for holdover time testing, and initial qualification aerodynamic testing. For the holdover times and lowest operation use temperature to be valid, the viscosity of the fluid on the wing shall not be lower than the LOWV value in this table and higher than the HOWV value in this table. The user should periodically ensure that the viscosity of a fluid sample taken from the wing surface complies with these limits.
9	Aerodynamic Performance and Anti-Icing Performance test data has expired; fluids listed in italics will be removed from this listing four years after expiry.
10	Manufacturer has not provided fluid information as required in SAE ARP5718B; fluid may be removed from this listing in subsequent revisions.
11	Manufacturer has indicated fluid was not tested.
12 	Dow Inc. UCAR™ PG ADF Concentrate, sold under the product name DeiceX PG ADF Concentrate, qualified from 2023-06-15.
13 	Currently in the test/re-test process. Contact the fluid manufacturer for latest information (see Appendix C for latest available contact information).
14	Fluid was not retested for low speed aerodynamics. This data will be removed four years after the expiry of the last low speed test.
15	For UCAR™ ADF XL54, refer to primary site qualification of UCAR™ ADF Concentrate.
16	For UCAR™ PG ADF Dilute 55/45, refer to primary site qualification of UCAR™ PG ADF Concentrate.
17	Dow Inc. UCAR™ ADF Concentrate, sold under the product name Inland ADF Concentrate, qualified from 2015-09-04.
18	Refer to preproduction qualification of SafeTemp® ES Plus submitted by HOC Industries, qualified from 2017-11-20.
19	Manufacturer has not provided an alternate method for measuring viscosity. Please use the Manufacturer Method.
[bookmark: _Ref233887420][bookmark: _Toc234306104]Table 62:
Viscosity measurement methods for Type II, III, and IV Fluids Tested for Anti-Icing Performance and Aerodynamic Acceptance
	Method
	Brookfield Spindle*
	Container
	Fluid Volume
	Temp.**
	Speed
	Duration

	a
	LV1 (with guard leg)
	600 mL low form (Griffin) beaker
	575 mL***
	20 °C
	0.3 rpm
	10.0 minutes

	b
	LV1 (with guard leg)
	600 mL low form (Griffin) beaker
	575 mL***
	20 °C
	0.3 rpm
	33.3 minutes

	c
	LV2-disc (with guard leg)
	600 mL low form (Griffin) beaker
	425 mL***
	20 °C
	0.3 rpm
	10.0 minutes

	d
	LV2-disc (with guard leg)
	600 mL low form (Griffin) beaker
	575 mL***
	20 °C
	0.3 rpm
	10.0 minutes

	e
	LV2-disc (with guard leg)
	150 mL tall form (Berzelius) beaker
	135 mL***
	20 °C
	0.3 rpm
	10.0 minutes

	f
	SC4-34/13R
	small sample adapter
	10 mL
	20 °C
	0.3 rpm
	10.0 minutes

	g
	SC4-34/13R
	small sample adapter
	10 mL
	0 °C
	0.3 rpm
	30.0 minutes

	h
	SC4-31/13R
	small sample adapter
	10 mL
	20 °C
	0.3 rpm
	10.0 minutes

	i
	SC4-31/13R
	small sample adapter
	10 mL
	20 °C
	0.3 rpm
	30.0 minutes

	j
	SC4-31/13R
	small sample adapter
	10 mL
	0 °C
	0.3 rpm
	10.0 minutes

	k
	SC4-31/13R
	small sample adapter
	10 mL
	0 °C
	0.3 rpm
	30.0 minutes

	l
	SC4-31/13R
	small sample adapter
	9.6 mL
	20 °C
	0.3 rpm
	10.0 minutes

	m
	SC4-31/13R
	small sample adapter
	9 mL
	20 °C
	0.3 rpm
	15.0 minutes

	n
	SC4-31/13R
	small sample adapter
	9 mL
	0 °C
	0.3 rpm
	10.0 minutes

	o
	SC4-31/13R
	small sample adapter
	9 mL
	0 °C
	0.3 rpm
	30.0 minutes

	p
	SC4-31/13R
	small sample adapter
	9 mL
	0 °C
	0.3 rpm
	65.0 minutes

	q
	LV1
	big sample adapter
	55 mL
	20 °C
	0.3 rpm
	10.0 minutes

	r
	LV2-disc
	big sample adapter
	60 mL
	20 °C
	0.3 rpm
	10.0 minutes


* Spindle must be attached to a Brookfield viscometer model equipped with an LV spring.
** Sample temperature will affect readings; ensure sufficient time is allowed for sample to reach thermal equilibrium before starting test. Use of a cooling bath strongly recommended.
*** If necessary, adjust fluid volume to ensure fluid is level with notch on the spindle shaft.


[bookmark: _Ref9506598][bookmark: _Toc508704848][bookmark: _Toc43986198][bookmark: _Toc234306105]Table 63: Guidelines for the Application of SAE Type I Fluid 
	Outside Air Temperature
(OAT)1
	One-Step Procedure
De/Anti-icing2
	Two-Step Procedure

	
	
	First Step: Deicing
	Second Step: Anti-icing3

	0 °C (32 °F)
and above
	Fluid/water mixture heated to at least 60 °C (140 °F) at the nozzle with a freezing point of at least 10° C (18 °F) below OAT
	Heated water or a heated 
fluid/water mixture 
	Fluid/water mixture heated to at least 60 °C (140 °F) at the nozzle with a freezing point of at least 10 °C (18 °F) below OAT

	Below 
0 °C (32 °F) 
	
	Heated fluid/water mixture with a freezing point at OAT or below
	


NOTES
1. Fluids must not be used at temperatures below their lowest operational use temperature (LOUT). 
[bookmark: _Hlk71276417]When anti-icing using the one-step procedure, a minimum quantity of 1 liter/m2 (~2 gal./100 sq. ft.) of Type I fluid mixture heated to at least 60 °C (140 °F) is required after all frozen contamination is removed. This is achieved using a continuous process. This application is necessary to heat the surfaces, as heat contributes significantly to the Type I fluid holdover times.
To be applied before first-step fluid freezes, typically within 3 minutes. This time may be higher than 3 minutes in some conditions, but potentially lower in heavy precipitation, colder temperatures, or for critical surfaces constructed of composite materials. If necessary, the second step shall be applied area by area (sectionally).
CAUTIONs
This table is applicable for the use of Type I holdover time guidelines in all conditions, including active frost. If holdover times are not required, a temperature of 60 °C (140 °F) at the nozzle is desirable.
If holdover times are required, the temperature of water or fluid/water mixtures shall be at least 60 °C (140 °F) at the nozzle. Upper temperature limit shall not exceed fluid and aircraft manufacturers’ recommendations.
To use Type I Holdover Times Guidelines in all conditions including active frost, an additional minimum of 1 liter/m2 (~2 gal./100 sq. ft.) of heated Type I fluid mixture must be applied to the surfaces after all frozen contamination is removed. This application is necessary to heat the surfaces, as heat contributes significantly to the Type I fluid holdover times. The required protection can be provided using a 1-step method by applying more fluid than is strictly needed to just remove all of the frozen contamination (the same additional amount stated above is required).
The lowest operational use temperature (LOUT) for a given Type I fluid is the higher (warmer) of:
a) The lowest temperature at which the fluid meets the aerodynamic acceptance test for a given aircraft type; or
b) The actual freezing point of the fluid plus a freezing point buffer of 10 °C (18 °F).
Wing skin temperatures may be colder or warmer than the OAT. Causes can include: radiation cooling, cold-soaked wing, or hangar storage. Consult the appropriate guidance (HOT Tables and FAA Ground Deicing General Information Document, Winter 2026-2027) for the contaminant in question.
When conducting aircraft deicing using a Type I fluid and not using the 10 °C/18 °F buffer, procedures must be developed and approved to ensure refreezing does not occur prior to takeoff.


[bookmark: _TABLE_10._GUIDELINES][bookmark: _TABLE_9-II/IV._GUIDELINES][bookmark: _Ref195099901][bookmark: _Toc508704849][bookmark: _Toc43986199][bookmark: _Toc234306106][bookmark: _Toc425184899][bookmark: _Toc436349458]Table 64: Guidelines for the Application of
SAE Type II and IV Fluid 
(FLUID CONCENTRATIONS IN % VOLUME)
	Outside Air Temperature
(OAT)1
	One-Step Procedure
De/Anti-icing
	Two-Step Procedure

	
	
	First Step: Deicing
	Second Step: Anti-icing2

	0 °C (32 °F) 
and above
	100/0, 75/25 or 50/50
Heated3 
Type II or IV
fluid/water mixture
	Heated water or a heated 
Type I, II, III, or IV 
fluid/water mixture
	100/0, 75/25 or 50/50
Heated or unheated 
Type II or IV 
fluid/water mixture

	Below 
0 °C (32 °F) 
to ‑3 °C (27 °F)
	100/0, 75/25 or 50/50
Heated3 
Type II or IV
fluid/water mixture
	Heated Type I, II, III, or IV fluid/water mixture with a freezing point at OAT or below
	100/0, 75/25 or 50/50
Heated or unheated 
Type II or IV 
fluid/water mixture

	Below 
-3 °C (27 °F) 
to ‑14 °C (7 °F)
	100/0 or 75/25
Heated3 
Type II or IV 
fluid/water mixture
	Heated Type I, II, III, or IV fluid/water mixture with a freezing point at OAT or below
	100/0 or 75/25
Heated or unheated 
Type II or IV 
fluid/water mixture

	Below
 -14 °C (7 °F) 
	100/0
Heated3 
Type II or IV fluid
	Heated Type I, II, III, or IV fluid/water mixture with a freezing point at OAT or below
	100/0
Heated or unheated 
Type II or IV fluid


NOTES
1. Fluids used for the anti-icing procedure must not be used at temperatures below their lowest operational use temperature (LOUT). First step fluids must not be used below their freezing points. Consideration should be given to the use of Type I/III fluid when Type II/IV fluid cannot be used due to LOUT limitations (see Table 59 and Table 61). The LOUT for a given Type II/IV fluid is the higher (warmer) of:
a) The lowest temperature at which the fluid meets the aerodynamic acceptance test for a given aircraft type; or
b) The actual freezing point of the fluid plus its freezing point buffer of 7 °C (13 °F).
Although some LOUTs are lower than the temperatures stated in the HOT table, holdover times do not apply when anti‑icing below the lowest temperature stated in the band.
To be applied before first step fluid freezes, typically within 3 minutes. Time may be longer than 3 minutes in some conditions, but potentially shorter in heavy precipitation, colder temperatures, or for critical surfaces constructed of composite materials. If necessary, the second step shall be applied area by area (sectionally). 
Clean aircraft may be anti-iced with unheated fluid.
CAUTIONS
For heated fluids, a fluid temperature not less than 60 °C (140 °F) at the nozzle is desirable.
Upper temperature limit shall not exceed fluid and aircraft manufacturers’ recommendations.
Wing skin temperatures may be colder or warmer than the OAT. Causes can include: radiation cooling, cold-soaked wing, or hangar storage. Consult the appropriate guidance (HOT Tables and FAA Ground Deicing General Information Document, Winter 2026-2027”) for the contaminant in question.
Whenever frost or ice occurs on the lower surface of the wing in the area of the fuel tank, indicating a cold-soaked wing, the 50/50 dilution of Type II or IV are not to be used for the anti-icing step because fluid freezing may occur.
An insufficient amount of anti-icing fluid may cause a substantial loss of holdover time. This is particularly true when using a Type I fluid mixture for the first step in a two-step procedure.
[bookmark: _TABLE_9-III-H._GUIDELINES]When conducting aircraft deicing using a Type I fluid and not using the 10 °C/18 °F buffer, procedures must be developed and approved to ensure refreezing does not occur prior to takeoff.


[bookmark: _TABLE_11-H._GUIDELINES][bookmark: _TABLE_9-III-U._GUIDELINES][bookmark: _Ref485906859][bookmark: _Toc508704851][bookmark: _Toc43986200][bookmark: _Toc234306107]Table 65: Guidelines for the Application of
Unheated SAE Type III Fluid 
(FLUID CONCENTRATIONS IN % VOLUME)
	Outside Air
Temperature
(OAT)1
	Anti-icing Only4
	Two-Step Procedure

	
	
	First Step: Deicing
	Second Step: Anti-icing2

	0 °C (32 °F) 
and above
	100/0, 75/25 or 50/50
Unheated Type III fluid/water mixture
	Heated3 water or a heated3 Type I, II, III, or IV 
fluid/water mixture
	100/0, 75/25 or 50/50
Unheated Type III 
fluid/water mixture

	Below 
0 °C (32 °F) to ‑3 °C (27 °F)
	100/0, 75/25 or 50/50
Unheated Type III fluid/water mixture
	Heated3 Type I, II, III, or IV fluid/water mixture with a freezing point at OAT or below
	100/0, 75/25 or 50/50
Unheated Type III 
fluid/water mixture

	Below 
-3 °C (27 °F) to ‑10 °C (14 °F)
	100/0 or 75/25
Unheated Type III fluid/water mixture
	Heated3 Type I, II, III, or IV fluid/water mixture with a freezing point at OAT or below
	100/0 or 75/25
Unheated Type III 
fluid/water mixture

	Below 
-10 °C (14 °F) 
	100/0
Unheated Type III fluid
	Heated3 Type I, II, III, or IV fluid/water mixture with a freezing point at OAT or below
	100/0
Unheated Type III fluid


NOTES
1. Fluids used for the anti-icing procedure must not be used at temperatures below their lowest operational use temperature (LOUT). First step fluids must not be used below their freezing points. Consider the use of Type I when Type III fluid cannot be used (see Table 60). The LOUT for a given Type III fluid is the higher (warmer) of: 
a) The lowest temperature at which the fluid meets the aerodynamic acceptance test for a given aircraft type; or
b) The actual freezing point of the fluid plus its freezing point buffer of 7 °C (13 °F).
Although the LOUTs may be lower than the temperatures stated in the HOT table, holdover times do not apply when anti‑icing below the lowest temperature stated in the band.
To be applied before first step fluid freezes, typically within 3 minutes. This time may be longer than 3 minutes in some conditions, but potentially shorter in heavy precipitation, colder temperatures, or for critical surfaces constructed of composite materials. If necessary, the second step shall be applied area by area (sectionally).
For heated fluids, a fluid temperature not less than 60 °C (140 °F) at the nozzle is desirable.
Anti-icing only with unheated Type III fluid is only possible on a clean aircraft. If deicing is required, a two-step procedure must be used.
CAUTIONS
Upper temperature limit shall not exceed fluid and aircraft manufacturers’ recommendations.
Wing skin temperatures may be colder or warmer than the OAT. Causes can include: radiation cooling, cold-soaked wing, or hangar storage. Consult the appropriate guidance (HOT Tables and FAA Ground Deicing General Information Document, Winter 2026-2027”) for the contaminant in question.
Whenever frost or ice occurs on the lower surface of the wing in the area of the fuel tank, indicating a cold-soaked wing, the 50/50 dilution of Type III is not to be used for the anti-icing step because fluid freezing may occur.
An insufficient amount of anti-icing fluid may cause a substantial loss of holdover time. This is particularly true when using a Type I fluid mixture for the first step in a two-step procedure.
When conducting aircraft deicing using a Type I fluid and not using the 10 °C/18 °F buffer, procedures must be developed and approved to ensure refreezing does not occur prior to takeoff.
FAA Holdover Time Guidelines	Winter 2026-2027

Original Issue	Page 62 of 91	August 11, 2026
[bookmark: _TABLE_0-90%._90][bookmark: _Toc508704852][bookmark: _Toc43986201][bookmark: _Toc234306108]Appendix A:
Adjusted Holdover Time (HOT) Guidelines

These tables are for use when flaps/slats are deployed prior to de/anti-icing. Holdover and allowance times have been adjusted to 76 percent of standard times. Standard holdover and allowance times can be used if flaps and slats are deployed as close to departure as safety allows.


Note: Industry data indicates the possibility of increased takeoff misconfigurations when the selection of takeoff flaps is delayed later in the taxi regime. If an air carrier chooses to select the flaps/slats to the takeoff configuration prior to beginning the anti-icing process, operators should have robust procedures in place to ensure that the aircraft is properly configured prior to takeoff. Air Carriers should follow the airframe manufacturer’s recommended procedures regarding anti-icing operations and the configuration of flaps/slats while taxiing.


Appendix A: FAA Adjusted Holdover Time Guidelines	Winter 2026-2027
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ADJUSTED HOLDOVER TIME (HOT) GUIDELINES
FOR WINTER 2026-2027
Adjusted Active Frost HOT Guidelines  Winter 2026-2027	A-4
Table Adj-1: Adjusted Active Frost Holdover Times for SAE Type I, Type II, Type III, and Type IV Fluids	A-5
Adjusted HOT Guidelines for SAE Type I Fluids Winter 2026-2027	A-6
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The HOT Guidelines are provided for information and guidance purposes. The HOT Guidelines on their own do not change, create, amend or permit deviations from regulatory requirements.

The HOT Guidelines may use mandatory terms such as “must”, “shall” and “is/are required” so as to convey the intent of meeting regulatory requirements and SAE Standards, where applicable. The term “should” is to be understood, unless an alternative method of achieving safety is implemented that would meet or exceed the intent of the recommendation.



[bookmark: ActiveFrostCautionsAdj]CAUTIONS
The responsibility for the application of these data remains with the user.
Fluids used during ground de/anti-icing do not provide in-flight icing protection.
This table is for departure planning only and should be used in conjunction with pre-takeoff check procedures.
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[bookmark: _Toc107305560][bookmark: _Toc231475370]Table Adj-1: Adjusted Active Frost Holdover Times
for SAE Type I, Type II, Type III, and Type IV Fluids1
	Outside Air 
Temperature2,3,4
	Type I Aluminum
	Type I Composite
	
	Outside Air 
Temperature3,4
	Concentration Fluid/Water
By % Volume
	Type II
	Type III5
	Type IV

	-1 °C and above
(30 °F and above)
	0:34
	0:27
	
	-1 °C and above
(30 °F and above)
	100/0
	6:05
	1:31
	9:07

	
	
	
	
	
	75/25
	3:48
	0:46
	3:48

	
	
	
	
	
	50/50
	1:31
	0:23
	2:17

	below -1 to -3 °C
(below 30 to 27 °F)
	
	
	
	below -1 to -3 °C
(below 30 to 27 °F)
	100/0
	6:05
	1:31
	9:07

	
	
	
	
	
	75/25
	3:48
	0:46
	3:48

	
	
	
	
	
	50/50
	1:08
	0:23
	2:17

	below -3 to -10 °C
(below 27 to 14 °F)
	
	
	
	below -3 to -10 °C
(below 27 to 14 °F)
	100/0
	6:05
	1:31
	7:36

	
	
	
	
	
	75/25
	3:02
	0:46
	3:48

	below -10 to -14 °C
(below 14 to 7 °F)
	
	
	
	below -10 to -14 °C
(below 14 to 7 °F)
	100/0
	4:34
	1:31
	4:34

	
	
	
	
	
	75/25
	0:46
	0:46
	0:46

	below -14 to -21 °C
(below 7 to -6 °F)
	
	
	
	below -14 to -21 °C
(below 7 to -6 °F)
	100/0
	2:17
	1:31
	4:34

	below -21 to -25 °C
(below -6 to -13 °F)
	
	
	
	below -21 to -25 °C
(below -6 to -13 °F)
	100/0
	1:31
	1:31
	3:02

	below -25 °C 
(below -13 °F)
	
	
	
	below -25 °C 
(below -13 °F)
	100/0
	No Holdover Time Guidelines Exist


THIS TABLE IS FOR USE WHEN FLAPS/SLATS ARE DEPLOYED PRIOR TO DE/ANTI-ICING. HOLDOVER TIMES HAVE BEEN ADJUSTED TO 76 PERCENT.
NOTES
To use the holdover times in this table, ensure that the fluid and dilution being used is listed in the List of Qualified Fluids Tested for Anti-Icing Performance and Aerodynamic Acceptance table (Table 58 - Table 61). Any restrictions on the use of the fluid have to be identified and applied.
Type I Fluid / Water Mixture must be selected so that the freezing point of the mixture is at least 10 °C (18 °F) below outside air temperature.
Ensure that the lowest operational use temperature (LOUT) is respected. 
Changes in outside air temperature (OAT) over the course of longer frost events can be significant; the appropriate holdover time to use is the one provided for the coldest OAT that has occurred in the time between the de/anti-icing fluid application and takeoff.
To use the Type III fluid frost holdover times, the fluid brand being used must be known. AllClear AeroClear MAX must be applied unheated. 
CAUTIONS
The cautions that apply to the holdover times in the table above can be found on page A-4.

Appendix A: FAA Adjusted Holdover Time Guidelines	Winter 2026-2027

Original Issue	Page A-3	August 11, 2026
[bookmark: _TABLE_1A-90%._90][bookmark: _Toc107305561][bookmark: _Toc231475371][bookmark: _Toc517088942][bookmark: _Toc517253599][bookmark: _Toc519674702][bookmark: _Toc519674809][bookmark: _Toc520288561][bookmark: _Toc520289433][bookmark: _Toc9500338][bookmark: _Toc14166548][bookmark: _Toc14867885][bookmark: _Toc43986203][bookmark: _Toc44053669][bookmark: _Toc44054088][bookmark: _Toc45715321][bookmark: _Toc75345453][bookmark: _Toc77777019][bookmark: _Toc77777069][bookmark: _Toc105048912][bookmark: _Toc105049266][bookmark: _Toc105049389][bookmark: _Toc105399206][bookmark: _Toc105399417]Adjusted HOT Guidelines for SAE Type I Fluids
Winter 2026-2027

The HOT Guidelines are provided for information and guidance purposes. The HOT Guidelines on their own do not change, create, amend or permit deviations from regulatory requirements.

The HOT Guidelines may use mandatory terms such as “must”, “shall” and “is/are required” so as to convey the intent of meeting regulatory requirements and SAE Standards, where applicable. The term “should” is to be understood, unless an alternative method of achieving safety is implemented that would meet or exceed the intent of the recommendation.



[bookmark: TypeICautionsAdj]CAUTIONS
The responsibility for the application of these data remains with the user.
The time of protection will be shortened in heavy weather conditions, heavy precipitation rates or high moisture content.
High wind velocity, jet blast or blowing snow may reduce holdover time below the lowest time stated in the range.
The holdover time may be reduced when aircraft skin temperature is lower than outside air temperature.
Fluids used during ground de/anti-icing do not provide in-flight icing protection.
This table is for departure planning only and should be used in conjunction with pre-takeoff check procedures.
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[bookmark: _Toc107305562][bookmark: _Toc231475372]Table Adj-2: Adjusted Holdover Times for SAE Type I Fluid on Critical Aircraft Surfaces Composed Predominantly of Aluminum1
	Outside Air 
Temperature2,3
	Freezing Fog, Freezing Mist4, or Ice Crystals5
	Snow 
mixed with 
Freezing Fog6
	Very Light Snow, Snow Grains or Snow Pellets6,7
	Light 
Snow, Snow Grains or Snow Pellets6,7
	Moderate Snow, Snow Grains or Snow Pellets6,7
	Freezing 
Drizzle8
	Light 
Freezing Rain
	Moderate Snow mixed with Rain9,10
	Rain on Cold‑Soaked Wing10
	Other11

	-3 °C and above
(27 °F and above)
	0:08 - 0:13
	0:05 - 0:08
	0:14 - 0:17
	0:08 - 0:14
	0:05 - 0:08
	0:07 - 0:10
	0:02 - 0:04
	0:02 - 0:02
	0:02 - 0:04
	 

	below -3 to -6 °C
(below 27 to 21 °F)
	0:06 - 0:10
	0:04 - 0:06
	0:11 - 0:13
	0:06 - 0:11
	0:04 - 0:06
	0:04 - 0:07
	0:02 - 0:04
	CAUTION: 
No holdover time 
guidelines exist

	below -6 to -10 °C
(below 21 to 14 °F)
	0:05 - 0:08
	0:03 - 0:05
	0:08 - 0:10
	0:05 - 0:08
	0:03 - 0:05
	0:03 - 0:05
	0:02 - 0:04
	

	below -10 °C
(below 14 °F)
	0:04 - 0:07
	0:02 - 0:03
	0:05 - 0:06
	0:03 - 0:05
	0:02 - 0:03
	 
	 
	


THIS TABLE IS FOR USE WHEN FLAPS/SLATS ARE DEPLOYED PRIOR TO DE/ANTI-ICING. HOLDOVER TIMES HAVE BEEN ADJUSTED TO 76 PERCENT.
NOTES
1. To use the holdover times in this table, ensure that the fluid and dilution being used is listed in the Type I Fluids Tested for Anti-Icing Performance and Aerodynamic Acceptance table (Table 58). Any restrictions on the use of the fluid have to be identified and applied.
178 Type I fluid / water mixture must be selected so that the freezing point of the mixture is at least 10 °C (18 °F) below outside air temperature.
Ensure that the lowest operational use temperature (LOUT) is respected.
Freezing mist is best confirmed by observation. It is never reported by METAR; however, it can occur when mist is present at 0 °C (32 °F) and below. 
Use freezing fog holdover times in conditions of ice crystals mixed with freezing fog or freezing mist.
To determine snowfall intensity, the Snowfall Intensities as a Function of Prevailing Visibility table (Table 57) is required. No holdover times exist if the reported visibility correlates to a “heavy” precipitation intensity. .
Use snow holdover times in conditions of very light, light, or moderate snow mixed with ice crystals.
Includes light, moderate and heavy freezing drizzle. Use light freezing rain holdover times if positive identification of freezing drizzle is not possible.
These holdover times apply to conditions of “moderate” precipitation intensity. In cases of very light or light snow mixed with light rain or drizzle, use light freezing rain holdover times. The Snowfall Intensities as a Function of Prevailing Visibility table (Table 57) is required to confirm the precipitation intensity. No holdover times exist if the reported visibility correlates to a “heavy” precipitation intensity.
No holdover time guidelines exist for this condition for 0 °C (32 °F) and below.
Heavy snow, ice pellets, moderate and heavy freezing rain, small hail and hail.
CAUTIONS
The cautions that apply to the holdover times in the table above can be found on page A-6.
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	Outside Air 
Temperature2,3
	Freezing Fog, Freezing Mist4, or Ice Crystals5
	Snow 
mixed with 
Freezing Fog6
	Very Light Snow, Snow Grains or Snow Pellets6,7
	Light 
Snow, Snow Grains or Snow Pellets6,7
	Moderate Snow, Snow Grains or Snow Pellets6,7
	Freezing 
Drizzle8
	Light 
Freezing Rain
	Moderate Snow mixed with Rain9,10
	Rain on Cold‑Soaked Wing10
	Other11

	-3 °C and above
(27 °F and above)
	0:07 - 0:12
	0:02 - 0:05
	0:09 - 0:11
	0:05 - 0:09
	0:02 - 0:05
	0:06 - 0:10
	0:02 - 0:04
	0:01 - 0:01
	0:01 - 0:04
	 

	below -3 to -6 °C
(below 27 to 21 °F)
	0:05 - 0:06
	0:02 - 0:04
	0:08 - 0:10
	0:04 - 0:08
	0:02 - 0:04
	0:04 - 0:07
	0:02 - 0:04
	CAUTION: 
No holdover time 
guidelines exist

	below -6 to -10 °C
(below 21 to 14 °F)
	0:03 - 0:06
	0:02 - 0:04
	0:07 - 0:09
	0:04 - 0:07
	0:02 - 0:04
	0:03 - 0:05
	0:02 - 0:04
	

	below -10 °C
(below 14 °F)
	0:03 - 0:05
	0:02 - 0:03
	0:05 - 0:06
	0:03 - 0:05
	0:02 - 0:03
	 
	 
	


THIS TABLE IS FOR USE WHEN FLAPS/SLATS ARE DEPLOYED PRIOR TO DE/ANTI-ICING. HOLDOVER TIMES HAVE BEEN ADJUSTED TO 76 PERCENT.
NOTES
1. To use the holdover times in this table, ensure that the fluid and dilution being used is listed in the Type I Fluids Tested for Anti-Icing Performance and Aerodynamic Acceptance table (Table 58). Any restrictions on the use of the fluid have to be identified and applied.
180 Type I fluid / water mixture must be selected so that the freezing point of the mixture is at least 10 °C (18 °F) below outside air temperature.
Ensure that the lowest operational use temperature (LOUT) is respected.
Freezing mist is best confirmed by observation. It is never reported by METAR; however, it can occur when mist is present at 0 °C (32 °F) and below. 
Use freezing fog holdover times in conditions of ice crystals mixed with freezing fog or freezing mist.
To determine snowfall intensity, the Snowfall Intensities as a Function of Prevailing Visibility table (Table 57) is required. No holdover times exist if the reported visibility correlates to a “heavy” precipitation intensity. 
Use snow holdover times in conditions of very light, light, or moderate snow mixed with ice crystals.
Includes light, moderate and heavy freezing drizzle. Use light freezing rain holdover times if positive identification of freezing drizzle is not possible.
These holdover times apply to conditions of “moderate” precipitation intensity. In cases of very light or light snow mixed with light rain or drizzle, use light freezing rain holdover times. The Snowfall Intensities as a Function of Prevailing Visibility table (Table 57) is required to confirm the precipitation intensity. No holdover times exist if the reported visibility correlates to a “heavy” precipitation intensity.
No holdover time guidelines exist for this condition for 0 °C (32 °F) and below.
Heavy snow, ice pellets, moderate and heavy freezing rain, small hail and hail.
CAUTIONS
The cautions that apply to the holdover times in the table above can be found on page A-6.
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The HOT Guidelines are provided for information and guidance purposes. The HOT Guidelines on their own do not change, create, amend or permit deviations from regulatory requirements.

The HOT Guidelines may use mandatory terms such as “must”, “shall” and “is/are required” so as to convey the intent of meeting regulatory requirements and SAE Standards, where applicable. The term “should” is to be understood, unless an alternative method of achieving safety is implemented that would meet or exceed the intent of the recommendation.



[bookmark: TypeIICautionsAdj]CAUTIONS
The responsibility for the application of these data remains with the user.
The time of protection will be shortened in heavy weather conditions, heavy precipitation rates or high moisture content.
High wind velocity, jet blast or blowing snow may reduce holdover time below the lowest time stated in the range.
The holdover time may be reduced when aircraft skin temperature is lower than outside air temperature.
Fluids used during ground de/anti-icing do not provide in-flight icing protection.
This table is for departure planning only and should be used in conjunction with pre-takeoff check procedures.
Whenever frost or ice occurs on the lower surface of the wing in the area of the fuel tank, indicating a cold-soaked wing, the 50/50 dilution of Type II or IV are not to be used for the anti-icing step because fluid freezing may occur.
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[bookmark: _Toc107305565][bookmark: _Toc231475375]Table Adj-4: Adjusted Generic Holdover Times for SAE Type II Fluids1
	Outside Air 
Temperature2
	Fluid 
Concentration 
Fluid/Water 
By % Volume
	Freezing Fog, Freezing Mist3, 
or Ice Crystals4
	Snow 
mixed with 
Freezing Fog5
	Snow, 
Snow Grains or Snow Pellets5,6
	Freezing 
Drizzle7
	Light 
Freezing Rain
	Moderate
Snow mixed with Rain8,9
	Rain on Cold‑Soaked Wing9
	Other10

	-3 °C and above
(27 °F and above)
	100/0
	0:42 - 1:24
	0:15 - 0:30
	0:23 - 0:42
	0:27 - 0:49
	0:19 - 0:27
	0:04 - 0:04
	0:05 - 0:34
	 

	
	75/25
	0:30 - 0:53
	0:11 - 0:19
	0:11 - 0:23
	0:19 - 0:30
	0:11 - 0:19
	0:02 - 0:02
	0:03 - 0:19
	 

	
	50/50
	0:11 - 0:23
	0:04 - 0:08
	0:05 - 0:11
	0:07 - 0:11
	0:05 - 0:07
	CAUTION: 
No holdover time 
guidelines exist

	below -3 to -8 °C
(below 27 to 18 °F)
	100/0
	0:23 - 0:34
	0:11 - 0:23
	0:15 - 0:30
	0:15 - 0:34
	0:11 - 0:15
	

	
	75/25
	0:19 - 0:42
	0:07 - 0:11
	0:08 - 0:19
	0:11 - 0:23
	0:07 - 0:15
	

	below -8 to -14 °C
(below 18 to 7 °F)
	100/0
	0:23 - 0:34
	0:08 - 0:19
	0:11 - 0:23
	0:15 - 0:3411
	0:11 - 0:1511
	

	
	75/25
	0:19 - 0:42
	0:05 - 0:11
	0:07 - 0:15
	0:11 - 0:2311
	0:07 - 0:1511
	

	below -14 to -18 °C
(below 7 to 0 °F)
	100/0
	0:11 - 0:15
	0:01 - 0:04
	0:02 - 0:05
	 
	

	below -18 to -25 °C
(below 0 to -13 °F)
	100/0
	0:11 - 0:15
	0:00 - 0:02
	0:01 - 0:02
	 
	 
	

	below -25 °C 
(below -13 °F)
	100/0
	0:11 - 0:15
	0:00 - 0:00
	0:00 - 0:01
	 
	


THIS TABLE IS FOR USE WHEN FLAPS/SLATS ARE DEPLOYED PRIOR TO DE/ANTI-ICING. HOLDOVER TIMES HAVE BEEN ADJUSTED TO 76 PERCENT.
NOTES
1. To use the holdover times in this table, ensure that the fluid and dilution being used is listed in the Type II Fluids Tested for Anti-Icing Performance and Aerodynamic Acceptance table (Table 59). Any restrictions on the use of the fluid have to be identified and applied.
1. Ensure that the lowest operational use temperature (LOUT) is respected. Consider use of Type I fluid when Type II fluid cannot be used.
1. Freezing mist is best confirmed by observation. It is never reported by METAR; however, it can occur when mist is present at 0 °C (32 °F) and below. 
1. Use freezing fog holdover times in conditions of ice crystals mixed with freezing fog or freezing mist.
1. To determine snowfall intensity, the Snowfall Intensities as a Function of Prevailing Visibility table (Table 57) is required. No holdover times exist if the reported visibility correlates to a “heavy” precipitation intensity. 
Use snow holdover times in conditions of very light, light, or moderate snow mixed with ice crystals.
Includes light, moderate and heavy freezing drizzle. Use light freezing rain holdover times if positive identification of freezing drizzle is not possible.
These holdover times apply to conditions of “moderate” precipitation intensity. In cases of very light or light snow mixed with light rain or drizzle, use light freezing rain holdover times. The Snowfall Intensities as a Function of Prevailing Visibility table (Table 57) is required to confirm the precipitation intensity. No holdover times exist if the reported visibility correlates to a “heavy” precipitation intensity.
No holdover time guidelines exist for this condition for 0 °C (32 °F) and below.
Heavy snow, ice pellets, moderate and heavy freezing rain, small hail and hail.
No holdover time guidelines exist for this condition below -10 °C (14 °F).
CAUTIONS
The cautions that apply to the holdover times in the table above can be found on page A-9.

[bookmark: _Toc517088946][bookmark: _Toc517253603][bookmark: _Toc519674706][bookmark: _Toc519674813][bookmark: _Toc520288565][bookmark: _Toc520289437][bookmark: _Toc9500342][bookmark: _Toc14166552][bookmark: _Toc14867889][bookmark: _Toc43986206][bookmark: _Toc44053672][bookmark: _Toc44054091][bookmark: _Toc45715324][bookmark: _Toc75345456][bookmark: _Toc77777022][bookmark: _Toc77777072][bookmark: _Toc105048915][bookmark: _Toc105049269][bookmark: _Toc105049392][bookmark: _Toc105399209][bookmark: _Toc105399420][bookmark: _Toc107305566][bookmark: _Toc231475376]Table Adj-5: Adjusted Type II Holdover Times for
ABAX ECOWING AD-2
	Outside Air 
Temperature1
	Fluid 
Concentration 
Fluid/Water 
By % Volume
	Freezing Fog, Freezing Mist2, or Ice Crystals3
	Snow 
mixed with 
Freezing Fog4
	Very Light Snow, Snow Grains or Snow Pellets4,5
	Light 
Snow, Snow Grains or Snow Pellets4,5
	Moderate Snow, Snow Grains or Snow Pellets4,5
	Freezing 
Drizzle6
	Light 
Freezing Rain
	Moderate
Snow mixed with Rain7,8
	Rain on 
Cold‑Soaked Wing8
	Other9

	-3 °C and above
(27 °F and above)
	100/0
	1:01 - 2:17
	0:23 - 0:42
	1:50 - 2:13
	0:57 - 1:50
	0:30 - 0:57
	0:30 - 1:16
	0:23 - 0:34
	0:05 - 0:05
	0:07 - 1:05
	 

	
	75/25
	0:57 - 1:05
	0:15 - 0:30
	1:20 - 1:39
	0:42 - 1:20
	0:19 - 0:42
	0:27 - 0:49
	0:15 - 0:23
	0:02 - 0:02
	0:03 - 0:38
	 

	
	50/50
	0:11 - 0:23
	0:04 - 0:08
	0:27 - 0:30
	0:11 - 0:27
	0:05 - 0:11
	0:07 - 0:11
	0:05 - 0:07
	CAUTION: 
No holdover time 
guidelines exist

	below -3 to -8 °C
(below 27 to 18 °F)
	100/0
	0:34 - 1:54
	0:19 - 0:34
	1:31 - 1:50
	0:46 - 1:31
	0:23 - 0:46
	0:19 - 0:53
	0:15 - 0:23
	

	
	75/25
	0:27 - 1:27
	0:15 - 0:27
	1:16 - 1:35
	0:38 - 1:16
	0:19 - 0:38
	0:11 - 0:42
	0:15 - 0:27
	

	below -8 to -14 °C
(below 18 to 7 °F)
	100/0
	0:34 - 1:54
	0:15 - 0:30
	1:20 - 1:35
	0:42 - 1:20
	0:23 - 0:42
	0:19 - 0:5310
	0:15 - 0:2310
	

	
	75/25
	0:27 - 1:27
	0:15 - 0:27
	1:12 - 1:31
	0:38 - 1:12
	0:19 - 0:38
	0:11 - 0:4210
	0:15 - 0:2710
	

	below -14 to -18 °C
(below 7 to 0 °F)
	100/0
	0:11 - 0:30
	0:01 - 0:04
	0:15 - 0:23
	0:05 - 0:15
	0:02 - 0:05
	
	

	below -18 to -25 °C
(below 0 to -13 °F)
	100/0
	0:11 - 0:30
	0:00 - 0:02
	0:07 - 0:11
	0:02 - 0:07
	0:01 - 0:02
	
	

	below -25 to -27 °C
(below -13 to -17 °F)
	100/0
	0:11 - 0:30
	0:00 - 0:00
	0:04 - 0:05
	0:01 - 0:04
	0:00 - 0:01
	
	


THIS TABLE IS FOR USE WHEN FLAPS/SLATS ARE DEPLOYED PRIOR TO DE/ANTI-ICING. HOLDOVER TIMES HAVE BEEN ADJUSTED TO 76 PERCENT.
NOTES
1. Ensure that the lowest operational use temperature (LOUT) is respected. Consider use of Type I fluid when Type II fluid cannot be used.
1. Freezing mist is best confirmed by observation. It is never reported by METAR; however, it can occur when mist is present at 0 °C (32 °F) and below. 
1. Use freezing fog holdover times in conditions of ice crystals mixed with freezing fog or freezing mist.
1. To determine snowfall intensity, the Snowfall Intensities as a Function of Prevailing Visibility table (Table 57) is required. No holdover times exist if the reported visibility correlates to a “heavy” precipitation intensity. 
Use snow holdover times in conditions of very light, light, or moderate snow mixed with ice crystals.
Includes light, moderate and heavy freezing drizzle. Use light freezing rain holdover times if positive identification of freezing drizzle is not possible.
These holdover times apply to conditions of “moderate” precipitation intensity. In cases of very light or light snow mixed with light rain or drizzle, use light freezing rain holdover times. The Snowfall Intensities as a Function of Prevailing Visibility table (Table 57) is required to confirm the precipitation intensity. No holdover times exist if the reported visibility correlates to a “heavy” precipitation intensity.
No holdover time guidelines exist for this condition for 0 °C (32 °F) and below.
Heavy snow, ice pellets, moderate and heavy freezing rain, small hail and hail.
No holdover time guidelines exist for this condition below -10 °C (14 °F).
CAUTIONS
The cautions that apply to the holdover times in the table above can be found on page A-9.
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Aviation Xi’an High-Tech Cleanwing II
	Outside Air 
Temperature1
	Fluid 
Concentration 
Fluid/Water 
By % Volume
	Freezing Fog, Freezing Mist2, or Ice Crystals3
	Snow 
mixed with 
Freezing Fog4
	Very Light Snow, Snow Grains or Snow Pellets4,5
	Light 
Snow, Snow Grains or Snow Pellets4,5
	Moderate Snow, Snow Grains or Snow Pellets4,5
	Freezing 
Drizzle6
	Light 
Freezing Rain
	Moderate
Snow mixed with Rain7,8
	Rain on 
Cold‑Soaked Wing8
	Other9

	-3 °C and above
(27 °F and above)
	100/0
	0:42 - 1:24
	0:15 - 0:30
	1:12 - 1:27
	0:42 - 1:12
	0:23 - 0:42
	0:27 - 0:49
	0:19 - 0:27
	0:05 - 0:05
	0:08 - 0:42
	 

	
	75/25
	0:38 - 1:01
	0:11 - 0:19
	0:49 - 0:57
	0:27 - 0:49
	0:15 - 0:27
	0:27 - 0:46
	0:15 - 0:23
	0:04 - 0:04
	0:05 - 0:38
	 

	
	50/50
	0:27 - 0:46
	0:08 - 0:15
	0:38 - 0:49
	0:19 - 0:38
	0:11 - 0:19
	0:15 - 0:30
	0:08 - 0:15
	CAUTION: 
No holdover time 
guidelines exist

	below -3 to -8 °C
(below 27 to 18 °F)
	100/0
	0:34 - 1:24
	0:11 - 0:23
	1:01 - 1:12
	0:30 - 1:01
	0:19 - 0:30
	0:23 - 0:42
	0:15 - 0:19
	

	
	75/25
	0:30 - 1:20
	0:11 - 0:19
	0:49 - 0:57
	0:27 - 0:49
	0:15 - 0:27
	0:27 - 0:30
	0:15 - 0:19
	

	below -8 to -14 °C
(below 18 to 7 °F)
	100/0
	0:34 - 1:24
	0:11 - 0:19
	0:49 - 1:01
	0:27 - 0:49
	0:15 - 0:27
	0:23 - 0:4210
	0:15 - 0:1910
	

	
	75/25
	0:30 - 1:20
	0:11 - 0:19
	0:49 - 0:57
	0:27 - 0:49
	0:15 - 0:27
	0:27 - 0:3010
	0:15 - 0:1910
	

	below -14 to -18 °C
(below 7 to 0 °F)
	100/0
	0:15 - 0:38
	0:07 - 0:15
	0:34 - 0:46
	0:19 - 0:34
	0:11 - 0:19
	
	

	below -18 to -25 °C
(below 0 to -13 °F)
	100/0
	0:15 - 0:38
	0:04 - 0:08
	0:23 - 0:27
	0:11 - 0:23
	0:05 - 0:11
	
	


THIS TABLE IS FOR USE WHEN FLAPS/SLATS ARE DEPLOYED PRIOR TO DE/ANTI-ICING. HOLDOVER TIMES HAVE BEEN ADJUSTED TO 76 PERCENT.
NOTES
1. Ensure that the lowest operational use temperature (LOUT) is respected. Consider use of Type I fluid when Type II fluid cannot be used.
1. Freezing mist is best confirmed by observation. It is never reported by METAR; however, it can occur when mist is present at 0 °C (32 °F) and below. 
1. Use freezing fog holdover times in conditions of ice crystals mixed with freezing fog or freezing mist.
1. To determine snowfall intensity, the Snowfall Intensities as a Function of Prevailing Visibility table (Table 57) is required. No holdover times exist if the reported visibility correlates to a “heavy” precipitation intensity. 
Use snow holdover times in conditions of very light, light, or moderate snow mixed with ice crystals.
Includes light, moderate and heavy freezing drizzle. Use light freezing rain holdover times if positive identification of freezing drizzle is not possible.
These holdover times apply to conditions of “moderate” precipitation intensity. In cases of very light or light snow mixed with light rain or drizzle, use light freezing rain holdover times. The Snowfall Intensities as a Function of Prevailing Visibility table (Table 57) is required to confirm the precipitation intensity. No holdover times exist if the reported visibility correlates to a “heavy” precipitation intensity.
No holdover time guidelines exist for this condition for 0 °C (32 °F) and below.
Heavy snow, ice pellets, moderate and heavy freezing rain, small hail and hail.
No holdover time guidelines exist for this condition below -10 °C (14 °F).
CAUTIONS
The cautions that apply to the holdover times in the table above can be found on page A-9.
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Clariant Safewing MP II FLIGHT
	Outside Air 
Temperature1
	Fluid 
Concentration 
Fluid/Water 
By % Volume
	Freezing Fog, Freezing Mist2, or Ice Crystals3
	Snow 
mixed with 
Freezing Fog4
	Very Light Snow, Snow Grains or Snow Pellets4,5
	Light 
Snow, Snow Grains or Snow Pellets4,5
	Moderate Snow, Snow Grains or Snow Pellets4,5
	Freezing 
Drizzle6
	Light 
Freezing Rain
	Moderate
Snow mixed with Rain7,8
	Rain on 
Cold‑Soaked Wing8
	Other9

	-3 °C and above
(27 °F and above)
	100/0
	2:40 - 3:02
	0:34 - 0:53
	1:58 - 2:21
	1:12 - 1:58
	0:46 - 1:12
	1:01 - 1:31
	0:34 - 1:05
	0:06 - 0:06
	0:08 - 1:08
	 

	
	75/25
	1:24 - 2:05
	0:23 - 0:46
	1:58 - 2:24
	1:01 - 1:58
	0:30 - 1:01
	0:53 - 1:08
	0:23 - 0:42
	0:03 - 0:03
	0:05 - 0:38
	 

	
	50/50
	0:42 - 1:20
	0:07 - 0:15
	0:34 - 0:42
	0:19 - 0:34
	0:08 - 0:19
	0:15 - 0:23
	0:08 - 0:11
	CAUTION: 
No holdover time 
guidelines exist

	below -3 to -8 °C
(below 27 to 18 °F)
	100/0
	0:42 - 1:20
	0:27 - 0:46
	1:35 - 1:54
	0:57 - 1:35
	0:34 - 0:57
	0:27 - 1:08
	0:19 - 0:34
	

	
	75/25
	0:19 - 0:49
	0:15 - 0:30
	1:20 - 1:39
	0:42 - 1:20
	0:23 - 0:42
	0:19 - 0:53
	0:15 - 0:27
	

	below -8 to -14 °C
(below 18 to 7 °F)
	100/0
	0:42 - 1:20
	0:23 - 0:38
	1:24 - 1:39
	0:49 - 1:24
	0:30 - 0:49
	0:27 - 1:0810
	0:19 - 0:3410
	

	
	75/25
	0:19 - 0:49
	0:11 - 0:23
	1:01 - 1:16
	0:30 - 1:01
	0:15 - 0:30
	0:19 - 0:5310
	0:15 - 0:2710
	

	below -14 to -18 °C
(below 7 to 0 °F)
	100/0
	0:23 - 0:38
	0:05 - 0:15
	0:53 - 1:16
	0:19 - 0:53
	0:06 - 0:19
	
	

	below -18 to -25 °C
(below 0 to -13 °F)
	100/0
	0:23 - 0:38
	0:02 - 0:05
	0:23 - 0:30
	0:08 - 0:23
	0:02 - 0:08
	
	

	below -25 to -29 °C
(below -13 to -20 °F)
	100/0
	0:23 - 0:38
	0:01 - 0:04
	0:15 - 0:23
	0:05 - 0:15
	0:02 - 0:05
	
	


THIS TABLE IS FOR USE WHEN FLAPS/SLATS ARE DEPLOYED PRIOR TO DE/ANTI-ICING. HOLDOVER TIMES HAVE BEEN ADJUSTED TO 76 PERCENT.
NOTES
1. Ensure that the lowest operational use temperature (LOUT) is respected. Consider use of Type I fluid when Type II fluid cannot be used.
1. Freezing mist is best confirmed by observation. It is never reported by METAR; however, it can occur when mist is present at 0 °C (32 °F) and below. 
1. Use freezing fog holdover times in conditions of ice crystals mixed with freezing fog or freezing mist.
1. To determine snowfall intensity, the Snowfall Intensities as a Function of Prevailing Visibility table (Table 57) is required. No holdover times exist if the reported visibility correlates to a “heavy” precipitation intensity. 
Use snow holdover times in conditions of very light, light, or moderate snow mixed with ice crystals.
Includes light, moderate and heavy freezing drizzle. Use light freezing rain holdover times if positive identification of freezing drizzle is not possible.
These holdover times apply to conditions of “moderate” precipitation intensity. In cases of very light or light snow mixed with light rain or drizzle, use light freezing rain holdover times. The Snowfall Intensities as a Function of Prevailing Visibility table (Table 57) is required to confirm the precipitation intensity. No holdover times exist if the reported visibility correlates to a “heavy” precipitation intensity.
No holdover time guidelines exist for this condition for 0 °C (32 °F) and below.
Heavy snow, ice pellets, moderate and heavy freezing rain, small hail and hail.
No holdover time guidelines exist for this condition below -10 °C (14 °F).
CAUTIONS
The cautions that apply to the holdover times in the table above can be found on page A-9.
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Cryotech Polar Guard® II
	Outside Air 
Temperature1
	Fluid 
Concentration 
Fluid/Water 
By % Volume
	Freezing Fog, Freezing Mist2, or Ice Crystals3
	Snow 
mixed with 
Freezing Fog4
	Very Light Snow, Snow Grains or Snow Pellets4,5
	Light 
Snow, Snow Grains or Snow Pellets4,5
	Moderate Snow, Snow Grains or Snow Pellets4,5
	Freezing 
Drizzle6
	Light 
Freezing Rain
	Moderate
Snow mixed with Rain7,8
	Rain on 
Cold‑Soaked Wing8
	Other9

	-3 °C and above
(27 °F and above)
	100/0
	2:09 - 3:02
	0:38 - 1:05
	2:28 - 2:59
	1:27 - 2:28
	0:49 - 1:27
	1:12 - 1:31
	0:57 - 1:08
	0:08 - 0:08
	0:11 - 1:31
	 

	
	75/25
	1:54 - 3:02
	0:23 - 0:49
	2:17 - 2:55
	1:05 - 2:17
	0:30 - 1:05
	1:16 - 1:31
	0:30 - 0:53
	0:05 - 0:05
	0:07 - 1:16
	 

	
	50/50
	0:38 - 1:05
	0:05 - 0:15
	0:53 - 1:12
	0:19 - 0:53
	0:08 - 0:19
	0:15 - 0:34
	0:07 - 0:15
	CAUTION: 
No holdover time 
guidelines exist

	below -3 to -8 °C
(below 27 to 18 °F)
	100/0
	0:42 - 1:54
	0:27 - 0:49
	1:50 - 2:09
	1:05 - 1:50
	0:38 - 1:05
	0:27 - 1:12
	0:27 - 0:34
	

	
	75/25
	0:30 - 1:08
	0:19 - 0:38
	1:46 - 2:17
	0:49 - 1:46
	0:23 - 0:49
	0:19 - 0:49
	0:27 - 0:34
	

	below -8 to -14 °C
(below 18 to 7 °F)
	100/0
	0:42 - 1:54
	0:23 - 0:38
	1:31 - 1:46
	0:53 - 1:31
	0:30 - 0:53
	0:27 - 1:1210
	0:27 - 0:3410
	

	
	75/25
	0:30 - 1:08
	0:15 - 0:34
	1:31 - 1:54
	0:42 - 1:31
	0:19 - 0:42
	0:19 - 0:4910
	0:27 - 0:3410
	

	below -14 to -18 °C
(below 7 to 0 °F)
	100/0
	0:19 - 0:38
	0:06 - 0:19
	1:12 - 1:43
	0:27 - 1:12
	0:08 - 0:27
	
	

	below -18 to -25 °C
(below 0 to -13 °F)
	100/0
	0:19 - 0:38
	0:02 - 0:08
	0:30 - 0:42
	0:11 - 0:30
	0:03 - 0:11
	
	

	below -25 to -30.5 °C
(below -13 to -23 °F)
	100/0
	0:19 - 0:38
	0:02 - 0:04
	0:19 - 0:23
	0:05 - 0:19
	0:02 - 0:05
	
	


THIS TABLE IS FOR USE WHEN FLAPS/SLATS ARE DEPLOYED PRIOR TO DE/ANTI-ICING. HOLDOVER TIMES HAVE BEEN ADJUSTED TO 76 PERCENT.
NOTES
1. Ensure that the lowest operational use temperature (LOUT) is respected. Consider use of Type I fluid when Type II fluid cannot be used.
1. Freezing mist is best confirmed by observation. It is never reported by METAR; however, it can occur when mist is present at 0 °C (32 °F) and below. 
1. Use freezing fog holdover times in conditions of ice crystals mixed with freezing fog or freezing mist.
1. To determine snowfall intensity, the Snowfall Intensities as a Function of Prevailing Visibility table (Table 57) is required. No holdover times exist if the reported visibility correlates to a “heavy” precipitation intensity. 
Use snow holdover times in conditions of very light, light, or moderate snow mixed with ice crystals.
Includes light, moderate and heavy freezing drizzle. Use light freezing rain holdover times if positive identification of freezing drizzle is not possible.
These holdover times apply to conditions of “moderate” precipitation intensity. In cases of very light or light snow mixed with light rain or drizzle, use light freezing rain holdover times. The Snowfall Intensities as a Function of Prevailing Visibility table (Table 57) is required to confirm the precipitation intensity. No holdover times exist if the reported visibility correlates to a “heavy” precipitation intensity.
No holdover time guidelines exist for this condition for 0 °C (32 °F) and below.
Heavy snow, ice pellets, moderate and heavy freezing rain, small hail and hail.
No holdover time guidelines exist for this condition below -10 °C (14 °F).
CAUTIONS
The cautions that apply to the holdover times in the table above can be found on page A-9.

[bookmark: _Toc231475380]Table Adj-9: Adjusted Type II Holdover Times for
ESSPO CHEMICALS D.O.O Nordwing PG2
	Outside Air 
Temperature1
	Fluid 
Concentration 
Fluid/Water 
By % Volume
	Freezing Fog, Freezing Mist2, or Ice Crystals3
	Snow 
mixed with 
Freezing Fog4
	Very Light Snow, Snow Grains or Snow Pellets4,5
	Light 
Snow, Snow Grains or Snow Pellets4,5
	Moderate Snow, Snow Grains or Snow Pellets4,5
	Freezing 
Drizzle6
	Light 
Freezing Rain
	Moderate
Snow mixed with Rain7,8
	Rain on 
Cold‑Soaked Wing8
	Other9

	-3 °C and above
(27 °F and above)
	100/0
	1:16 - 2:24
	0:23 - 0:46
	1:58 - 2:28
	1:01 - 1:58
	0:30 - 1:01
	0:49 - 1:24
	0:38 - 0:49
	0:11 - 0:11
	0:15 - 1:20
	 

	
	75/25
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	 

	
	50/50
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	CAUTION: 
No holdover time 
guidelines exist

	below -3 to -8 °C
(below 27 to 18 °F)
	100/0
	0:49 - 1:46
	0:19 - 0:34
	1:31 - 1:54
	0:46 - 1:31
	0:23 - 0:46
	0:38 - 1:08
	0:19 - 0:38
	

	
	75/25
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	

	below -8 to -14 °C
(below 18 to 7 °F)
	100/0
	0:49 - 1:46
	0:15 - 0:30
	1:20 - 1:39
	0:38 - 1:20
	0:19 - 0:38
	0:38 - 1:0810
	0:19 - 0:3810
	

	
	75/25
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	

	below -14 to -18 °C
(below 7 to 0 °F)
	100/0
	0:15 - 0:27
	0:08 - 0:19
	0:57 - 1:16
	0:23 - 0:57
	0:11 - 0:23
	
	

	below -18 to -25 °C
(below 0 to -13 °F)
	100/0
	0:15 - 0:27
	0:05 - 0:11
	0:38 - 0:49
	0:15 - 0:38
	0:06 - 0:15
	
	

	below -25 to -30 °C
(below -13 to -22 °F)
	100/0
	0:15 - 0:23
	0:02 - 0:05
	0:19 - 0:23
	0:07 - 0:19
	0:03 - 0:07
	
	


THIS TABLE IS FOR USE WHEN FLAPS/SLATS ARE DEPLOYED PRIOR TO DE/ANTI-ICING. HOLDOVER TIMES HAVE BEEN ADJUSTED TO 76 PERCENT.
NOTES
1. Ensure that the lowest operational use temperature (LOUT) is respected. Consider use of Type I fluid when Type II fluid cannot be used.
1. Freezing mist is best confirmed by observation. It is never reported by METAR; however, it can occur when mist is present at 0 °C (32 °F) and below. 
1. Use freezing fog holdover times in conditions of ice crystals mixed with freezing fog or freezing mist.
1. To determine snowfall intensity, the Snowfall Intensities as a Function of Prevailing Visibility table (Table 57) is required. No holdover times exist if the reported visibility correlates to a “heavy” precipitation intensity. 
Use snow holdover times in conditions of very light, light, or moderate snow mixed with ice crystals.
Includes light, moderate and heavy freezing drizzle. Use light freezing rain holdover times if positive identification of freezing drizzle is not possible.
These holdover times apply to conditions of “moderate” precipitation intensity. In cases of very light or light snow mixed with light rain or drizzle, use light freezing rain holdover times. The Snowfall Intensities as a Function of Prevailing Visibility table (Table 57) is required to confirm the precipitation intensity. No holdover times exist if the reported visibility correlates to a “heavy” precipitation intensity.
No holdover time guidelines exist for this condition for 0 °C (32 °F) and below.
Heavy snow, ice pellets, moderate and heavy freezing rain, small hail and hail.
No holdover time guidelines exist for this condition below -10 °C (14 °F).
CAUTIONS
The cautions that apply to the holdover times in the table above can be found on page A-9.

[bookmark: _Toc436349469][bookmark: _Toc517088952][bookmark: _Toc517253609][bookmark: _Toc519674712][bookmark: _Toc519674819][bookmark: _Toc520288571][bookmark: _Toc520289443][bookmark: _Toc9500348][bookmark: _Toc14166558][bookmark: _Toc14867895][bookmark: _Toc43986213][bookmark: _Toc44053679][bookmark: _Toc44054098][bookmark: _Toc45715331][bookmark: _Toc75345463][bookmark: _Toc77777029][bookmark: _Toc77777079][bookmark: _Toc105048921][bookmark: _Toc105049275][bookmark: _Toc105049398][bookmark: _Toc105399215][bookmark: _Toc105399426][bookmark: _Toc107305572][bookmark: _Toc231475381]Table Adj-10: Adjusted Type II Holdover Times for
Kilfrost ABC-K Plus
	Outside Air 
Temperature1
	Fluid 
Concentration 
Fluid/Water 
By % Volume
	Freezing Fog, Freezing Mist2, 
or Ice Crystals3
	Snow 
mixed with 
Freezing Fog4
	Snow, 
Snow Grains or Snow Pellets4,5
	Freezing 
Drizzle6
	Light 
Freezing Rain
	Moderate
Snow mixed with Rain7,8
	Rain on Cold‑Soaked Wing8
	Other9

	-3 °C and above
(27 °F and above)
	100/0
	1:43 - 2:51
	0:34 - 0:57
	0:46 - 1:16
	1:24 - 1:31
	0:46 - 1:05
	0:11 - 0:11
	0:15 - 1:31
	 

	
	75/25
	1:16 - 1:54
	0:19 - 0:34
	0:23 - 0:46
	1:05 - 1:31
	0:38 - 0:53
	0:08 - 0:08
	0:11 - 1:31
	 

	
	50/50
	0:27 - 0:49
	0:04 - 0:08
	0:05 - 0:11
	0:15 - 0:23
	0:08 - 0:11
	CAUTION: 
No holdover time 
guidelines exist

	below -3 to -8 °C
(below 27 to 18 °F)
	100/0
	0:23 - 0:49
	0:30 - 0:53
	0:42 - 1:08
	0:19 - 0:46
	0:11 - 0:27
	

	
	75/25
	0:19 - 1:05
	0:19 - 0:34
	0:23 - 0:46
	0:15 - 0:42
	0:07 - 0:23
	

	below -8 to -14 °C
(below 18 to 7 °F)
	100/0
	0:23 - 0:49
	0:30 - 0:49
	0:38 - 1:05
	0:19 - 0:4610
	0:11 - 0:2710
	

	
	75/25
	0:19 - 1:05
	0:19 - 0:34
	0:23 - 0:46
	0:15 - 0:4210
	0:07 - 0:2310
	

	below -14 to -18 °C
(below 7 to 0 °F)
	100/0
	0:23 - 0:42
	0:01 - 0:04
	0:02 - 0:05
	 
	

	below -18 to -25 °C
(below 0 to -13 °F)
	100/0
	0:23 - 0:42
	0:00 - 0:02
	0:01 - 0:02
	 
	 
	

	below -25 to -29 °C
(below -13 to -20 °F)
	100/0
	0:23 - 0:42
	0:00 - 0:00
	0:00 - 0:01
	 
	


THIS TABLE IS FOR USE WHEN FLAPS/SLATS ARE DEPLOYED PRIOR TO DE/ANTI-ICING. HOLDOVER TIMES HAVE BEEN ADJUSTED TO 76 PERCENT.
NOTES
1. Ensure that the lowest operational use temperature (LOUT) is respected. Consider use of Type I fluid when Type II fluid cannot be used.
1. Freezing mist is best confirmed by observation. It is never reported by METAR; however, it can occur when mist is present at 0 °C (32 °F) and below. 
1. Use freezing fog holdover times in conditions of ice crystals mixed with freezing fog or freezing mist.
1. To determine snowfall intensity, the Snowfall Intensities as a Function of Prevailing Visibility table (Table 57) is required. No holdover times exist if the reported visibility correlates to a “heavy” precipitation intensity. 
Use snow holdover times in conditions of very light, light, or moderate snow mixed with ice crystals.
Includes light, moderate and heavy freezing drizzle. Use light freezing rain holdover times if positive identification of freezing drizzle is not possible.
These holdover times apply to conditions of “moderate” precipitation intensity. In cases of very light or light snow mixed with light rain or drizzle, use light freezing rain holdover times. The Snowfall Intensities as a Function of Prevailing Visibility table (Table 57) is required to confirm the precipitation intensity. No holdover times exist if the reported visibility correlates to a “heavy” precipitation intensity.
No holdover time guidelines exist for this condition for 0 °C (32 °F) and below.
Heavy snow, ice pellets, moderate and heavy freezing rain, small hail and hail.
No holdover time guidelines exist for this condition below -10 °C (14 °F).
CAUTIONS
The cautions that apply to the holdover times in the table above can be found on page A-9.

[bookmark: _Toc107305573][bookmark: _Toc231475382][bookmark: _Toc436349471][bookmark: _Toc517088954][bookmark: _Toc517253611][bookmark: _Toc519674714][bookmark: _Toc519674821][bookmark: _Toc520288573][bookmark: _Toc520289445][bookmark: _Toc9500350][bookmark: _Toc14166560][bookmark: _Toc14867897][bookmark: _Toc43986215][bookmark: _Toc44053681][bookmark: _Toc44054100][bookmark: _Toc45715333][bookmark: _Toc75345464][bookmark: _Toc77777030][bookmark: _Toc77777080][bookmark: _Toc105048922][bookmark: _Toc105049276][bookmark: _Toc105049399][bookmark: _Toc105399216][bookmark: _Toc105399427]Table Adj-11: Adjusted Type II Holdover Times for
Kilfrost Ice Clear II
	Outside Air 
Temperature1
	Fluid 
Concentration 
Fluid/Water 
By % Volume
	Freezing Fog, Freezing Mist2, or Ice Crystals3
	Snow 
mixed with 
Freezing Fog4
	Very Light Snow, Snow Grains or Snow Pellets4,5
	Light 
Snow, Snow Grains or Snow Pellets4,5
	Moderate Snow, Snow Grains or Snow Pellets4,5
	Freezing 
Drizzle6
	Light 
Freezing Rain
	Moderate
Snow mixed with Rain7,8
	Rain on 
Cold‑Soaked Wing8
	Other9

	-3 °C and above
(27 °F and above)
	100/0
	1:05 - 1:50
	0:23 - 0:46
	1:50 - 2:13
	1:01 - 1:50
	0:30 - 1:01
	0:46 - 1:12
	0:30 - 0:49
	0:08 - 0:08
	0:11 - 1:31
	 

	
	75/25
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	 

	
	50/50
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	CAUTION: 
No holdover time 
guidelines exist

	below -3 to -8 °C
(below 27 to 18 °F)
	100/0
	0:49 - 1:58
	0:23 - 0:38
	1:39 - 1:58
	0:53 - 1:39
	0:30 - 0:53
	0:23 - 0:57
	0:27 - 0:42
	

	
	75/25
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	

	below -8 to -14 °C
(below 18 to 7 °F)
	100/0
	0:49 - 1:58
	0:19 - 0:38
	1:31 - 1:50
	0:49 - 1:31
	0:27 - 0:49
	0:23 - 0:5710
	0:27 - 0:4210
	

	
	75/25
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	

	below -14 to -18 °C
(below 7 to 0 °F)
	100/0
	0:27 - 0:34
	0:08 - 0:15
	0:42 - 0:49
	0:23 - 0:42
	0:11 - 0:23
	
	

	below -18 to -25 °C
(below 0 to -13 °F)
	100/0
	0:27 - 0:34
	0:05 - 0:08
	0:23 - 0:27
	0:11 - 0:23
	0:06 - 0:11
	
	

	below -25 to -28 °C
(below -13 to -18 °F)
	100/0
	0:27 - 0:34
	0:04 - 0:07
	0:19 - 0:23
	0:08 - 0:19
	0:05 - 0:08
	
	


THIS TABLE IS FOR USE WHEN FLAPS/SLATS ARE DEPLOYED PRIOR TO DE/ANTI-ICING. HOLDOVER TIMES HAVE BEEN ADJUSTED TO 76 PERCENT.
NOTES
1. Ensure that the lowest operational use temperature (LOUT) is respected. Consider use of Type I fluid when Type II fluid cannot be used.
1. Freezing mist is best confirmed by observation. It is never reported by METAR; however, it can occur when mist is present at 0 °C (32 °F) and below. 
1. Use freezing fog holdover times in conditions of ice crystals mixed with freezing fog or freezing mist.
1. To determine snowfall intensity, the Snowfall Intensities as a Function of Prevailing Visibility table (Table 57) is required. No holdover times exist if the reported visibility correlates to a “heavy” precipitation intensity. 
Use snow holdover times in conditions of very light, light, or moderate snow mixed with ice crystals.
Includes light, moderate and heavy freezing drizzle. Use light freezing rain holdover times if positive identification of freezing drizzle is not possible.
These holdover times apply to conditions of “moderate” precipitation intensity. In cases of very light or light snow mixed with light rain or drizzle, use light freezing rain holdover times. The Snowfall Intensities as a Function of Prevailing Visibility table (Table 57) is required to confirm the precipitation intensity. No holdover times exist if the reported visibility correlates to a “heavy” precipitation intensity.
No holdover time guidelines exist for this condition for 0 °C (32 °F) and below.
Heavy snow, ice pellets, moderate and heavy freezing rain, small hail and hail.
No holdover time guidelines exist for this condition below -10 °C (14 °F).
CAUTIONS
The cautions that apply to the holdover times in the table above can be found on page A-9.

[bookmark: _Toc231475383]Table Adj-12: Adjusted Type II Holdover Times for
LNT Solutions P250
	Outside Air 
Temperature1
	Fluid 
Concentration 
Fluid/Water 
By % Volume
	Freezing Fog, Freezing Mist2, or Ice Crystals3
	Snow 
mixed with 
Freezing Fog4
	Very Light Snow, Snow Grains or Snow Pellets4,5
	Light 
Snow, Snow Grains or Snow Pellets4,5
	Moderate Snow, Snow Grains or Snow Pellets4,5
	Freezing 
Drizzle6
	Light 
Freezing Rain
	Moderate
Snow mixed with Rain7,8
	Rain on 
Cold‑Soaked Wing8
	Other9

	-3 °C and above
(27 °F and above)
	100/0
	2:17 - 3:02
	0:30 - 1:01
	2:55 - 3:00
	1:24 - 2:55
	0:38 - 1:24
	1:24 - 1:31
	0:46 - 1:08
	0:15 - 0:15
	0:23 - 1:24
	 

	
	75/25
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	 

	
	50/50
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	CAUTION: 
No holdover time 
guidelines exist

	below -3 to -8 °C
(below 27 to 18 °F)
	100/0
	0:42 - 2:05
	0:23 - 0:49
	2:13 - 2:51
	1:05 - 2:13
	0:30 - 1:05
	0:27 - 1:20
	0:19 - 0:34
	

	
	75/25
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	

	below -8 to -14 °C
(below 18 to 7 °F)
	100/0
	0:42 - 2:05
	0:19 - 0:38
	1:54 - 2:21
	0:53 - 1:54
	0:27 - 0:53
	0:27 - 1:2010
	0:19 - 0:3410
	

	
	75/25
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	

	below -14 to -18 °C
(below 7 to 0 °F)
	100/0
	0:15 - 0:23
	0:01 - 0:04
	0:15 - 0:23
	0:05 - 0:15
	0:02 - 0:05
	
	

	below -18 to -25 °C
(below 0 to -13 °F)
	100/0
	0:15 - 0:23
	0:00 - 0:02
	0:07 - 0:11
	0:02 - 0:07
	0:01 - 0:02
	
	

	below -25 to -29 °C
(below -13 to -20 °F)
	100/0
	0:15 - 0:23
	0:00 - 0:00
	0:04 - 0:05
	0:01 - 0:04
	0:00 - 0:01
	
	


THIS TABLE IS FOR USE WHEN FLAPS/SLATS ARE DEPLOYED PRIOR TO DE/ANTI-ICING. HOLDOVER TIMES HAVE BEEN ADJUSTED TO 76 PERCENT.
NOTES
1. Ensure that the lowest operational use temperature (LOUT) is respected. Consider use of Type I fluid when Type II fluid cannot be used.
1. Freezing mist is best confirmed by observation. It is never reported by METAR; however, it can occur when mist is present at 0 °C (32 °F) and below. 
1. Use freezing fog holdover times in conditions of ice crystals mixed with freezing fog or freezing mist.
1. To determine snowfall intensity, the Snowfall Intensities as a Function of Prevailing Visibility table (Table 57) is required. No holdover times exist if the reported visibility correlates to a “heavy” precipitation intensity. 
Use snow holdover times in conditions of very light, light, or moderate snow mixed with ice crystals.
Includes light, moderate and heavy freezing drizzle. Use light freezing rain holdover times if positive identification of freezing drizzle is not possible.
These holdover times apply to conditions of “moderate” precipitation intensity. In cases of very light or light snow mixed with light rain or drizzle, use light freezing rain holdover times. The Snowfall Intensities as a Function of Prevailing Visibility table (Table 57) is required to confirm the precipitation intensity. No holdover times exist if the reported visibility correlates to a “heavy” precipitation intensity.
No holdover time guidelines exist for this condition for 0 °C (32 °F) and below.
Heavy snow, ice pellets, moderate and heavy freezing rain, small hail and hail.
No holdover time guidelines exist for this condition below -10 °C (14 °F).
CAUTIONS
The cautions that apply to the holdover times in the table above can be found on page A-9

[bookmark: _Toc107305574][bookmark: _Toc231475384]Table Adj-13: Adjusted Type II Holdover Times for
MKS DevO Chemicals COREICEPHOB TYPE II
	Outside Air 
Temperature1
	Fluid 
Concentration 
Fluid/Water 
By % Volume
	Freezing Fog, Freezing Mist2, or Ice Crystals3
	Snow 
mixed with 
Freezing Fog4
	Very Light Snow, Snow Grains or Snow Pellets4,5
	Light 
Snow, Snow Grains or Snow Pellets4,5
	Moderate Snow, Snow Grains or Snow Pellets4,5
	Freezing 
Drizzle6
	Light 
Freezing Rain
	Moderate
Snow mixed with Rain7,8
	Rain on 
Cold‑Soaked Wing8
	Other9

	-3 °C and above
(27 °F and above)
	100/0
	1:27 - 2:05
	0:23 - 0:46
	1:58 - 2:24
	1:05 - 1:58
	0:30 - 1:05
	0:53 - 1:31
	0:34 - 0:46
	0:07 - 0:07
	0:11 - 1:12
	 

	
	75/25
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	 

	
	50/50
	0:49 - 1:20
	0:11 - 0:27
	1:12 - 1:27
	0:34 - 1:12
	0:19 - 0:34
	0:38 - 0:57
	0:19 - 0:23
	CAUTION: 
No holdover time 
guidelines exist

	below -3 to -8 °C
(below 27 to 18 °F)
	100/0
	0:34 - 1:05
	0:19 - 0:34
	1:24 - 1:43
	0:46 - 1:24
	0:23 - 0:46
	0:23 - 0:53
	0:19 - 0:27
	

	
	75/25
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	

	below -8 to -14 °C
(below 18 to 7 °F)
	100/0
	0:34 - 1:05
	0:15 - 0:27
	1:08 - 1:24
	0:38 - 1:08
	0:19 - 0:38
	0:23 - 0:5310
	0:19 - 0:2710
	

	
	75/25
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	

	below -14 to -18 °C
(below 7 to 0 °F)
	100/0
	0:11 - 0:19
	0:06 - 0:11
	0:27 - 0:30
	0:15 - 0:27
	0:08 - 0:15
	
	

	below -18 to -25 °C
(below 0 to -13 °F)
	100/0
	0:11 - 0:19
	0:02 - 0:04
	0:11 - 0:11
	0:05 - 0:11
	0:03 - 0:05
	
	

	below -25 to -27 °C
(below -13 to -17 °F)
	100/0
	0:11 - 0:19
	0:02 - 0:03
	0:08 - 0:08
	0:04 - 0:08
	0:02 - 0:04
	
	


THIS TABLE IS FOR USE WHEN FLAPS/SLATS ARE DEPLOYED PRIOR TO DE/ANTI-ICING. HOLDOVER TIMES HAVE BEEN ADJUSTED TO 76 PERCENT.
NOTES
1 Ensure that the lowest operational use temperature (LOUT) is respected. Consider use of Type I fluid when Type II fluid cannot be used.
2 Freezing mist is best confirmed by observation. It is never reported by METAR; however, it can occur when mist is present at 0 °C (32 °F) and below. 
3 Use freezing fog holdover times in conditions of ice crystals mixed with freezing fog or freezing mist.
4 To determine snowfall intensity, the Snowfall Intensities as a Function of Prevailing Visibility table (Table 57) is required. No holdover times exist if the reported visibility correlates to a “heavy” precipitation intensity. 
5 Use snow holdover times in conditions of very light, light, or moderate snow mixed with ice crystals.
6 Includes light, moderate and heavy freezing drizzle. Use light freezing rain holdover times if positive identification of freezing drizzle is not possible.
7 These holdover times apply to conditions of “moderate” precipitation intensity. In cases of very light or light snow mixed with light rain or drizzle, use light freezing rain holdover times. The Snowfall Intensities as a Function of Prevailing Visibility table (Table 57) is required to confirm the precipitation intensity. No holdover times exist if the reported visibility correlates to a “heavy” precipitation intensity.
8 No holdover time guidelines exist for this condition for 0 °C (32 °F) and below.
9 Heavy snow, ice pellets, moderate and heavy freezing rain, small hail and hail.
10 No holdover time guidelines exist for this condition below -10 °C (14 °F).
CAUTIONS
The cautions that apply to the holdover times in the table above can be found on page A-9.

[bookmark: _Toc107305575][bookmark: _Toc231475385]Table Adj-14: Adjusted Type II Holdover Times for
Newave Aerochemical FCY-2
	Outside Air 
Temperature1
	Fluid 
Concentration 
Fluid/Water 
By % Volume
	Freezing Fog, Freezing Mist2, 
or Ice Crystals3
	Snow 
mixed with 
Freezing Fog4
	Snow, 
Snow Grains or Snow Pellets4,5
	Freezing 
Drizzle6
	Light 
Freezing Rain
	Moderate
Snow mixed with Rain7,8
	Rain on Cold‑Soaked Wing8
	Other9

	-3 °C and above
(27 °F and above)
	100/0
	0:57 - 1:50
	0:19 - 0:30
	0:23 - 0:42
	0:27 - 0:49
	0:19 - 0:27
	0:05 - 0:05
	0:06 - 0:34
	 

	
	75/25
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	 

	
	50/50
	N/A
	N/A
	N/A
	N/A
	N/A
	CAUTION: 
No holdover time 
guidelines exist

	below -3 to -8 °C
(below 27 to 18 °F)
	100/0
	0:34 - 1:08
	0:11 - 0:23
	0:15 - 0:30
	0:15 - 0:34
	0:11 - 0:15
	

	
	75/25
	N/A
	N/A
	N/A
	N/A
	N/A
	

	below -8 to -14 °C
(below 18 to 7 °F)
	100/0
	0:34 - 1:08
	0:08 - 0:19
	0:11 - 0:23
	0:1510 - 0:3410
	0:1110 - 0:1510
	

	
	75/25
	N/A
	N/A
	N/A
	N/A
	N/A
	

	below -14 to -18 °C
(below 7 to 0 °F)
	100/0
	0:19 - 0:27
	0:01 - 0:04
	0:02 - 0:05
	 
	

	below -18 to -25 °C
(below 0 to -13 °F)
	100/0
	0:19 - 0:27
	0:00 - 0:02
	0:01 - 0:02
	 
	 
	

	below -25 to -28 °C
(below -13 to -18 °F)
	100/0
	0:19 - 0:27
	0:00 - 0:00
	0:00 - 0:01
	 
	


THIS TABLE IS FOR USE WHEN FLAPS/SLATS ARE DEPLOYED PRIOR TO DE/ANTI-ICING. HOLDOVER TIMES HAVE BEEN ADJUSTED TO 76 PERCENT.
NOTES
1. Ensure that the lowest operational use temperature (LOUT) is respected. Consider use of Type I fluid when Type II fluid cannot be used.
1. Freezing mist is best confirmed by observation. It is never reported by METAR; however, it can occur when mist is present at 0 °C (32 °F) and below. 
1. Use freezing fog holdover times in conditions of ice crystals mixed with freezing fog or freezing mist.
1. To determine snowfall intensity, the Snowfall Intensities as a Function of Prevailing Visibility table (Table 57) is required. No holdover times exist if the reported visibility correlates to a “heavy” precipitation intensity. 
Use snow holdover times in conditions of very light, light, or moderate snow mixed with ice crystals.
Includes light, moderate and heavy freezing drizzle. Use light freezing rain holdover times if positive identification of freezing drizzle is not possible.
These holdover times apply to conditions of “moderate” precipitation intensity. In cases of very light or light snow mixed with light rain or drizzle, use light freezing rain holdover times. The Snowfall Intensities as a Function of Prevailing Visibility table (Table 57) is required to confirm the precipitation intensity. No holdover times exist if the reported visibility correlates to a “heavy” precipitation intensity.
No holdover time guidelines exist for this condition for 0 °C (32 °F) and below.
Heavy snow, ice pellets, moderate and heavy freezing rain, small hail and hail.
No holdover time guidelines exist for this condition below -10 °C (14 °F).
CAUTIONS
The cautions that apply to the holdover times in the table above can be found on page A-9.

[bookmark: _Toc75345466][bookmark: _Toc77777032][bookmark: _Toc77777082][bookmark: _Toc105048924][bookmark: _Toc105049278][bookmark: _Toc105049401][bookmark: _Toc105399218][bookmark: _Toc105399429][bookmark: _Toc107305577][bookmark: _Toc231475386][bookmark: _Toc9500353][bookmark: _Toc14166563][bookmark: _Toc14867900][bookmark: _Toc43986217][bookmark: _Toc44053683][bookmark: _Toc44054102][bookmark: _Toc45715335][bookmark: _Toc517088957][bookmark: _Toc517253614][bookmark: _Toc519674717][bookmark: _Toc519674824][bookmark: _Toc520288576][bookmark: _Toc520289448][bookmark: _Toc436349473]Table Adj-15: Adjusted Type II Holdover Times for
ROMCHIM ADD-PROTECT NG Type II
	Outside Air 
Temperature1
	Fluid 
Concentration 
Fluid/Water 
By % Volume
	Freezing Fog, Freezing Mist2, or Ice Crystals3
	Snow 
mixed with 
Freezing Fog4
	Very Light Snow, Snow Grains or Snow Pellets4,5
	Light 
Snow, Snow Grains or Snow Pellets4,5
	Moderate Snow, Snow Grains or Snow Pellets4,5
	Freezing 
Drizzle6
	Light 
Freezing Rain
	Moderate
Snow mixed with Rain7,8
	Rain on 
Cold‑Soaked Wing8
	Other9

	-3 °C and above
(27 °F and above)
	100/0
	0:53 - 1:50
	0:19 - 0:42
	1:58 - 2:28
	0:53 - 1:58
	0:27 - 0:53
	0:38 - 1:01
	0:27 - 0:38
	0:04 - 0:04
	0:05 - 0:53
	 

	
	75/25
	0:46 - 1:24
	0:15 - 0:30
	1:27 - 1:50
	0:42 - 1:27
	0:19 - 0:42
	0:30 - 0:57
	0:19 - 0:30
	0:04 - 0:04
	0:05 - 0:42
	 

	
	50/50
	0:19 - 0:42
	0:08 - 0:15
	0:42 - 0:49
	0:23 - 0:42
	0:11 - 0:23
	0:15 - 0:27
	0:08 - 0:15
	CAUTION: 
No holdover time 
guidelines exist

	below -3 to -8 °C
(below 27 to 18 °F)
	100/0
	0:42 - 1:12
	0:15 - 0:30
	1:24 - 1:46
	0:38 - 1:24
	0:19 - 0:38
	0:27 - 0:53
	0:19 - 0:27
	

	
	75/25
	0:42 - 1:05
	0:11 - 0:23
	1:05 - 1:20
	0:30 - 1:05
	0:15 - 0:30
	0:19 - 0:49
	0:15 - 0:23
	

	below -8 to -14 °C
(below 18 to 7 °F)
	100/0
	0:42 - 1:12
	0:11 - 0:23
	1:05 - 1:24
	0:30 - 1:05
	0:15 - 0:30
	0:27 - 0:5310
	0:19 - 0:2710
	

	
	75/25
	0:42 - 1:05
	0:08 - 0:19
	0:49 - 1:05
	0:23 - 0:49
	0:11 - 0:23
	0:19 - 0:4910
	0:15 - 0:2310
	

	below -14 to -18 °C
(below 7 to 0 °F)
	100/0
	0:11 - 0:15
	0:01 - 0:04
	0:15 - 0:23
	0:05 - 0:15
	0:02 - 0:05
	
	

	below -18 to -25 °C
(below 0 to -13 °F)
	100/0
	0:11 - 0:15
	0:00 - 0:02
	0:07 - 0:11
	0:02 - 0:07
	0:01 - 0:02
	
	

	below -25 to -28 °C
(below -13 to -18 °F)
	100/0
	0:11 - 0:15
	0:00 - 0:00
	0:04 - 0:05
	0:01 - 0:04
	0:00 - 0:01
	
	


THIS TABLE IS FOR USE WHEN FLAPS/SLATS ARE DEPLOYED PRIOR TO DE/ANTI-ICING. HOLDOVER TIMES HAVE BEEN ADJUSTED TO 76 PERCENT.
NOTES
1. Ensure that the lowest operational use temperature (LOUT) is respected. Consider use of Type I fluid when Type II fluid cannot be used.
1. Freezing mist is best confirmed by observation. It is never reported by METAR; however, it can occur when mist is present at 0 °C (32 °F) and below. 
1. Use freezing fog holdover times in conditions of ice crystals mixed with freezing fog or freezing mist.
1. To determine snowfall intensity, the Snowfall Intensities as a Function of Prevailing Visibility table (Table 57) is required. No holdover times exist if the reported visibility correlates to a “heavy” precipitation intensity.
Use snow holdover times in conditions of very light, light, or moderate snow mixed with ice crystals.
Includes light, moderate and heavy freezing drizzle. Use light freezing rain holdover times if positive identification of freezing drizzle is not possible.
These holdover times apply to conditions of “moderate” precipitation intensity. In cases of very light or light snow mixed with light rain or drizzle, use light freezing rain holdover times. The Snowfall Intensities as a Function of Prevailing Visibility table (Table 57) is required to confirm the precipitation intensity. No holdover times exist if the reported visibility correlates to a “heavy” precipitation intensity.
No holdover time guidelines exist for this condition for 0 °C (32 °F) and below.
Heavy snow, ice pellets, moderate and heavy freezing rain, small hail and hail.
No holdover time guidelines exist for this condition below -10 °C (14 °F).
CAUTIONS
The cautions that apply to the holdover times in the table above can be found on page A-9.

[bookmark: _Toc75345467][bookmark: _Toc77777033][bookmark: _Toc77777083][bookmark: _Toc105048925][bookmark: _Toc105049279][bookmark: _Toc105049402][bookmark: _Toc105399219][bookmark: _Toc105399430][bookmark: _Toc107305578][bookmark: _Toc231475387]Table Adj-16: Adjusted Type II Holdover Times for
ROMCHIM ADD-PROTECT Type II
	Outside Air 
Temperature1
	Fluid 
Concentration 
Fluid/Water 
By % Volume
	Freezing Fog, Freezing Mist2, or Ice Crystals3
	Snow 
mixed with 
Freezing Fog4
	Very Light Snow, Snow Grains or Snow Pellets4,5
	Light 
Snow, Snow Grains or Snow Pellets4,5
	Moderate Snow, Snow Grains or Snow Pellets4,5
	Freezing 
Drizzle6
	Light 
Freezing Rain
	Moderate
Snow mixed with Rain7,8
	Rain on 
Cold‑Soaked Wing8
	Other9

	-3 °C and above
(27 °F and above)
	100/0
	1:16 - 2:40
	0:15 - 0:34
	1:27 - 1:50
	0:46 - 1:27
	0:23 - 0:46
	0:30 - 1:12
	0:19 - 0:34
	0:05 - 0:05
	0:07 - 0:38
	 

	
	75/25
	0:30 - 0:53
	0:11 - 0:19
	0:46 - 0:53
	0:23 - 0:46
	0:11 - 0:23
	0:19 - 0:30
	0:11 - 0:19
	0:03 - 0:03
	0:04 - 0:19
	 

	
	50/50
	0:15 - 0:27
	0:05 - 0:11
	0:23 - 0:27
	0:11 - 0:23
	0:07 - 0:11
	0:08 - 0:23
	0:06 - 0:08
	CAUTION: 
No holdover time 
guidelines exist

	below -3 to -8 °C
(below 27 to 18 °F)
	100/0
	0:23 - 0:34
	0:11 - 0:23
	1:01 - 1:16
	0:30 - 1:01
	0:15 - 0:30
	0:19 - 0:38
	0:15 - 0:23
	

	
	75/25
	0:23 - 0:42
	0:07 - 0:11
	0:30 - 0:38
	0:19 - 0:30
	0:08 - 0:19
	0:15 - 0:23
	0:11 - 0:15
	

	below -8 to -14 °C
(below 18 to 7 °F)
	100/0
	0:23 - 0:34
	0:11 - 0:19
	0:49 - 1:01
	0:27 - 0:49
	0:11 - 0:27
	0:19 - 0:3810
	0:15 - 0:2310
	

	
	75/25
	0:23 - 0:42
	0:05 - 0:11
	0:27 - 0:30
	0:15 - 0:27
	0:07 - 0:15
	0:15 - 0:2310
	0:11 - 0:1510
	

	below -14 to -18 °C
(below 7 to 0 °F)
	100/0
	0:11 - 0:19
	0:01 - 0:04
	0:15 - 0:23
	0:05 - 0:15
	0:02 - 0:05
	
	

	below -18 to -25 °C
(below 0 to -13 °F)
	100/0
	0:11 - 0:19
	0:00 - 0:02
	0:07 - 0:11
	0:02 - 0:07
	0:01 - 0:02
	
	

	below -25 to -28 °C
(below -13 to -18 °F)
	100/0
	0:11 - 0:19
	0:00 - 0:00
	0:04 - 0:05
	0:01 - 0:04
	0:00 - 0:01
	
	


THIS TABLE IS FOR USE WHEN FLAPS/SLATS ARE DEPLOYED PRIOR TO DE/ANTI-ICING. HOLDOVER TIMES HAVE BEEN ADJUSTED TO 76 PERCENT.
NOTES
1. Ensure that the lowest operational use temperature (LOUT) is respected. Consider use of Type I fluid when Type II fluid cannot be used.
1. Freezing mist is best confirmed by observation. It is never reported by METAR; however, it can occur when mist is present at 0 °C (32 °F) and below. 
1. Use freezing fog holdover times in conditions of ice crystals mixed with freezing fog or freezing mist.
1. To determine snowfall intensity, the Snowfall Intensities as a Function of Prevailing Visibility table (Table 57) is required. No holdover times exist if the reported visibility correlates to a “heavy” precipitation intensity.
Use snow holdover times in conditions of very light, light, or moderate snow mixed with ice crystals.
Includes light, moderate and heavy freezing drizzle. Use light freezing rain holdover times if positive identification of freezing drizzle is not possible.
These holdover times apply to conditions of “moderate” precipitation intensity. In cases of very light or light snow mixed with light rain or drizzle, use light freezing rain holdover times. The Snowfall Intensities as a Function of Prevailing Visibility table (Table 57) is required to confirm the precipitation intensity. No holdover times exist if the reported visibility correlates to a “heavy” precipitation intensity.
No holdover time guidelines exist for this condition for 0 °C (32 °F) and below.
Heavy snow, ice pellets, moderate and heavy freezing rain, small hail and hail.
No holdover time guidelines exist for this condition below -10 °C (14 °F).
CAUTIONS
The cautions that apply to the holdover times in the table above can be found on page A-9.
Appendix A: FAA Adjusted Holdover Time Guidelines	Winter 2026-2027
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[bookmark: _Toc107305579][bookmark: _Toc231475388]Adjusted HOT Guidelines for SAE Type III Fluids
Winter 2026-2027

The HOT Guidelines are provided for information and guidance purposes. The HOT Guidelines on their own do not change, create, amend or permit deviations from regulatory requirements.

The HOT Guidelines may use mandatory terms such as “must”, “shall” and “is/are required” so as to convey the intent of meeting regulatory requirements and SAE Standards, where applicable. The term “should” is to be understood, unless an alternative method of achieving safety is implemented that would meet or exceed the intent of the recommendation.



[bookmark: TypeIIICautionsAdj]CAUTIONS
The responsibility for the application of these data remains with the user.
The time of protection will be shortened in heavy weather conditions, heavy precipitation rates or high moisture content.
High wind velocity, jet blast or blowing snow may reduce holdover time below the lowest time stated in the range.
The holdover time may be reduced when aircraft skin temperature is lower than outside air temperature.
Fluids used during ground de/anti-icing do not provide in-flight icing protection.
This table is for departure planning only and should be used in conjunction with pre-takeoff check procedures.


Appendix A: FAA Adjusted Holdover Time Guidelines	Winter 2026-2027

Original Issue	Page A-99	August 11, 2026
[bookmark: _Toc231475389][bookmark: _Toc9500354][bookmark: _Toc14166564][bookmark: _Toc14867901][bookmark: _Toc43986218][bookmark: _Toc44053684][bookmark: _Toc44054103][bookmark: _Toc45715336][bookmark: _Toc75345468][bookmark: _Toc77777034][bookmark: _Toc77777084][bookmark: _Toc105048926][bookmark: _Toc105049280][bookmark: _Toc105049403][bookmark: _Toc105399220][bookmark: _Toc105399431][bookmark: _Toc107305580]Table Adj-17: Adjusted Type III Holdover Times for 
AllClear AeroClear MAX Applied Unheated – Low Speed Ramp Test1,2
	Outside Air 
Temperature3
	Fluid 
Concentration 
Fluid/Water 
By % Volume
	Freezing Fog, Freezing Mist4, or Ice Crystals5
	Snow 
mixed with 
Freezing Fog6
	Very Light Snow, Snow Grains or Snow Pellets6,7
	Light 
Snow, Snow Grains or Snow Pellets6,7
	Moderate Snow, Snow Grains or Snow Pellets6,7
	Freezing 
Drizzle8
	Light 
Freezing Rain
	Moderate
Snow mixed with Rain9,10
	Rain on
Cold‑Soaked Wing10
	Other11

	-3 °C and above
(27 °F and above)
	100/0
	0:34 - 1:27
	0:08 - 0:19
	0:53 - 1:08
	0:27 - 0:53
	0:11 - 0:27
	0:19 - 0:38
	0:11 - 0:19
	0:03 - 0:03
	0:04 - 0:30
	 

	
	75/25
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	 

	
	50/50
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	CAUTION: 
No holdover time 
guidelines exist

	below -3 to -10 °C
(below 27 to 14 °F)
	100/0
	0:38 - 1:16
	0:08 - 0:19
	0:53 - 1:08
	0:27 - 0:53
	0:11 - 0:27
	0:19 - 0:34
	0:11 - 0:19
	

	
	75/25
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	

	below -10 to -16 °C
(below 14 to 3 °F)
	100/0
	0:30 - 1:20
	0:08 - 0:19
	0:53 - 1:08
	0:27 - 0:53
	0:11 - 0:27
	
	


THIS TABLE IS FOR USE WHEN FLAPS/SLATS ARE DEPLOYED PRIOR TO DE/ANTI-ICING. HOLDOVER TIMES HAVE BEEN ADJUSTED TO 76 PERCENT.
NOTES
1. Consult the aircraft manufacturer’s documentation to determine application of low, middle, or high speed ramp test values. If uncertain, apply low speed test values.
1. Fluid must be applied unheated to use these holdover times. No holdover times exist for this fluid applied heated.
Ensure that the lowest operational use temperature (LOUT) is respected. Consider use of Type I fluid when Type III fluid cannot be used.
Freezing mist is best confirmed by observation. It is never reported by METAR; however, it can occur when mist is present at 0 °C (32 °F) and below. 
Use freezing fog holdover times in conditions of ice crystals mixed with freezing fog or freezing mist.
To determine snowfall intensity, the Snowfall Intensities as a Function of Prevailing Visibility table (Table 57) is required. No holdover times exist if the reported visibility correlates to a “heavy” precipitation intensity.
Use snow holdover times in conditions of very light, light, or moderate snow mixed with ice crystals.
Includes light, moderate and heavy freezing drizzle. Use light freezing rain holdover times if positive identification of freezing drizzle is not possible.
These holdover times apply to conditions of “moderate” precipitation intensity. In cases of very light or light snow mixed with light rain or drizzle, use light freezing rain holdover times. The Snowfall Intensities as a Function of Prevailing Visibility table (Table 57) is required to confirm the precipitation intensity. No holdover times exist if the reported visibility correlates to a “heavy” precipitation intensity.
No holdover time guidelines exist for this condition for 0 °C (32 °F) and below.
Heavy snow, ice pellets, moderate and heavy freezing rain, small hail and hail.
CAUTIONS
The cautions that apply to the holdover times in the table above can be found on page A-23.

[bookmark: _Toc231475390][bookmark: _Toc105048927][bookmark: _Toc105049281][bookmark: _Toc105049404][bookmark: _Toc105399221][bookmark: _Toc105399432][bookmark: _Toc107305581][bookmark: _Toc517088958][bookmark: _Toc517253615][bookmark: _Toc519674718][bookmark: _Toc519674825][bookmark: _Toc520288577][bookmark: _Toc520289449][bookmark: _Toc9500355][bookmark: _Toc14166565][bookmark: _Toc14867902][bookmark: _Toc43986219][bookmark: _Toc44053685][bookmark: _Toc44054104][bookmark: _Toc45715337][bookmark: _Toc75345469][bookmark: _Toc77777035][bookmark: _Toc77777085][bookmark: _Toc436349474]Table Adj-18: Adjusted Type III Holdover Times for 
AllClear AeroClear MAX Applied Unheated – Middle Speed Ramp Test1,2
	Outside Air 
Temperature3
	Fluid 
Concentration 
Fluid/Water 
By % Volume
	Freezing Fog, Freezing Mist4, or Ice Crystals5
	Snow 
mixed with 
Freezing Fog6
	Very Light Snow, Snow Grains or Snow Pellets6,7
	Light 
Snow, Snow Grains or Snow Pellets6,7
	Moderate Snow, Snow Grains or Snow Pellets6,7
	Freezing 
Drizzle8
	Light 
Freezing Rain
	Moderate
Snow mixed with Rain9,10
	Rain on
Cold‑Soaked Wing10
	Other11

	-3 °C and above
(27 °F and above)
	100/0
	0:34 - 1:27
	0:08 - 0:19
	0:53 - 1:08
	0:27 - 0:53
	0:11 - 0:27
	0:19 - 0:38
	0:11 - 0:19
	0:03 - 0:03
	0:04 - 0:30
	 

	
	75/25
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	 

	
	50/50
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	CAUTION: 
No holdover time 
guidelines exist

	below -3 to -10 °C
(below 27 to 14 °F)
	100/0
	0:38 - 1:16
	0:08 - 0:19
	0:53 - 1:08
	0:27 - 0:53
	0:11 - 0:27
	0:19 - 0:34
	0:11 - 0:19
	

	
	75/25
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	

	below -10 to -20.5 °C
(below 14 to -5 °F)
	100/0
	0:30 - 1:20
	0:08 - 0:19
	0:53 - 1:08
	0:27 - 0:53
	0:11 - 0:27
	
	


THIS TABLE IS FOR USE WHEN FLAPS/SLATS ARE DEPLOYED PRIOR TO DE/ANTI-ICING. HOLDOVER TIMES HAVE BEEN ADJUSTED TO 76 PERCENT.
NOTES
1. Consult the aircraft manufacturer’s documentation to determine application of low, middle, or high speed ramp test values. If uncertain, apply low speed test values.
Fluid must be applied unheated to use these holdover times. No holdover times exist for this fluid applied heated.
Ensure that the lowest operational use temperature (LOUT) is respected. Consider use of Type I fluid when Type III fluid cannot be used.
Freezing mist is best confirmed by observation. It is never reported by METAR; however, it can occur when mist is present at 0 °C (32 °F) and below. 
Use freezing fog holdover times in conditions of ice crystals mixed with freezing fog or freezing mist.
To determine snowfall intensity, the Snowfall Intensities as a Function of Prevailing Visibility table (Table 57) is required. No holdover times exist if the reported visibility correlates to a “heavy” precipitation intensity.
Use snow holdover times in conditions of very light, light, or moderate snow mixed with ice crystals.
Includes light, moderate and heavy freezing drizzle. Use light freezing rain holdover times if positive identification of freezing drizzle is not possible.
These holdover times apply to conditions of “moderate” precipitation intensity. In cases of very light or light snow mixed with light rain or drizzle, use light freezing rain holdover times. The Snowfall Intensities as a Function of Prevailing Visibility table (Table 57) is required to confirm the precipitation intensity. No holdover times exist if the reported visibility correlates to a “heavy” precipitation intensity.
No holdover time guidelines exist for this condition for 0 °C (32 °F) and below.
Heavy snow, ice pellets, moderate and heavy freezing rain, small hail and hail.
CAUTIONS
The cautions that apply to the holdover times in the table above can be found on page A-23.

[bookmark: _Toc231475391][bookmark: _Toc105048928][bookmark: _Toc105049282][bookmark: _Toc105049405][bookmark: _Toc105399222][bookmark: _Toc105399433][bookmark: _Toc107305582]Table Adj-19: Adjusted Type III Holdover Times for 
AllClear AeroClear MAX Applied Unheated – High Speed Ramp Test1,2
	Outside Air 
Temperature3
	Fluid 
Concentration 
Fluid/Water 
By % Volume
	Freezing Fog, Freezing Mist4, or Ice Crystals5
	Snow 
mixed with 
Freezing Fog6
	Very Light Snow, Snow Grains or Snow Pellets6,7
	Light 
Snow, Snow Grains or Snow Pellets6,7
	Moderate Snow, Snow Grains or Snow Pellets6,7
	Freezing 
Drizzle8
	Light 
Freezing Rain
	Moderate
Snow mixed with Rain9,10
	Rain on
Cold‑Soaked Wing10
	Other11

	-3 °C and above
(27 °F and above)
	100/0
	0:34 - 1:27
	0:08 - 0:19
	0:53 - 1:08
	0:27 - 0:53
	0:11 - 0:27
	0:19 - 0:38
	0:11 - 0:19
	0:03 - 0:03
	0:04 - 0:30
	 

	
	75/25
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	 

	
	50/50
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	CAUTION: 
No holdover time 
guidelines exist

	below -3 to -10 °C
(below 27 to 14 °F)
	100/0
	0:38 - 1:16
	0:08 - 0:19
	0:53 - 1:08
	0:27 - 0:53
	0:11 - 0:27
	0:19 - 0:34
	0:11 - 0:19
	

	
	75/25
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	

	below -10 to -25 °C
(below 14 to -13 °F)
	100/0
	0:30 - 1:20
	0:08 - 0:19
	0:53 - 1:08
	0:27 - 0:53
	0:11 - 0:27
	
	

	below -25 to -35 °C (below -13 to -31 °F)
	100/0
	0:19 - 0:46
	0:05 - 0:10
	0:30 - 0:38
	0:14 - 0:30
	0:06 - 0:14
	
	


THIS TABLE IS FOR USE WHEN FLAPS/SLATS ARE DEPLOYED PRIOR TO DE/ANTI-ICING. HOLDOVER TIMES HAVE BEEN ADJUSTED TO 76 PERCENT.
NOTES
1. Consult the aircraft manufacturer’s documentation to determine application of low, middle, or high speed ramp test values. If uncertain, apply low speed test values.
Fluid must be applied unheated to use these holdover times. No holdover times exist for this fluid applied heated.
Ensure that the lowest operational use temperature (LOUT) is respected. Consider use of Type I fluid when Type III fluid cannot be used.
Freezing mist is best confirmed by observation. It is never reported by METAR; however, it can occur when mist is present at 0 °C (32 °F) and below. 
Use freezing fog holdover times in conditions of ice crystals mixed with freezing fog or freezing mist.
To determine snowfall intensity, the Snowfall Intensities as a Function of Prevailing Visibility table (Table 57) is required. No holdover times exist if the reported visibility correlates to a “heavy” precipitation intensity.
Use snow holdover times in conditions of very light, light, or moderate snow mixed with ice crystals.
Includes light, moderate and heavy freezing drizzle. Use light freezing rain holdover times if positive identification of freezing drizzle is not possible.
These holdover times apply to conditions of “moderate” precipitation intensity. In cases of very light or light snow mixed with light rain or drizzle, use light freezing rain holdover times. The Snowfall Intensities as a Function of Prevailing Visibility table (Table 57) is required to confirm the precipitation intensity. No holdover times exist if the reported visibility correlates to a “heavy” precipitation intensity.
No holdover time guidelines exist for this condition for 0 °C (32 °F) and below.
Heavy snow, ice pellets, moderate and heavy freezing rain, small hail and hail (Table Adj-53 provides adjusted allowance times for ice pellets and small hail for SAE Type III fluids, applied unheated).
CAUTIONS
The cautions that apply to the holdover times in the table above can be found on page A-23.

Appendix A: FAA Adjusted Holdover Time Guidelines	Winter 2026-2027

Original Issue	Page A-3	August 11, 2026
[bookmark: _Toc107305583][bookmark: _Toc231475392][bookmark: _Toc436349477][bookmark: _Toc517088959][bookmark: _Toc517253616][bookmark: _Toc519674719][bookmark: _Toc519674826][bookmark: _Toc520288578][bookmark: _Toc520289450][bookmark: _Toc9500356][bookmark: _Toc14166566][bookmark: _Toc14867903][bookmark: _Toc43986220][bookmark: _Toc44053686][bookmark: _Toc44054105][bookmark: _Toc45715338][bookmark: _Toc75345470][bookmark: _Toc77777036][bookmark: _Toc77777086][bookmark: _Toc105048929][bookmark: _Toc105049283][bookmark: _Toc105049406][bookmark: _Toc105399223][bookmark: _Toc105399434]Adjusted HOT Guidelines for SAE Type IV Fluids
Winter 2026-2027

The HOT Guidelines are provided for information and guidance purposes. The HOT Guidelines on their own do not change, create, amend or permit deviations from regulatory requirements.

The HOT Guidelines may use mandatory terms such as “must”, “shall” and “is/are required” so as to convey the intent of meeting regulatory requirements and SAE Standards, where applicable. The term “should” is to be understood, unless an alternative method of achieving safety is implemented that would meet or exceed the intent of the recommendation.



[bookmark: TypeIVCautionsAdj]CAUTIONS
The responsibility for the application of these data remains with the user.
The time of protection will be shortened in heavy weather conditions, heavy precipitation rates or high moisture content.
High wind velocity, jet blast or blowing snow may reduce holdover time below the lowest time stated in the range.
The holdover time may be reduced when aircraft skin temperature is lower than outside air temperature.
Fluids used during ground de/anti-icing do not provide in-flight icing protection.
This table is for departure planning only and should be used in conjunction with pre-takeoff check procedures.
Whenever frost or ice occurs on the lower surface of the wing in the area of the fuel tank, indicating a cold-soaked wing, the 50/50 dilution of Type II or IV are not to be used for the anti-icing step because fluid freezing may occur.


Appendix A: FAA Adjusted Holdover Time Guidelines	Winter 2026-2027

Original Issue	Page A-99	August 11, 2026
[bookmark: _Toc107305584][bookmark: _Toc231475393]Table Adj-20: Adjusted Generic Holdover Times for SAE Type IV Fluids1
	Outside Air 
Temperature2
	Fluid 
Concentration 
Fluid/Water 
By % Volume
	Freezing Fog, Freezing Mist3, or Ice Crystals4
	Snow 
mixed with 
Freezing Fog5
	Very Light Snow, Snow Grains or Snow Pellets5,6
	Light 
Snow, Snow Grains or Snow Pellets5,6
	Moderate Snow, Snow Grains or Snow Pellets5,6
	Freezing 
Drizzle7
	Light 
Freezing Rain
	Moderate
Snow mixed with Rain8,9
	Rain on 
Cold‑Soaked Wing9
	Other10

	-3 °C and above
(27 °F and above)
	100/0
	0:57 - 1:43
	0:15 - 0:30
	1:24 - 1:43
	0:42 - 1:24
	0:19 - 0:42
	0:27 - 0:53
	0:11 - 0:23
	0:05 - 0:05
	0:06 - 0:49
	 

	
	75/25
	1:05 - 2:02
	0:23 - 0:42
	1:35 - 1:50
	0:57 - 1:35
	0:30 - 0:57
	0:46 - 1:01
	0:23 - 0:38
	0:05 - 0:05
	0:07 - 1:01
	 

	
	50/50
	0:23 - 0:42
	0:05 - 0:15
	0:46 - 0:53
	0:19 - 0:46
	0:08 - 0:19
	0:11 - 0:30
	0:07 - 0:15
	CAUTION: 
No holdover time 
guidelines exist

	below -3 to -8 °C
(below 27 to 18 °F)
	100/0
	0:11 - 0:27
	0:15 - 0:27
	1:12 - 1:31
	0:34 - 1:12
	0:19 - 0:34
	0:19 - 0:46
	0:15 - 0:19
	

	
	75/25
	0:30 - 1:01
	0:19 - 0:38
	1:24 - 1:39
	0:49 - 1:24
	0:23 - 0:49
	0:15 - 0:49
	0:11 - 0:19
	

	below -8 to -14 °C
(below 18 to 7 °F)
	100/0
	0:11 - 0:27
	0:11 - 0:23
	1:05 - 1:24
	0:34 - 1:05
	0:15 - 0:34
	0:19 - 0:4611
	0:11 - 0:1911
	

	
	75/25
	0:30 - 1:01
	0:15 - 0:34
	1:20 - 1:31
	0:42 - 1:20
	0:19 - 0:42
	0:15 - 0:4911
	0:11 - 0:1911
	

	below -14 to -18 °C
(below 7 to 0 °F)
	100/0
	0:11 - 0:19
	0:01 - 0:05
	0:23 - 0:34
	0:07 - 0:23
	0:02 - 0:07
	
	

	below -18 to -25 °C
(below 0 to -13 °F)
	100/0
	0:11 - 0:19
	0:00 - 0:02
	0:08 - 0:15
	0:02 - 0:08
	0:01 - 0:02
	
	

	below -25 °C 
(below -13 °F)
	100/0
	0:11 - 0:19
	0:00 - 0:01
	0:05 - 0:08
	0:02 - 0:05
	0:00 - 0:02
	
	


THIS TABLE IS FOR USE WHEN FLAPS/SLATS ARE DEPLOYED PRIOR TO DE/ANTI-ICING. HOLDOVER TIMES HAVE BEEN ADJUSTED TO 76 PERCENT.
NOTES
1. [bookmark: _Hlk107411458]To use the holdover times in this table, ensure that the fluid and dilution being used is listed in the Type IV Fluids Tested for Anti-Icing Performance and Aerodynamic Acceptance table (Table 61). Any restrictions on the use of the fluid have to be identified and applied.
1. Ensure that the lowest operational use temperature (LOUT) is respected. Consider use of Type I fluid when Type IV fluid cannot be used.
1. Freezing mist is best confirmed by observation. It is never reported by METAR; however, it can occur when mist is present at 0 °C (32 °F) and below. 
1. Use freezing fog holdover times in conditions of ice crystals mixed with freezing fog or freezing mist.
1. To determine snowfall intensity, the Snowfall Intensities as a Function of Prevailing Visibility table (Table 57) is required. No holdover times exist if the reported visibility correlates to a “heavy” precipitation intensity.
Use snow holdover times in conditions of very light, light, or moderate snow mixed with ice crystals.
Includes light, moderate and heavy freezing drizzle. Use light freezing rain holdover times if positive identification of freezing drizzle is not possible.
These holdover times apply to conditions of “moderate” precipitation intensity. In cases of very light or light snow mixed with light rain or drizzle, use light freezing rain holdover times. The Snowfall Intensities as a Function of Prevailing Visibility table (Table 57) is required to confirm the precipitation intensity. No holdover times exist if the reported visibility correlates to a “heavy” precipitation intensity.
No holdover time guidelines exist for this condition for 0 °C (32 °F) and below.
[bookmark: _Hlk77764398]Heavy snow, ice pellets, moderate and heavy freezing rain, small hail and hail (Table Adj-54 and Table Adj-55 provides allowance times for Type IV EG and Type IV PG fluids in ice pellets and small hail. To use these allowance times, ensure that the fluid being used is listed as validated in Table 53). 
No holdover time guidelines exist for this condition below -10 °C (14 °F).
CAUTIONS
The cautions that apply to the holdover times in the table above can be found on page A-27.

[bookmark: _Toc436349478][bookmark: _Toc517088960][bookmark: _Toc517253617][bookmark: _Toc519674720][bookmark: _Toc519674827][bookmark: _Toc520288579][bookmark: _Toc520289451][bookmark: _Toc9500357][bookmark: _Toc14166567][bookmark: _Toc14867904][bookmark: _Toc43986221][bookmark: _Toc44053687][bookmark: _Toc44054106][bookmark: _Toc45715339][bookmark: _Toc75345471][bookmark: _Toc77777037][bookmark: _Toc77777087][bookmark: _Toc105048930][bookmark: _Toc105049284][bookmark: _Toc105049407][bookmark: _Toc105399224][bookmark: _Toc105399435][bookmark: _Toc107305585][bookmark: _Toc231475394]Table Adj-21: Adjusted Type IV Holdover Times for 
ABAX ECOWING AD-49
	Outside Air 
Temperature1
	Fluid 
Concentration 
Fluid/Water 
By % Volume
	Freezing Fog, Freezing Mist2, or Ice Crystals3
	Snow 
mixed with 
Freezing Fog4
	Very Light Snow, Snow Grains or Snow Pellets4,5
	Light 
Snow, Snow Grains or Snow Pellets4,5
	Moderate Snow, Snow Grains or Snow Pellets4,5
	Freezing 
Drizzle6
	Light 
Freezing Rain
	Moderate
Snow mixed with Rain7,8
	Rain on 
Cold‑Soaked Wing8
	Other9

	-3 °C and above
(27 °F and above)
	100/0
	2:32 - 3:02
	0:34 - 1:05
	2:47 - 3:00
	1:27 - 2:47
	0:46 - 1:27
	1:05 - 1:31
	0:46 - 1:05
	0:06 - 0:06
	0:08 - 1:27
	 

	
	75/25
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	 

	
	50/50
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	CAUTION: 
No holdover time 
guidelines exist

	below -3 to -8 °C
(below 27 to 18 °F)
	100/0
	0:15 - 1:12
	0:27 - 0:49
	2:13 - 2:40
	1:08 - 2:13
	0:34 - 1:08
	0:19 - 1:05
	0:15 - 0:19
	

	
	75/25
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	

	below -8 to -14 °C
(below 18 to 7 °F)
	100/0
	0:15 - 1:12
	0:23 - 0:42
	1:50 - 2:17
	0:57 - 1:50
	0:30 - 0:57
	0:19 - 1:0510
	0:15 - 0:1910
	

	
	75/25
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	

	below -14 to -18 °C
(below 7 to 0 °F)
	100/0
	0:19 - 0:30
	0:01 - 0:05
	0:23 - 0:34
	0:07 - 0:23
	0:02 - 0:07
	
	

	below -18 to -25 °C
(below 0 to -13 °F)
	100/0
	0:19 - 0:30
	0:00 - 0:02
	0:08 - 0:15
	0:02 - 0:08
	0:01 - 0:02
	
	

	below -25 to -26 °C
(below -13 to -15 °F)
	100/0
	0:19 - 0:30
	0:00 - 0:01
	0:05 - 0:08
	0:02 - 0:05
	0:00 - 0:02
	
	


THIS TABLE IS FOR USE WHEN FLAPS/SLATS ARE DEPLOYED PRIOR TO DE/ANTI-ICING. HOLDOVER TIMES HAVE BEEN ADJUSTED TO 76 PERCENT.
NOTES
1. Ensure that the lowest operational use temperature (LOUT) is respected. Consider use of Type I fluid when Type IV fluid cannot be used.
1. Freezing mist is best confirmed by observation. It is never reported by METAR; however, it can occur when mist is present at 0 °C (32 °F) and below. 
1. Use freezing fog holdover times in conditions of ice crystals mixed with freezing fog or freezing mist.
1. To determine snowfall intensity, the Snowfall Intensities as a Function of Prevailing Visibility table (Table 57) is required. No holdover times exist if the reported visibility correlates to a “heavy” precipitation intensity.
Use snow holdover times in conditions of very light, light, or moderate snow mixed with ice crystals.
Includes light, moderate and heavy freezing drizzle. Use light freezing rain holdover times if positive identification of freezing drizzle is not possible.
These holdover times apply to conditions of “moderate” precipitation intensity. In cases of very light or light snow mixed with light rain or drizzle, use light freezing rain holdover times. The Snowfall Intensities as a Function of Prevailing Visibility table (Table 57) is required to confirm the precipitation intensity. No holdover times exist if the reported visibility correlates to a “heavy” precipitation intensity.
No holdover time guidelines exist for this condition for 0 °C (32 °F) and below.
Heavy snow, ice pellets, moderate and heavy freezing rain, small hail and hail (Table Adj-55 provides adjusted allowance times for Type IV PG fluids in ice pellets and small hail).
No holdover time guidelines exist for this condition below -10 °C (14 °F).
CAUTIONS
The cautions that apply to the holdover times in the table above can be found on page A-27.

[bookmark: _Toc231475395]Table Adj-22: Adjusted Type IV Holdover Times for 
AFLRUS LLC Green Flo Type 4
	Outside Air 
Temperature1
	Fluid 
Concentration 
Fluid/Water 
By % Volume
	Freezing Fog, Freezing Mist2, or Ice Crystals3
	Snow 
mixed with 
Freezing Fog4
	Very Light Snow, Snow Grains or Snow Pellets4,5
	Light 
Snow, Snow Grains or Snow Pellets4,5
	Moderate Snow, Snow Grains or Snow Pellets4,5
	Freezing 
Drizzle6
	Light 
Freezing Rain
	Moderate
Snow mixed with Rain7,8
	Rain on 
Cold‑Soaked Wing8
	Other9

	-3 °C and above
(27 °F and above)
	100/0
	0:57 - 1:54
	0:15 - 0:30
	1:24 - 1:43
	0:42 - 1:24
	0:19 - 0:42
	0:27 - 0:53
	0:11 - 0:23
	0:05 - 0:05
	0:06 - 0:53
	 

	
	75/25
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	 

	
	50/50
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	CAUTION: 
No holdover time 
guidelines exist

	below -3 to -8 °C
(below 27 to 18 °F)
	100/0
	0:38 - 1:58
	0:15 - 0:27
	1:12 - 1:31
	0:34 - 1:12
	0:19 - 0:34
	0:27 - 0:46
	0:15 - 0:23
	

	
	75/25
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	

	below -8 to -14 °C
(below 18 to 7 °F)
	100/0
	0:38 - 1:58
	0:11 - 0:23
	1:05 - 1:24
	0:34 - 1:05
	0:15 - 0:34
	0:27 - 0:4610
	0:15 - 0:2310
	

	
	75/25
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	

	below -14 to -18 °C
(below 7 to 0 °F)
	100/0
	0:27 - 0:53
	0:08 - 0:19
	1:01 - 1:20
	0:27 - 1:01
	0:11 - 0:27
	
	

	below -18 to -25 °C
(below 0 to -13 °F)
	100/0
	0:27 - 0:53
	0:08 - 0:19
	0:53 - 1:08
	0:23 - 0:53
	0:11 - 0:23
	
	

	below -25 to -30 °C
(below -13 to -22 °F)
	100/0
	0:19 - 0:46
	0:03 - 0:08
	0:27 - 0:30
	0:11 - 0:27
	0:05 - 0:11
	
	


THIS TABLE IS FOR USE WHEN FLAPS/SLATS ARE DEPLOYED PRIOR TO DE/ANTI-ICING. HOLDOVER TIMES HAVE BEEN ADJUSTED TO 76 PERCENT.
NOTES
1. Ensure that the lowest operational use temperature (LOUT) is respected. Consider use of Type I fluid when Type IV fluid cannot be used.
1. Freezing mist is best confirmed by observation. It is never reported by METAR; however, it can occur when mist is present at 0 °C (32 °F) and below. 
1. Use freezing fog holdover times in conditions of ice crystals mixed with freezing fog or freezing mist.
1. To determine snowfall intensity, the Snowfall Intensities as a Function of Prevailing Visibility table (Table 57) is required. No holdover times exist if the reported visibility correlates to a “heavy” precipitation intensity.
Use snow holdover times in conditions of very light, light, or moderate snow mixed with ice crystals.
Includes light, moderate and heavy freezing drizzle. Use light freezing rain holdover times if positive identification of freezing drizzle is not possible.
These holdover times apply to conditions of “moderate” precipitation intensity. In cases of very light or light snow mixed with light rain or drizzle, use light freezing rain holdover times. The Snowfall Intensities as a Function of Prevailing Visibility table (Table 57) is required to confirm the precipitation intensity. No holdover times exist if the reported visibility correlates to a “heavy” precipitation intensity.
No holdover time guidelines exist for this condition for 0 °C (32 °F) and below.
Heavy snow, ice pellets, moderate and heavy freezing rain, small hail and hail.
No holdover time guidelines exist for this condition below -10 °C (14 °F).
CAUTIONS
The cautions that apply to the holdover times in the table above can be found on page A-27.

[bookmark: _Toc231475396][bookmark: _Toc75345472][bookmark: _Toc77777038][bookmark: _Toc77777088][bookmark: _Toc105048931][bookmark: _Toc105049285][bookmark: _Toc105049408][bookmark: _Toc105399225][bookmark: _Toc105399436][bookmark: _Toc107305586][bookmark: _Toc9500358][bookmark: _Toc14166568][bookmark: _Toc14867905][bookmark: _Toc43986222][bookmark: _Toc44053688][bookmark: _Toc44054107][bookmark: _Toc45715340][bookmark: _Toc517088961][bookmark: _Toc517253618][bookmark: _Toc519674721][bookmark: _Toc519674828][bookmark: _Toc520288580][bookmark: _Toc520289452]Table Adj-23: Adjusted Type IV Holdover Times for 
ALAB International PROFLIGHT EG4
	[bookmark: _Hlk197936398]Outside Air 
Temperature1
	Fluid 
Concentration 
Fluid/Water 
By % Volume
	Freezing Fog, Freezing Mist2, or Ice Crystals3
	Snow 
mixed with 
Freezing Fog4
	Very Light Snow, Snow Grains or Snow Pellets4,5
	Light 
Snow, Snow Grains or Snow Pellets4,5
	Moderate Snow, Snow Grains or Snow Pellets4,5
	Freezing 
Drizzle6
	Light 
Freezing Rain
	Moderate
Snow mixed with Rain7,8
	Rain on 
Cold‑Soaked Wing8
	Other9

	-3 °C and above
(27 °F and above)
	100/0
	2:21 - 3:02
	0:30 - 0:57
	2:21 - 2:51
	1:12 - 2:21
	0:38 - 1:12
	1:05 - 1:31
	0:30 - 0:46
	0:06 - 0:06
	0:08 - 1:31
	 

	
	75/25
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	 

	
	50/50
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	CAUTION: 
No holdover time 
guidelines exist

	below -3 to -8 °C
(below 27 to 18 °F)
	100/0
	1:54 - 2:59
	0:30 - 0:57
	2:21 - 2:51
	1:12 - 2:21
	0:38 - 1:12
	0:49 - 1:31
	0:38 - 1:12
	

	
	75/25
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	

	below -8 to -14 °C
(below 18 to 7 °F)
	100/0
	1:54 - 2:59
	0:30 - 0:57
	2:21 - 2:51
	1:12 - 2:21
	0:38 - 1:12
	0:49 - 1:3110
	0:38 - 1:1210
	

	
	75/25
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	

	below -14 to -18 °C
(below 7 to 0 °F)
	100/0
	0:27 - 1:12
	0:23 - 0:46
	2:05 - 2:40
	1:01 - 2:05
	0:30 - 1:01
	
	

	below -18 to -25 °C
(below 0 to -13 °F)
	100/0
	0:27 - 1:12
	0:11 - 0:27
	1:08 - 1:27
	0:34 - 1:08
	0:15 - 0:34
	
	

	below -25 to -26 °C
(below -13 to -15 °F)
	100/0
	0:27 - 1:12
	0:11 - 0:23
	1:05 - 1:20
	0:30 - 1:05
	0:15 - 0:30
	
	


THIS TABLE IS FOR USE WHEN FLAPS/SLATS ARE DEPLOYED PRIOR TO DE/ANTI-ICING. HOLDOVER TIMES HAVE BEEN ADJUSTED TO 76 PERCENT.
NOTES
1. Ensure that the lowest operational use temperature (LOUT) is respected. Consider use of Type I fluid when Type IV fluid cannot be used.
1. Freezing mist is best confirmed by observation. It is never reported by METAR; however, it can occur when mist is present at 0 °C (32 °F) and below. 
1. Use freezing fog holdover times in conditions of ice crystals mixed with freezing fog or freezing mist.
1. To determine snowfall intensity, the Snowfall Intensities as a Function of Prevailing Visibility table (Table 57) is required. No holdover times exist if the reported visibility correlates to a “heavy” precipitation intensity.
Use snow holdover times in conditions of very light, light, or moderate snow mixed with ice crystals.
Includes light, moderate and heavy freezing drizzle. Use light freezing rain holdover times if positive identification of freezing drizzle is not possible.
These holdover times apply to conditions of “moderate” precipitation intensity. In cases of very light or light snow mixed with light rain or drizzle, use light freezing rain holdover times. The Snowfall Intensities as a Function of Prevailing Visibility table (Table 57) is required to confirm the precipitation intensity. No holdover times exist if the reported visibility correlates to a “heavy” precipitation intensity.
No holdover time guidelines exist for this condition for 0 °C (32 °F) and below.
Heavy snow, ice pellets, moderate and heavy freezing rain, small hail and hail.
No holdover time guidelines exist for this condition below -10 °C (14 °F).
CAUTIONS
The cautions that apply to the holdover times in the table above can be found on page A-27.

[bookmark: _Toc231475397]Table Adj-24: Adjusted Type IV Holdover Times for 
ALAB International PROFLIGHT PG4
	Outside Air 
Temperature1
	Fluid 
Concentration 
Fluid/Water 
By % Volume
	Freezing Fog, Freezing Mist2, or Ice Crystals3
	Snow 
mixed with 
Freezing Fog4
	Very Light Snow, Snow Grains or Snow Pellets4,5
	Light 
Snow, Snow Grains or Snow Pellets4,5
	Moderate Snow, Snow Grains or Snow Pellets4,5
	Freezing 
Drizzle6
	Light 
Freezing Rain
	Moderate
Snow mixed with Rain7,8
	Rain on 
Cold‑Soaked Wing8
	Other9

	-3 °C and above
(27 °F and above)
	100/0
	1:05 - 1:43
	0:23 - 0:46
	2:02 - 2:32
	1:01 - 2:02
	0:30 - 1:01
	0:49 - 1:05
	0:30 - 0:38
	0:08 - 0:08
	0:11 - 1:01
	 

	
	75/25
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	 

	
	50/50
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	CAUTION: 
No holdover time 
guidelines exist

	below -3 to -8 °C
(below 27 to 18 °F)
	100/0
	0:49 - 1:46
	0:19 - 0:38
	1:46 - 2:13
	0:53 - 1:46
	0:27 - 0:53
	0:34 - 0:53
	0:27 - 0:34
	

	
	75/25
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	

	below -8 to -14 °C
(below 18 to 7 °F)
	100/0
	0:49 - 1:46
	0:15 - 0:34
	1:35 - 1:58
	0:46 - 1:35
	0:23 - 0:46
	0:34 - 0:5310
	0:27 - 0:3410
	

	
	75/25
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	

	below -14 to -18 °C
(below 7 to 0 °F)
	100/0
	0:27 - 0:38
	0:08 - 0:19
	0:57 - 1:16
	0:27 - 0:57
	0:11 - 0:27
	
	

	below -18 to -25 °C
(below 0 to -13 °F)
	100/0
	0:27 - 0:38
	0:05 - 0:11
	0:38 - 0:46
	0:15 - 0:38
	0:07 - 0:15
	
	

	below -25 to -29 °C
(below -13 to -20 °F)
	100/0
	0:27 - 0:38
	0:04 - 0:11
	0:30 - 0:38
	0:11 - 0:30
	0:05 - 0:11
	
	


THIS TABLE IS FOR USE WHEN FLAPS/SLATS ARE DEPLOYED PRIOR TO DE/ANTI-ICING. HOLDOVER TIMES HAVE BEEN ADJUSTED TO 76 PERCENT.
NOTES
1. Ensure that the lowest operational use temperature (LOUT) is respected. Consider use of Type I fluid when Type IV fluid cannot be used.
1. Freezing mist is best confirmed by observation. It is never reported by METAR; however, it can occur when mist is present at 0 °C (32 °F) and below. 
1. Use freezing fog holdover times in conditions of ice crystals mixed with freezing fog or freezing mist.
1. To determine snowfall intensity, the Snowfall Intensities as a Function of Prevailing Visibility table (Table 57) is required. No holdover times exist if the reported visibility correlates to a “heavy” precipitation intensity.
Use snow holdover times in conditions of very light, light, or moderate snow mixed with ice crystals.
Includes light, moderate and heavy freezing drizzle. Use light freezing rain holdover times if positive identification of freezing drizzle is not possible.
These holdover times apply to conditions of “moderate” precipitation intensity. In cases of very light or light snow mixed with light rain or drizzle, use light freezing rain holdover times. The Snowfall Intensities as a Function of Prevailing Visibility table (Table 57) is required to confirm the precipitation intensity. No holdover times exist if the reported visibility correlates to a “heavy” precipitation intensity.
No holdover time guidelines exist for this condition for 0 °C (32 °F) and below.
Heavy snow, ice pellets, moderate and heavy freezing rain, small hail and hail.
No holdover time guidelines exist for this condition below -10 °C (14 °F).
CAUTIONS
The cautions that apply to the holdover times in the table above can be found on page A-27.

[bookmark: _Toc231475398]Table Adj-25: Adjusted Type IV Holdover Times for 
AllClear Clear IV Flight
	Outside Air 
Temperature1
	Fluid 
Concentration 
Fluid/Water 
By % Volume
	Freezing Fog, Freezing Mist2, or Ice Crystals3
	Snow 
mixed with 
Freezing Fog4
	Very Light Snow, Snow Grains or Snow Pellets4,5
	Light 
Snow, Snow Grains or Snow Pellets4,5
	Moderate Snow, Snow Grains or Snow Pellets4,5
	Freezing 
Drizzle6
	Light 
Freezing Rain
	Moderate
Snow mixed with Rain7,8
	Rain on 
Cold‑Soaked Wing8
	Other9

	-3 °C and above
(27 °F and above)
	100/0
	1:12 - 2:09
	0:23 - 0:46
	1:54 - 2:21
	1:01 - 1:54
	0:30 - 1:01
	0:49 - 1:20
	0:38 - 0:53
	0:11 - 0:11
	0:15 - 0:57
	 

	
	75/25
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	 

	
	50/50
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	CAUTION: 
No holdover time 
guidelines exist

	below -3 to -8 °C
(below 27 to 18 °F)
	100/0
	0:38 - 1:27
	0:19 - 0:34
	1:27 - 1:50
	0:46 - 1:27
	0:23 - 0:46
	0:38 - 1:05
	0:30 - 0:38
	

	
	75/25
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	

	below -8 to -14 °C
(below 18 to 7 °F)
	100/0
	0:38 - 1:27
	0:15 - 0:30
	1:16 - 1:31
	0:38 - 1:16
	0:19 - 0:38
	0:38 - 1:0510
	0:30 - 0:3810
	

	
	75/25
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	

	below -14 to -18 °C
(below 7 to 0 °F)
	100/0
	0:19 - 0:34
	0:08 - 0:15
	0:46 - 0:53
	0:23 - 0:46
	0:11 - 0:23
	
	

	below -18 to -23 °C
(below 0 to -9 °F)
	100/0
	0:19 - 0:34
	0:06 - 0:11
	0:30 - 0:38
	0:15 - 0:30
	0:08 - 0:15
	
	


THIS TABLE IS FOR USE WHEN FLAPS/SLATS ARE DEPLOYED PRIOR TO DE/ANTI-ICING. HOLDOVER TIMES HAVE BEEN ADJUSTED TO 76 PERCENT.
NOTES
1. Ensure that the lowest operational use temperature (LOUT) is respected. Consider use of Type I fluid when Type IV fluid cannot be used.
1. Freezing mist is best confirmed by observation. It is never reported by METAR; however, it can occur when mist is present at 0 °C (32 °F) and below. 
1. Use freezing fog holdover times in conditions of ice crystals mixed with freezing fog or freezing mist.
1. To determine snowfall intensity, the Snowfall Intensities as a Function of Prevailing Visibility table (Table 57) is required. No holdover times exist if the reported visibility correlates to a “heavy” precipitation intensity.
Use snow holdover times in conditions of very light, light, or moderate snow mixed with ice crystals.
Includes light, moderate and heavy freezing drizzle. Use light freezing rain holdover times if positive identification of freezing drizzle is not possible.
These holdover times apply to conditions of “moderate” precipitation intensity. In cases of very light or light snow mixed with light rain or drizzle, use light freezing rain holdover times. The Snowfall Intensities as a Function of Prevailing Visibility table (Table 57) is required to confirm the precipitation intensity. No holdover times exist if the reported visibility correlates to a “heavy” precipitation intensity.
No holdover time guidelines exist for this condition for 0 °C (32 °F) and below.
Heavy snow, ice pellets, moderate and heavy freezing rain, small hail and hail.
No holdover time guidelines exist for this condition below -10 °C (14 °F).
CAUTIONS
The cautions that apply to the holdover times in the table above can be found on page A-27.


[bookmark: _Toc75345473][bookmark: _Toc77777039][bookmark: _Toc77777089][bookmark: _Toc105048932][bookmark: _Toc105049286][bookmark: _Toc105049409][bookmark: _Toc105399226][bookmark: _Toc105399437][bookmark: _Toc107305587][bookmark: _Toc231475399]Table Adj-26: Adjusted Type IV Holdover Times for 
AllClear ClearWing EG
	Outside Air 
Temperature1
	Fluid 
Concentration 
Fluid/Water 
By % Volume
	Freezing Fog, Freezing Mist2, or Ice Crystals3
	Snow 
mixed with 
Freezing Fog4
	Very Light Snow, Snow Grains or Snow Pellets4,5
	Light 
Snow, Snow Grains or Snow Pellets4,5
	Moderate Snow, Snow Grains or Snow Pellets4,5
	Freezing 
Drizzle6
	Light 
Freezing Rain
	Moderate
Snow mixed with Rain7,8
	Rain on 
Cold‑Soaked Wing8
	Other9

	-3 °C and above
(27 °F and above)
	100/0
	1:24 - 2:28
	0:23 - 0:46
	2:02 - 2:32
	1:01 - 2:02
	0:30 - 1:01
	0:53 - 1:12
	0:23 - 0:46
	0:06 - 0:06
	0:08 - 1:08
	 

	
	75/25
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	 

	
	50/50
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	CAUTION: 
No holdover time 
guidelines exist

	below -3 to -8 °C
(below 27 to 18 °F)
	100/0
	1:12 - 2:51
	0:19 - 0:42
	1:50 - 2:17
	0:53 - 1:50
	0:27 - 0:53
	0:49 - 1:08
	0:23 - 0:46
	

	
	75/25
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	

	below -8 to -14 °C
(below 18 to 7 °F)
	100/0
	1:12 - 2:51
	0:19 - 0:38
	1:43 - 2:05
	0:49 - 1:43
	0:23 - 0:49
	0:49 - 1:0810
	0:23 - 0:4610
	

	
	75/25
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	

	below -14 to -18 °C
(below 7 to 0 °F)
	100/0
	0:42 - 1:31
	0:11 - 0:27
	1:12 - 1:35
	0:34 - 1:12
	0:15 - 0:34
	
	

	below -18 to -25 °C
(below 0 to -13 °F)
	100/0
	0:42 - 1:31
	0:07 - 0:15
	0:42 - 0:53
	0:19 - 0:42
	0:11 - 0:19
	
	

	below -25 to -29 °C
(below -13 to -20 °F)
	100/0
	0:42 - 1:31
	0:05 - 0:11
	0:34 - 0:42
	0:15 - 0:34
	0:08 - 0:15
	
	


THIS TABLE IS FOR USE WHEN FLAPS/SLATS ARE DEPLOYED PRIOR TO DE/ANTI-ICING. HOLDOVER TIMES HAVE BEEN ADJUSTED TO 76 PERCENT.
NOTES
1. Ensure that the lowest operational use temperature (LOUT) is respected. Consider use of Type I fluid when Type IV fluid cannot be used.
Freezing mist is best confirmed by observation. It is never reported by METAR; however, it can occur when mist is present at 0 °C (32 °F) and below. 
Use freezing fog holdover times in conditions of ice crystals mixed with freezing fog or freezing mist.
To determine snowfall intensity, the Snowfall Intensities as a Function of Prevailing Visibility table (Table 57) is required. No holdover times exist if the reported visibility correlates to a “heavy” precipitation intensity.
Use snow holdover times in conditions of very light, light, or moderate snow mixed with ice crystals.
Includes light, moderate and heavy freezing drizzle. Use light freezing rain holdover times if positive identification of freezing drizzle is not possible.
These holdover times apply to conditions of “moderate” precipitation intensity. In cases of very light or light snow mixed with light rain or drizzle, use light freezing rain holdover times. The Snowfall Intensities as a Function of Prevailing Visibility table (Table 57) is required to confirm the precipitation intensity. No holdover times exist if the reported visibility correlates to a “heavy” precipitation intensity.
No holdover time guidelines exist for this condition for 0 °C (32 °F) and below.
Heavy snow, ice pellets, moderate and heavy freezing rain, small hail and hail (Table Adj-54 provides adjusted allowance times for Type IV EG fluids in ice pellets and small hail).
No holdover time guidelines exist for this condition below -10 °C (14 °F).
CAUTIONS
The cautions that apply to the holdover times in the table above can be found on page A-27. 
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ASGlobal 4Flite EG
	Outside Air 
Temperature1
	Fluid 
Concentration 
Fluid/Water 
By % Volume
	Freezing Fog, Freezing Mist2, or Ice Crystals3
	Snow 
mixed with 
Freezing Fog4
	Very Light Snow, Snow Grains or Snow Pellets4,5
	Light 
Snow, Snow Grains or Snow Pellets4,5
	Moderate Snow, Snow Grains or Snow Pellets4,5
	Freezing 
Drizzle6
	Light 
Freezing Rain
	Moderate
Snow mixed with Rain7,8
	Rain on 
Cold‑Soaked Wing8
	Other9

	-3 °C and above
(27 °F and above)
	100/0
	1:12 - 2:28
	0:19 - 0:34
	1:35 - 1:58
	0:46 - 1:35
	0:23 - 0:46
	0:30 - 0:53
	0:15 - 0:27
	0:05 - 0:05
	0:06 - 0:49
	 

	
	75/25
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	 

	
	50/50
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	CAUTION: 
No holdover time 
guidelines exist

	below -3 to -8 °C
(below 27 to 18 °F)
	100/0
	1:05 - 2:05
	0:15 - 0:30
	1:24 - 1:43
	0:42 - 1:24
	0:19 - 0:42
	0:30 - 0:53
	0:15 - 0:27
	

	
	75/25
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	

	below -8 to -14 °C
(below 18 to 7 °F)
	100/0
	1:05 - 2:05
	0:15 - 0:27
	1:12 - 1:31
	0:38 - 1:12
	0:19 - 0:38
	0:30 - 0:5310
	0:15 - 0:2710
	

	
	75/25
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	

	below -14 to -18 °C
(below 7 to 0 °F)
	100/0
	0:38 - 1:05
	0:11 - 0:27
	1:12 - 1:31
	0:34 - 1:12
	0:15 - 0:34
	
	

	below -18 to -25 °C
(below 0 to -13 °F)
	100/0
	0:38 - 1:05
	0:11 - 0:23
	1:01 - 1:16
	0:27 - 1:01
	0:15 - 0:27
	
	

	below -25 to -30 °C
(below -13 to -22 °F)
	100/0
	0:23 - 0:49
	0:07 - 0:15
	0:42 - 0:49
	0:19 - 0:42
	0:08 - 0:19
	
	


THIS TABLE IS FOR USE WHEN FLAPS/SLATS ARE DEPLOYED PRIOR TO DE/ANTI-ICING. HOLDOVER TIMES HAVE BEEN ADJUSTED TO 76 PERCENT.
NOTES
1. Ensure that the lowest operational use temperature (LOUT) is respected. Consider use of Type I fluid when Type IV fluid cannot be used.
1. Freezing mist is best confirmed by observation. It is never reported by METAR; however, it can occur when mist is present at 0 °C (32 °F) and below. 
1. Use freezing fog holdover times in conditions of ice crystals mixed with freezing fog or freezing mist.
1. To determine snowfall intensity, the Snowfall Intensities as a Function of Prevailing Visibility table (Table 57) is required. No holdover times exist if the reported visibility correlates to a “heavy” precipitation intensity.
Use snow holdover times in conditions of very light, light, or moderate snow mixed with ice crystals.
Includes light, moderate and heavy freezing drizzle. Use light freezing rain holdover times if positive identification of freezing drizzle is not possible.
These holdover times apply to conditions of “moderate” precipitation intensity. In cases of very light or light snow mixed with light rain or drizzle, use light freezing rain holdover times. The Snowfall Intensities as a Function of Prevailing Visibility table (Table 57) is required to confirm the precipitation intensity. No holdover times exist if the reported visibility correlates to a “heavy” precipitation intensity.
No holdover time guidelines exist for this condition for 0 °C (32 °F) and below.
Heavy snow, ice pellets, moderate and heavy freezing rain, small hail and hail.
No holdover time guidelines exist for this condition below -10 °C (14 °F).
CAUTIONS
The cautions that apply to the holdover times in the table above can be found on page A-27. 
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ASGlobal 4Flite PG
	Outside Air 
Temperature1
	Fluid 
Concentration 
Fluid/Water 
By % Volume
	Freezing Fog, Freezing Mist2, or Ice Crystals3
	Snow 
mixed with 
Freezing Fog4
	Very Light Snow, Snow Grains or Snow Pellets4,5
	Light 
Snow, Snow Grains or Snow Pellets4,5
	Moderate Snow, Snow Grains or Snow Pellets4,5
	Freezing 
Drizzle6
	Light 
Freezing Rain
	Moderate
Snow mixed with Rain7,8
	Rain on 
Cold‑Soaked Wing8
	Other9

	-3 °C and above
(27 °F and above)
	100/0
	1:24 - 2:28
	0:30 - 0:53
	2:09 - 2:36
	1:12 - 2:09
	0:38 - 1:12
	0:53 - 1:12
	0:34 - 0:49
	0:11 - 0:11
	0:11 - 1:01
	 

	
	75/25
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	 

	
	50/50
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	CAUTION: 
No holdover time 
guidelines exist

	below -3 to -8 °C
(below 27 to 18 °F)
	100/0
	0:49 - 1:27
	0:23 - 0:38
	1:35 - 1:54
	0:53 - 1:35
	0:27 - 0:53
	0:42 - 0:53
	0:27 - 0:42
	

	
	75/25
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	

	below -8 to -14 °C
(below 18 to 7 °F)
	100/0
	0:49 - 1:27
	0:15 - 0:30
	1:16 - 1:31
	0:42 - 1:16
	0:23 - 0:42
	0:42 - 0:5310
	0:27 - 0:4210
	

	
	75/25
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	

	below -14 to -18 °C
(below 7 to 0 °F)
	100/0
	0:23 - 0:34
	0:11 - 0:19
	0:49 - 1:01
	0:27 - 0:49
	0:11 - 0:27
	
	

	below -18 to -25 °C
(below 0 to -13 °F)
	100/0
	0:23 - 0:34
	0:05 - 0:11
	0:27 - 0:34
	0:15 - 0:27
	0:07 - 0:15
	
	

	below -25 to -26 °C
(below -13 to -15 °F)
	100/0
	0:23 - 0:34
	0:05 - 0:11
	0:27 - 0:34
	0:15 - 0:27
	0:06 - 0:15
	
	


THIS TABLE IS FOR USE WHEN FLAPS/SLATS ARE DEPLOYED PRIOR TO DE/ANTI-ICING. HOLDOVER TIMES HAVE BEEN ADJUSTED TO 76 PERCENT.
NOTES
1. Ensure that the lowest operational use temperature (LOUT) is respected. Consider use of Type I fluid when Type IV fluid cannot be used.
1. Freezing mist is best confirmed by observation. It is never reported by METAR; however, it can occur when mist is present at 0 °C (32 °F) and below. 
1. Use freezing fog holdover times in conditions of ice crystals mixed with freezing fog or freezing mist.
1. To determine snowfall intensity, the Snowfall Intensities as a Function of Prevailing Visibility table (Table 57) is required. No holdover times exist if the reported visibility correlates to a “heavy” precipitation intensity.
Use snow holdover times in conditions of very light, light, or moderate snow mixed with ice crystals.
Includes light, moderate and heavy freezing drizzle. Use light freezing rain holdover times if positive identification of freezing drizzle is not possible.
These holdover times apply to conditions of “moderate” precipitation intensity. In cases of very light or light snow mixed with light rain or drizzle, use light freezing rain holdover times. The Snowfall Intensities as a Function of Prevailing Visibility table (Table 57) is required to confirm the precipitation intensity. No holdover times exist if the reported visibility correlates to a “heavy” precipitation intensity.
No holdover time guidelines exist for this condition for 0 °C (32 °F) and below.
Heavy snow, ice pellets, moderate and heavy freezing rain, small hail and hail (Table Adj-55 provides adjusted allowance times for Type IV PG fluids in ice pellets and small hail).
No holdover time guidelines exist for this condition below -10 °C (14 °F).
CAUTIONS
The cautions that apply to the holdover times in the table above can be found on page A-27.

[bookmark: _Toc75345477][bookmark: _Toc77777043][bookmark: _Toc77777093][bookmark: _Toc105048936][bookmark: _Toc105049290][bookmark: _Toc105049413][bookmark: _Toc105399230][bookmark: _Toc105399441][bookmark: _Toc107305591][bookmark: _Toc231475402]Table Adj-29: Adjusted Type IV Holdover Times for 
AVIAFLUID AVIAFlight PG
	Outside Air 
Temperature1
	Fluid 
Concentration 
Fluid/Water 
By % Volume
	Freezing Fog, Freezing Mist2, or Ice Crystals3
	Snow 
mixed with 
Freezing Fog4
	Very Light Snow, Snow Grains or Snow Pellets4,5
	Light 
Snow, Snow Grains or Snow Pellets4,5
	Moderate Snow, Snow Grains or Snow Pellets4,5
	Freezing 
Drizzle6
	Light 
Freezing Rain
	Moderate
Snow mixed with Rain7,8
	Rain on 
Cold‑Soaked Wing8
	Other9

	-3 °C and above
(27 °F and above)
	100/0
	1:43 - 3:02
	0:30 - 0:57
	2:17 - 2:47
	1:16 - 2:17
	0:42 - 1:16
	1:31 - 1:31
	0:53 - 1:27
	0:11 - 0:11
	0:15 - 1:31
	 

	
	75/25
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	 

	
	50/50
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	CAUTION: 
No holdover time 
guidelines exist

	below -3 to -8 °C
(below 27 to 18 °F)
	100/0
	0:49 - 1:39
	0:19 - 0:38
	1:31 - 1:50
	0:49 - 1:31
	0:27 - 0:49
	0:27 - 1:27
	0:34 - 0:49
	

	
	75/25
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	

	below -8 to -14 °C
(below 18 to 7 °F)
	100/0
	0:49 - 1:39
	0:15 - 0:27
	1:08 - 1:24
	0:38 - 1:08
	0:19 - 0:38
	0:27 - 1:2710
	0:34 - 0:4910
	

	
	75/25
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	

	below -14 to -18 °C
(below 7 to 0 °F)
	100/0
	0:15 - 0:27
	0:08 - 0:15
	0:38 - 0:46
	0:19 - 0:38
	0:11 - 0:19
	
	

	below -18 to -25 °C
(below 0 to -13 °F)
	100/0
	0:15 - 0:27
	0:04 - 0:07
	0:19 - 0:23
	0:11 - 0:19
	0:05 - 0:11
	
	

	below -25 to -25.5 °C
(below -13 to -14 °F)
	100/0
	0:15 - 0:27
	0:04 - 0:07
	0:19 - 0:23
	0:08 - 0:19
	0:05 - 0:08
	
	


THIS TABLE IS FOR USE WHEN FLAPS/SLATS ARE DEPLOYED PRIOR TO DE/ANTI-ICING. HOLDOVER TIMES HAVE BEEN ADJUSTED TO 76 PERCENT.
NOTES
1. Ensure that the lowest operational use temperature (LOUT) is respected. Consider use of Type I fluid when Type IV fluid cannot be used.
1. Freezing mist is best confirmed by observation. It is never reported by METAR; however, it can occur when mist is present at 0 °C (32 °F) and below. 
1. Use freezing fog holdover times in conditions of ice crystals mixed with freezing fog or freezing mist.
1. To determine snowfall intensity, the Snowfall Intensities as a Function of Prevailing Visibility table (Table 57) is required. No holdover times exist if the reported visibility correlates to a “heavy” precipitation intensity.
Use snow holdover times in conditions of very light, light, or moderate snow mixed with ice crystals.
Includes light, moderate and heavy freezing drizzle. Use light freezing rain holdover times if positive identification of freezing drizzle is not possible.
These holdover times apply to conditions of “moderate” precipitation intensity. In cases of very light or light snow mixed with light rain or drizzle, use light freezing rain holdover times. The Snowfall Intensities as a Function of Prevailing Visibility table (Table 57) is required to confirm the precipitation intensity. No holdover times exist if the reported visibility correlates to a “heavy” precipitation intensity.
No holdover time guidelines exist for this condition for 0 °C (32 °F) and below.
Heavy snow, ice pellets, moderate and heavy freezing rain, small hail and hail (Table Adj-55 provides adjusted allowance times for Type IV PG fluids in ice pellets and small hail).
No holdover time guidelines exist for this condition below -10 °C (14 °F).
CAUTIONS
The cautions that apply to the holdover times in the table above can be found on page A-27.
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CHEMCO ChemR EG IV
	Outside Air 
Temperature1
	Fluid 
Concentration 
Fluid/Water 
By % Volume
	Freezing Fog, Freezing Mist2, or Ice Crystals3
	Snow 
mixed with 
Freezing Fog4
	Very Light Snow, Snow Grains or Snow Pellets4,5
	Light 
Snow, Snow Grains or Snow Pellets4,5
	Moderate Snow, Snow Grains or Snow Pellets4,5
	Freezing 
Drizzle6
	Light 
Freezing Rain
	Moderate
Snow mixed with Rain7,8
	Rain on 
Cold‑Soaked Wing8
	Other9

	-3 °C and above
(27 °F and above)
	100/0
	1:35 - 2:43
	0:15 - 0:38
	1:50 - 2:24
	0:49 - 1:50
	0:23 - 0:49
	0:34 - 1:16
	0:19 - 0:30
	0:05 - 0:05
	0:07 - 1:20
	 

	
	75/25
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	 

	
	50/50
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	CAUTION: 
No holdover time 
guidelines exist

	below -3 to -8 °C
(below 27 to 18 °F)
	100/0
	1:05 - 2:47
	0:15 - 0:38
	1:50 - 2:24
	0:49 - 1:50
	0:23 - 0:49
	0:46 - 1:12
	0:27 - 0:38
	

	
	75/25
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	

	below -8 to -14 °C
(below 18 to 7 °F)
	100/0
	1:05 - 2:47
	0:15 - 0:38
	1:50 - 2:24
	0:49 - 1:50
	0:23 - 0:49
	0:46 - 1:1210
	0:27 - 0:3810
	

	
	75/25
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	

	below -14 to -18 °C
(below 7 to 0 °F)
	100/0
	0:30 - 1:05
	0:08 - 0:19
	0:49 - 1:05
	0:27 - 0:49
	0:11 - 0:27
	
	

	below -18 to -25 °C
(below 0 to -13 °F)
	100/0
	0:30 - 1:05
	0:08 - 0:19
	0:49 - 1:05
	0:27 - 0:49
	0:11 - 0:27
	
	

	below -25 to -27 °C
(below -13 to -17 °F)
	100/0
	0:30 - 1:05
	0:08 - 0:19
	0:49 - 1:05
	0:27 - 0:49
	0:11 - 0:27
	
	


THIS TABLE IS FOR USE WHEN FLAPS/SLATS ARE DEPLOYED PRIOR TO DE/ANTI-ICING. HOLDOVER TIMES HAVE BEEN ADJUSTED TO 76 PERCENT.
NOTES
1. Ensure that the lowest operational use temperature (LOUT) is respected. Consider use of Type I fluid when Type IV fluid cannot be used.
1. Freezing mist is best confirmed by observation. It is never reported by METAR; however, it can occur when mist is present at 0 °C (32 °F) and below. 
1. Use freezing fog holdover times in conditions of ice crystals mixed with freezing fog or freezing mist.
1. To determine snowfall intensity, the Snowfall Intensities as a Function of Prevailing Visibility table (Table 57) is required. No holdover times exist if the reported visibility correlates to a “heavy” precipitation intensity.
Use snow holdover times in conditions of very light, light, or moderate snow mixed with ice crystals.
Includes light, moderate and heavy freezing drizzle. Use light freezing rain holdover times if positive identification of freezing drizzle is not possible.
These holdover times apply to conditions of “moderate” precipitation intensity. In cases of very light or light snow mixed with light rain or drizzle, use light freezing rain holdover times. The Snowfall Intensities as a Function of Prevailing Visibility table (Table 57) is required to confirm the precipitation intensity. No holdover times exist if the reported visibility correlates to a “heavy” precipitation intensity.
No holdover time guidelines exist for this condition for 0 °C (32 °F) and below.
Heavy snow, ice pellets, moderate and heavy freezing rain, small hail and hail (Table Adj-54 provides adjusted allowance times for Type IV EG fluids in ice pellets and small hail).
No holdover time guidelines exist for this condition below -10 °C (14 °F).
CAUTIONS
The cautions that apply to the holdover times in the table above can be found on page A-27.
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CHEMCO ChemR Nordik IV
	Outside Air 
Temperature1
	Fluid 
Concentration 
Fluid/Water 
By % Volume
	Freezing Fog, Freezing Mist2, or Ice Crystals3
	Snow 
mixed with 
Freezing Fog4
	Very Light Snow, Snow Grains or Snow Pellets4,5
	Light 
Snow, Snow Grains or Snow Pellets4,5
	Moderate Snow, Snow Grains or Snow Pellets4,5
	Freezing 
Drizzle6
	Light 
Freezing Rain
	Moderate
Snow mixed with Rain7,8
	Rain on 
Cold‑Soaked Wing8
	Other9

	-3 °C and above
(27 °F and above)
	100/0
	1:43 - 3:02
	0:27 - 0:53
	2:09 - 2:40
	1:08 - 2:09
	0:38 - 1:08
	1:01 - 1:31
	0:42 - 1:01
	0:11 - 0:11
	0:19 - 1:31
	 

	
	75/25
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	 

	
	50/50
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	CAUTION: 
No holdover time 
guidelines exist

	below -3 to -8 °C
(below 27 to 18 °F)
	100/0
	1:24 - 3:02
	0:27 - 0:53
	2:09 - 2:40
	1:08 - 2:09
	0:38 - 1:08
	0:57 - 1:31
	0:34 - 1:01
	

	
	75/25
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	

	below -8 to -14 °C
(below 18 to 7 °F)
	100/0
	1:24 - 3:02
	0:27 - 0:53
	2:09 - 2:40
	1:08 - 2:09
	0:38 - 1:08
	0:57 - 1:3110
	0:34 - 1:0110
	

	
	75/25
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	

	below -14 to -18 °C
(below 7 to 0 °F)
	100/0
	0:30 - 1:08
	0:27 - 0:53
	2:21 - 2:51
	1:12 - 2:21
	0:38 - 1:12
	
	

	below -18 to -25 °C
(below 0 to -13 °F)
	100/0
	0:30 - 1:08
	0:19 - 0:38
	1:39 - 2:02
	0:49 - 1:39
	0:27 - 0:49
	
	

	below -25 to -29 °C
(below -13 to -20 °F)
	100/0
	0:30 - 1:08
	0:15 - 0:30
	1:24 - 1:43
	0:42 - 1:24
	0:23 - 0:42
	
	


THIS TABLE IS FOR USE WHEN FLAPS/SLATS ARE DEPLOYED PRIOR TO DE/ANTI-ICING. HOLDOVER TIMES HAVE BEEN ADJUSTED TO 76 PERCENT.
NOTES
1. Ensure that the lowest operational use temperature (LOUT) is respected. Consider use of Type I fluid when Type IV fluid cannot be used.
1. Freezing mist is best confirmed by observation. It is never reported by METAR; however, it can occur when mist is present at 0 °C (32 °F) and below. 
1. Use freezing fog holdover times in conditions of ice crystals mixed with freezing fog or freezing mist.
1. To determine snowfall intensity, the Snowfall Intensities as a Function of Prevailing Visibility table (Table 57) is required. No holdover times exist if the reported visibility correlates to a “heavy” precipitation intensity.
Use snow holdover times in conditions of very light, light, or moderate snow mixed with ice crystals.
Includes light, moderate and heavy freezing drizzle. Use light freezing rain holdover times if positive identification of freezing drizzle is not possible.
These holdover times apply to conditions of “moderate” precipitation intensity. In cases of very light or light snow mixed with light rain or drizzle, use light freezing rain holdover times. The Snowfall Intensities as a Function of Prevailing Visibility table (Table 57) is required to confirm the precipitation intensity. No holdover times exist if the reported visibility correlates to a “heavy” precipitation intensity.
No holdover time guidelines exist for this condition for 0 °C (32 °F) and below.
Heavy snow, ice pellets, moderate and heavy freezing rain, small hail and hail (Table Adj-54 provides adjusted allowance times for Type IV EG fluids in ice pellets and small hail).
No holdover time guidelines exist for this condition below -10 °C (14 °F).
CAUTIONS
The cautions that apply to the holdover times in the table above can be found on page A-27.
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Chongqing Joba Chemical FW-IV
	Outside Air 
Temperature1
	Fluid 
Concentration 
Fluid/Water 
By % Volume
	Freezing Fog, Freezing Mist2, or Ice Crystals3
	Snow 
mixed with 
Freezing Fog4
	Very Light Snow, Snow Grains or Snow Pellets4,5
	Light 
Snow, Snow Grains or Snow Pellets4,5
	Moderate Snow, Snow Grains or Snow Pellets4,5
	Freezing 
Drizzle6
	Light 
Freezing Rain
	Moderate
Snow mixed with Rain7,8
	Rain on 
Cold‑Soaked Wing8
	Other9

	-3 °C and above
(27 °F and above)
	100/0
	2:28 - 3:02
	0:27 - 0:57
	2:28 - 3:00
	1:16 - 2:28
	0:38 - 1:16
	1:08 - 1:31
	0:34 - 0:49
	0:08 - 0:08
	0:11 - 1:31
	 

	
	75/25
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	 

	
	50/50
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	CAUTION: 
No holdover time 
guidelines exist

	below -3 to -8 °C
(below 27 to 18 °F)
	100/0
	1:54 - 3:02
	0:23 - 0:46
	2:05 - 2:36
	1:05 - 2:05
	0:30 - 1:05
	0:38 - 1:31
	0:27 - 0:53
	

	
	75/25
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	

	below -8 to -14 °C
(below 18 to 7 °F)
	100/0
	1:54 - 3:02
	0:23 - 0:42
	1:50 - 2:17
	0:57 - 1:50
	0:27 - 0:57
	0:38 - 1:3110
	0:27 - 0:5310
	

	
	75/25
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	

	below -14 to -18 °C
(below 7 to 0 °F)
	100/0
	0:27 - 1:16
	0:15 - 0:30
	1:31 - 1:58
	0:42 - 1:31
	0:19 - 0:42
	
	

	below -18 to -25 °C
(below 0 to -13 °F)
	100/0
	0:27 - 1:16
	0:11 - 0:23
	1:01 - 1:20
	0:27 - 1:01
	0:11 - 0:27
	
	

	below -25 to -29 °C
(below -13 to -20 °F)
	100/0
	0:27 - 1:16
	0:08 - 0:19
	0:53 - 1:08
	0:23 - 0:53
	0:11 - 0:23
	
	


THIS TABLE IS FOR USE WHEN FLAPS/SLATS ARE DEPLOYED PRIOR TO DE/ANTI-ICING. HOLDOVER TIMES HAVE BEEN ADJUSTED TO 76 PERCENT.
NOTES
1. Ensure that the lowest operational use temperature (LOUT) is respected. Consider use of Type I fluid when Type IV fluid cannot be used.
1. Freezing mist is best confirmed by observation. It is never reported by METAR; however, it can occur when mist is present at 0 °C (32 °F) and below. 
1. Use freezing fog holdover times in conditions of ice crystals mixed with freezing fog or freezing mist.
1. To determine snowfall intensity, the Snowfall Intensities as a Function of Prevailing Visibility table (Table 57) is required. No holdover times exist if the reported visibility correlates to a “heavy” precipitation intensity.
Use snow holdover times in conditions of very light, light, or moderate snow mixed with ice crystals.
Includes light, moderate and heavy freezing drizzle. Use light freezing rain holdover times if positive identification of freezing drizzle is not possible.
These holdover times apply to conditions of “moderate” precipitation intensity. In cases of very light or light snow mixed with light rain or drizzle, use light freezing rain holdover times. The Snowfall Intensities as a Function of Prevailing Visibility table (Table 57) is required to confirm the precipitation intensity. No holdover times exist if the reported visibility correlates to a “heavy” precipitation intensity.
No holdover time guidelines exist for this condition for 0 °C (32 °F) and below.
Heavy snow, ice pellets, moderate and heavy freezing rain, small hail and hail (Table Adj-54 provides adjusted allowance times for Type IV EG fluids in ice pellets and small hail).
No holdover time guidelines exist for this condition below -10 °C (14 °F).
CAUTIONS
The cautions that apply to the holdover times in the table above can be found on page A-27.
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Clariant Safewing MP IV LAUNCH
	Outside Air 
Temperature1
	Fluid 
Concentration 
Fluid/Water 
By % Volume
	Freezing Fog, Freezing Mist2, or Ice Crystals3
	Snow 
mixed with 
Freezing Fog4
	Very Light Snow, Snow Grains or Snow Pellets4,5
	Light 
Snow, Snow Grains or Snow Pellets4,5
	Moderate Snow, Snow Grains or Snow Pellets4,5
	Freezing 
Drizzle6
	Light 
Freezing Rain
	Moderate
Snow mixed with Rain7,8
	Rain on 
Cold‑Soaked Wing8
	Other9

	-3 °C and above
(27 °F and above)
	100/0
	3:02 - 3:02
	0:38 - 1:01
	2:09 - 2:32
	1:20 - 2:09
	0:49 - 1:20
	1:08 - 1:31
	0:46 - 1:16
	0:08 - 0:08
	0:11 - 1:16
	 

	
	75/25
	2:47 - 3:02
	0:34 - 1:01
	2:21 - 2:47
	1:20 - 2:21
	0:46 - 1:20
	1:16 - 1:31
	0:34 - 0:57
	0:06 - 0:06
	0:08 - 1:20
	 

	
	50/50
	1:05 - 2:05
	0:15 - 0:27
	1:05 - 1:16
	0:34 - 1:05
	0:19 - 0:34
	0:23 - 0:38
	0:15 - 0:19
	CAUTION: 
No holdover time 
guidelines exist

	below -3 to -8 °C
(below 27 to 18 °F)
	100/0
	0:46 - 1:27
	0:30 - 0:49
	1:50 - 2:09
	1:08 - 1:50
	0:42 - 1:08
	0:27 - 1:16
	0:19 - 0:34
	

	
	75/25
	0:30 - 1:01
	0:30 - 0:53
	2:02 - 2:28
	1:08 - 2:02
	0:38 - 1:08
	0:19 - 0:53
	0:19 - 0:34
	

	below -8 to -14 °C
(below 18 to 7 °F)
	100/0
	0:46 - 1:27
	0:27 - 0:46
	1:39 - 1:54
	1:01 - 1:39
	0:38 - 1:01
	0:27 - 1:1610
	0:19 - 0:3410
	

	
	75/25
	0:30 - 1:01
	0:27 - 0:46
	1:50 - 2:13
	1:05 - 1:50
	0:34 - 1:05
	0:19 - 0:5310
	0:19 - 0:3410
	

	below -14 to -18 °C
(below 7 to 0 °F)
	100/0
	0:23 - 0:38
	0:04 - 0:11
	0:57 - 1:20
	0:15 - 0:57
	0:05 - 0:15
	
	

	below -18 to -25 °C
(below 0 to -13 °F)
	100/0
	0:23 - 0:38
	0:02 - 0:05
	0:23 - 0:34
	0:07 - 0:23
	0:02 - 0:07
	
	

	below -25 to -28.5 °C
(below -13 to -19 °F)
	100/0
	0:23 - 0:38
	0:01 - 0:03
	0:15 - 0:23
	0:05 - 0:15
	0:01 - 0:05
	
	


THIS TABLE IS FOR USE WHEN FLAPS/SLATS ARE DEPLOYED PRIOR TO DE/ANTI-ICING. HOLDOVER TIMES HAVE BEEN ADJUSTED TO 76 PERCENT.
NOTES
1. Ensure that the lowest operational use temperature (LOUT) is respected. Consider use of Type I fluid when Type IV fluid cannot be used.
1. Freezing mist is best confirmed by observation. It is never reported by METAR; however, it can occur when mist is present at 0 °C (32 °F) and below. 
1. Use freezing fog holdover times in conditions of ice crystals mixed with freezing fog or freezing mist.
1. To determine snowfall intensity, the Snowfall Intensities as a Function of Prevailing Visibility table (Table 57) is required. No holdover times exist if the reported visibility correlates to a “heavy” precipitation intensity.
Use snow holdover times in conditions of very light, light, or moderate snow mixed with ice crystals.
Includes light, moderate and heavy freezing drizzle. Use light freezing rain holdover times if positive identification of freezing drizzle is not possible.
These holdover times apply to conditions of “moderate” precipitation intensity. In cases of very light or light snow mixed with light rain or drizzle, use light freezing rain holdover times. The Snowfall Intensities as a Function of Prevailing Visibility table (Table 57) is required to confirm the precipitation intensity. No holdover times exist if the reported visibility correlates to a “heavy” precipitation intensity.
No holdover time guidelines exist for this condition for 0 °C (32 °F) and below.
Heavy snow, ice pellets, moderate and heavy freezing rain, small hail and hail (Table Adj-55 provides adjusted allowance times for Type IV PG fluids in ice pellets and small hail).
No holdover time guidelines exist for this condition below -10 °C (14 °F).
CAUTIONS
The cautions that apply to the holdover times in the table above can be found on page A-27.
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Clariant Safewing MP IV LAUNCH PLUS
	Outside Air 
Temperature1
	Fluid 
Concentration 
Fluid/Water 
By % Volume
	Freezing Fog, Freezing Mist2, or Ice Crystals3
	Snow 
mixed with 
Freezing Fog4
	Very Light Snow, Snow Grains or Snow Pellets4,5
	Light 
Snow, Snow Grains or Snow Pellets4,5
	Moderate Snow, Snow Grains or Snow Pellets4,5
	Freezing 
Drizzle6
	Light 
Freezing Rain
	Moderate
Snow mixed with Rain7,8
	Rain on 
Cold‑Soaked Wing8
	Other9

	-3 °C and above
(27 °F and above)
	100/0
	2:59 - 3:02
	0:30 - 1:12
	3:00 - 3:00
	1:35 - 3:00
	0:42 - 1:35
	1:31 - 1:31
	0:46 - 1:31
	0:11 - 0:11
	0:15 - 1:31
	 

	
	75/25
	2:59 - 3:02
	0:27 - 1:05
	3:00 - 3:00
	1:27 - 3:00
	0:38 - 1:27
	1:31 - 1:31
	1:01 - 1:05
	0:11 - 0:11
	0:15 - 1:24
	 

	
	50/50
	0:57 - 1:24
	0:11 - 0:27
	1:12 - 1:31
	0:34 - 1:12
	0:15 - 0:34
	0:19 - 0:46
	0:11 - 0:15
	CAUTION: 
No holdover time 
guidelines exist

	below -3 to -8 °C
(below 27 to 18 °F)
	100/0
	0:42 - 1:43
	0:27 - 0:57
	2:51 - 3:00
	1:16 - 2:51
	0:34 - 1:16
	0:19 - 1:12
	0:19 - 0:30
	

	
	75/25
	0:30 - 1:31
	0:23 - 0:49
	2:40 - 3:00
	1:08 - 2:40
	0:27 - 1:08
	0:15 - 0:49
	0:15 - 0:23
	

	below -8 to -14 °C
(below 18 to 7 °F)
	100/0
	0:42 - 1:43
	0:23 - 0:49
	2:28 - 3:00
	1:05 - 2:28
	0:30 - 1:05
	0:19 - 1:1210
	0:19 - 0:3010
	

	
	75/25
	0:30 - 1:31
	0:19 - 0:42
	2:13 - 2:55
	0:57 - 2:13
	0:23 - 0:57
	0:15 - 0:4910
	0:15 - 0:2310
	

	below -14 to -18 °C
(below 7 to 0 °F)
	100/0
	0:19 - 0:38
	0:04 - 0:15
	0:57 - 1:24
	0:19 - 0:57
	0:05 - 0:19
	
	

	below -18 to -25 °C
(below 0 to -13 °F)
	100/0
	0:19 - 0:38
	0:02 - 0:05
	0:23 - 0:34
	0:07 - 0:23
	0:02 - 0:07
	
	

	below -25 to -29 °C
(below -13 to -20 °F)
	100/0
	0:19 - 0:38
	0:01 - 0:03
	0:15 - 0:23
	0:05 - 0:15
	0:02 - 0:05
	
	


THIS TABLE IS FOR USE WHEN FLAPS/SLATS ARE DEPLOYED PRIOR TO DE/ANTI-ICING. HOLDOVER TIMES HAVE BEEN ADJUSTED TO 76 PERCENT.
NOTES
1. Ensure that the lowest operational use temperature (LOUT) is respected. Consider use of Type I fluid when Type IV fluid cannot be used.
1. Freezing mist is best confirmed by observation. It is never reported by METAR; however, it can occur when mist is present at 0 °C (32 °F) and below. 
1. Use freezing fog holdover times in conditions of ice crystals mixed with freezing fog or freezing mist.
1. To determine snowfall intensity, the Snowfall Intensities as a Function of Prevailing Visibility table (Table 57) is required. No holdover times exist if the reported visibility correlates to a “heavy” precipitation intensity.
Use snow holdover times in conditions of very light, light, or moderate snow mixed with ice crystals.
Includes light, moderate and heavy freezing drizzle. Use light freezing rain holdover times if positive identification of freezing drizzle is not possible.
These holdover times apply to conditions of “moderate” precipitation intensity. In cases of very light or light snow mixed with light rain or drizzle, use light freezing rain holdover times. The Snowfall Intensities as a Function of Prevailing Visibility table (Table 57) is required to confirm the precipitation intensity. No holdover times exist if the reported visibility correlates to a “heavy” precipitation intensity.
No holdover time guidelines exist for this condition for 0 °C (32 °F) and below.
Heavy snow, ice pellets, moderate and heavy freezing rain, small hail and hail (Table Adj-55 provides adjusted allowance times for Type IV PG fluids in ice pellets and small hail).
No holdover time guidelines exist for this condition below -10 °C (14 °F).
CAUTIONS
The cautions that apply to the holdover times in the table above can be found on page A-27.
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Cryotech Polar Guard® Advance
	Outside Air 
Temperature1
	Fluid 
Concentration 
Fluid/Water 
By % Volume
	Freezing Fog, Freezing Mist2, or Ice Crystals3
	Snow 
mixed with 
Freezing Fog4
	Very Light Snow, Snow Grains or Snow Pellets4,5
	Light 
Snow, Snow Grains or Snow Pellets4,5
	Moderate Snow, Snow Grains or Snow Pellets4,5
	Freezing 
Drizzle6
	Light 
Freezing Rain
	Moderate
Snow mixed with Rain7,8
	Rain on 
Cold‑Soaked Wing8
	Other9

	-3 °C and above
(27 °F and above)
	100/0
	2:09 - 3:02
	0:38 - 1:05
	2:28 - 2:59
	1:27 - 2:28
	0:49 - 1:27
	1:12 - 1:31
	0:57 - 1:08
	0:08 - 0:08
	0:11 - 1:31
	 

	
	75/25
	1:54 - 3:02
	0:23 - 0:49
	2:17 - 2:55
	1:05 - 2:17
	0:30 - 1:05
	1:16 - 1:31
	0:30 - 0:53
	0:05 - 0:05
	0:07 - 1:16
	 

	
	50/50
	0:38 - 1:05
	0:05 - 0:15
	0:53 - 1:12
	0:19 - 0:53
	0:08 - 0:19
	0:15 - 0:34
	0:07 - 0:15
	CAUTION: 
No holdover time 
guidelines exist

	below -3 to -8 °C
(below 27 to 18 °F)
	100/0
	0:42 - 1:54
	0:27 - 0:49
	1:50 - 2:09
	1:05 - 1:50
	0:38 - 1:05
	0:27 - 1:12
	0:27 - 0:34
	

	
	75/25
	0:30 - 1:08
	0:19 - 0:38
	1:46 - 2:17
	0:49 - 1:46
	0:23 - 0:49
	0:19 - 0:49
	0:27 - 0:34
	

	below -8 to -14 °C
(below 18 to 7 °F)
	100/0
	0:42 - 1:54
	0:23 - 0:38
	1:31 - 1:46
	0:53 - 1:31
	0:30 - 0:53
	0:27 - 1:1210
	0:27 - 0:3410
	

	
	75/25
	0:30 - 1:08
	0:15 - 0:34
	1:31 - 1:54
	0:42 - 1:31
	0:19 - 0:42
	0:19 - 0:4910
	0:27 - 0:3410
	

	below -14 to -18 °C
(below 7 to 0 °F)
	100/0
	0:19 - 0:38
	0:06 - 0:19
	1:12 - 1:43
	0:27 - 1:12
	0:08 - 0:27
	
	

	below -18 to -25 °C
(below 0 to -13 °F)
	100/0
	0:19 - 0:38
	0:02 - 0:08
	0:30 - 0:42
	0:11 - 0:30
	0:03 - 0:11
	
	

	below -25 to -30.5 °C
(below -13 to -23 °F)
	100/0
	0:19 - 0:38
	0:02 - 0:04
	0:19 - 0:23
	0:05 - 0:19
	0:02 - 0:05
	
	


THIS TABLE IS FOR USE WHEN FLAPS/SLATS ARE DEPLOYED PRIOR TO DE/ANTI-ICING. HOLDOVER TIMES HAVE BEEN ADJUSTED TO 76 PERCENT.
NOTES
1. Ensure that the lowest operational use temperature (LOUT) is respected. Consider use of Type I fluid when Type IV fluid cannot be used.
1. Freezing mist is best confirmed by observation. It is never reported by METAR; however, it can occur when mist is present at 0 °C (32 °F) and below. 
1. Use freezing fog holdover times in conditions of ice crystals mixed with freezing fog or freezing mist.
1. To determine snowfall intensity, the Snowfall Intensities as a Function of Prevailing Visibility table (Table 57) is required. No holdover times exist if the reported visibility correlates to a “heavy” precipitation intensity.
Use snow holdover times in conditions of very light, light, or moderate snow mixed with ice crystals.
Includes light, moderate and heavy freezing drizzle. Use light freezing rain holdover times if positive identification of freezing drizzle is not possible.
These holdover times apply to conditions of “moderate” precipitation intensity. In cases of very light or light snow mixed with light rain or drizzle, use light freezing rain holdover times. The Snowfall Intensities as a Function of Prevailing Visibility table (Table 57) is required to confirm the precipitation intensity. No holdover times exist if the reported visibility correlates to a “heavy” precipitation intensity.
No holdover time guidelines exist for this condition for 0 °C (32 °F) and below.
Heavy snow, ice pellets, moderate and heavy freezing rain, small hail and hail (Table Adj-55 provides adjusted allowance times for Type IV PG fluids in ice pellets and small hail).
No holdover time guidelines exist for this condition below -10 °C (14 °F).
CAUTIONS
The cautions that apply to the holdover times in the table above can be found on page A-27.
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Cryotech Polar Guard® Xtend
	Outside Air 
Temperature1
	Fluid 
Concentration 
Fluid/Water 
By % Volume
	Freezing Fog, Freezing Mist2, or Ice Crystals3
	Snow 
mixed with 
Freezing Fog4
	Very Light Snow, Snow Grains or Snow Pellets4,5
	Light 
Snow, Snow Grains or Snow Pellets4,5
	Moderate Snow, Snow Grains or Snow Pellets4,5
	Freezing 
Drizzle6
	Light 
Freezing Rain
	Moderate
Snow mixed with Rain7,8
	Rain on 
Cold‑Soaked Wing8
	Other9

	-3 °C and above
(27 °F and above)
	100/0
	1:54 - 3:02
	0:38 - 1:08
	2:43 - 3:00
	1:31 - 2:43
	0:49 - 1:31
	1:31 - 1:31
	0:46 - 1:24
	0:11 - 0:11
	0:15 - 1:20
	 

	
	75/25
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	 

	
	50/50
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	CAUTION: 
No holdover time 
guidelines exist

	below -3 to -8 °C
(below 27 to 18 °F)
	100/0
	0:46 - 1:24
	0:30 - 0:53
	2:09 - 2:36
	1:12 - 2:09
	0:38 - 1:12
	0:27 - 1:16
	0:38 - 0:42
	

	
	75/25
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	

	below -8 to -14 °C
(below 18 to 7 °F)
	100/0
	0:46 - 1:24
	0:27 - 0:46
	1:50 - 2:13
	1:01 - 1:50
	0:34 - 1:01
	0:27 - 1:1610
	0:38 - 0:4210
	

	
	75/25
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	

	below -14 to -18 °C
(below 7 to 0 °F)
	100/0
	0:19 - 0:30
	0:11 - 0:23
	1:01 - 1:16
	0:30 - 1:01
	0:15 - 0:30
	
	

	below -18 to -25 °C
(below 0 to -13 °F)
	100/0
	0:19 - 0:30
	0:04 - 0:08
	0:23 - 0:30
	0:11 - 0:23
	0:05 - 0:11
	
	

	below -25 to -29 °C
(below -13 to -20 °F)
	100/0
	0:19 - 0:30
	0:02 - 0:05
	0:15 - 0:19
	0:07 - 0:15
	0:03 - 0:07
	
	


THIS TABLE IS FOR USE WHEN FLAPS/SLATS ARE DEPLOYED PRIOR TO DE/ANTI-ICING. HOLDOVER TIMES HAVE BEEN ADJUSTED TO 76 PERCENT.
NOTES
1. Ensure that the lowest operational use temperature (LOUT) is respected. Consider use of Type I fluid when Type IV fluid cannot be used. 
1. Freezing mist is best confirmed by observation. It is never reported by METAR; however, it can occur when mist is present at 0 °C (32 °F) and below. 
1. Use freezing fog holdover times in conditions of ice crystals mixed with freezing fog or freezing mist.
1. To determine snowfall intensity, the Snowfall Intensities as a Function of Prevailing Visibility table (Table 57) is required. No holdover times exist if the reported visibility correlates to a “heavy” precipitation intensity.
Use snow holdover times in conditions of very light, light, or moderate snow mixed with ice crystals.
Includes light, moderate and heavy freezing drizzle. Use light freezing rain holdover times if positive identification of freezing drizzle is not possible. 
These holdover times apply to conditions of “moderate” precipitation intensity. In cases of very light or light snow mixed with light rain or drizzle, use light freezing rain holdover times. The Snowfall Intensities as a Function of Prevailing Visibility table (Table 57) is required to confirm the precipitation intensity. No holdover times exist if the reported visibility correlates to a “heavy” precipitation intensity.
No holdover time guidelines exist for this condition for 0 °C (32 °F) and below. 
Heavy snow, ice pellets, moderate and heavy freezing rain, small hail and hail (Table Adj-55 provides adjusted allowance times for Type IV PG fluids in ice pellets and small hail).
No holdover time guidelines exist for this condition below -10 °C (14 °F). 
CAUTIONS
The cautions that apply to the holdover times in the table above can be found on page A-27.

[bookmark: _Toc9500368][bookmark: _Toc14166578][bookmark: _Toc14867915][bookmark: _Toc43986231][bookmark: _Toc44053697][bookmark: _Toc44054116][bookmark: _Toc45715350][bookmark: _Toc75345488][bookmark: _Toc77777054][bookmark: _Toc77777104][bookmark: _Toc105048947][bookmark: _Toc105049301][bookmark: _Toc105049424][bookmark: _Toc105399241][bookmark: _Toc105399452][bookmark: _Toc107305602][bookmark: _Toc231475410]Table Adj-37: Adjusted Type IV Holdover Times for 
Dow Inc. UCAR Endurance™ EG106 ADF/AAF
	Outside Air 
Temperature1
	Fluid 
Concentration 
Fluid/Water 
By % Volume
	Freezing Fog, Freezing Mist2, or Ice Crystals3
	Snow 
mixed with 
Freezing Fog4
	Very Light Snow, Snow Grains or Snow Pellets4,5
	Light 
Snow, Snow Grains or Snow Pellets4,5
	Moderate Snow, Snow Grains or Snow Pellets4,5
	Freezing 
Drizzle6
	Light 
Freezing Rain
	Moderate
Snow mixed with Rain7,8
	Rain on 
Cold‑Soaked Wing8
	Other9

	-3 °C and above
(27 °F and above)
	100/0
	1:35 - 2:24
	0:23 - 0:46
	2:05 - 2:40
	1:01 - 2:05
	0:30 - 1:01
	0:53 - 1:31
	0:38 - 0:57
	0:11 - 0:11
	0:15 - 1:31
	 

	
	75/25
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	 

	
	50/50
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	CAUTION: 
No holdover time 
guidelines exist

	below -3 to -8 °C
(below 27 to 18 °F)
	100/0
	1:24 - 2:32
	0:19 - 0:38
	1:50 - 2:17
	0:53 - 1:50
	0:27 - 0:53
	0:42 - 1:24
	0:34 - 0:53
	

	
	75/25
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	

	below -8 to -14 °C
(below 18 to 7 °F)
	100/0
	1:24 - 2:32
	0:19 - 0:34
	1:39 - 2:05
	0:49 - 1:39
	0:23 - 0:49
	0:42 - 1:2410
	0:34 - 0:5310
	

	
	75/25
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	

	below -14 to -18 °C
(below 7 to 0 °F)
	100/0
	0:23 - 0:49
	0:11 - 0:27
	1:20 - 1:43
	0:38 - 1:20
	0:19 - 0:38
	
	

	below -18 to -25 °C
(below 0 to -13 °F)
	100/0
	0:23 - 0:49
	0:11 - 0:23
	1:08 - 1:27
	0:30 - 1:08
	0:15 - 0:30
	
	

	below -25 to -29 °C
(below -13 to -20 °F)
	100/0
	0:23 - 0:49
	0:11 - 0:23
	1:01 - 1:20
	0:30 - 1:01
	0:15 - 0:30
	
	


THIS TABLE IS FOR USE WHEN FLAPS/SLATS ARE DEPLOYED PRIOR TO DE/ANTI-ICING. HOLDOVER TIMES HAVE BEEN ADJUSTED TO 76 PERCENT.
NOTES
1. Ensure that the lowest operational use temperature (LOUT) is respected. Consider use of Type I fluid when Type IV fluid cannot be used.
1. Freezing mist is best confirmed by observation. It is never reported by METAR; however, it can occur when mist is present at 0 °C (32 °F) and below. 
1. Use freezing fog holdover times in conditions of ice crystals mixed with freezing fog or freezing mist.
1. To determine snowfall intensity, the Snowfall Intensities as a Function of Prevailing Visibility table (Table 57) is required. No holdover times exist if the reported visibility correlates to a “heavy” precipitation intensity.
Use snow holdover times in conditions of very light, light, or moderate snow mixed with ice crystals.
Includes light, moderate and heavy freezing drizzle. Use light freezing rain holdover times if positive identification of freezing drizzle is not possible.
These holdover times apply to conditions of “moderate” precipitation intensity. In cases of very light or light snow mixed with light rain or drizzle, use light freezing rain holdover times. The Snowfall Intensities as a Function of Prevailing Visibility table (Table 57) is required to confirm the precipitation intensity. No holdover times exist if the reported visibility correlates to a “heavy” precipitation intensity.
No holdover time guidelines exist for this condition for 0 °C (32 °F) and below.
Heavy snow, ice pellets, moderate and heavy freezing rain, small hail and hail (Table Adj-54 provides adjusted allowance times for Type IV EG fluids in ice pellets and small hail).
No holdover time guidelines exist for this condition below -10 °C (14 °F).
CAUTIONS
The cautions that apply to the holdover times in the table above can be found on page A-27.
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Dow inc. UCAR™ FLIGHTGUARD™ AD-49
	Outside Air 
Temperature1
	Fluid 
Concentration 
Fluid/Water 
By % Volume
	Freezing Fog, Freezing Mist2, or Ice Crystals3
	Snow 
mixed with 
Freezing Fog4
	Very Light Snow, Snow Grains or Snow Pellets4,5
	Light 
Snow, Snow Grains or Snow Pellets4,5
	Moderate Snow, Snow Grains or Snow Pellets4,5
	Freezing 
Drizzle6
	Light 
Freezing Rain
	Moderate
Snow mixed with Rain7,8
	Rain on 
Cold‑Soaked Wing8
	Other9

	-3 °C and above
(27 °F and above)
	100/0
	2:32 - 3:02
	0:34 - 1:05
	2:47 - 3:00
	1:27 - 2:47
	0:46 - 1:27
	1:05 - 1:31
	0:46 - 1:05
	0:06 - 0:06
	0:08 - 1:27
	 

	
	75/25
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	 

	
	50/50
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	CAUTION: 
No holdover time 
guidelines exist

	below -3 to -8 °C
(below 27 to 18 °F)
	100/0
	0:15 - 1:12
	0:27 - 0:49
	2:13 - 2:40
	1:08 - 2:13
	0:34 - 1:08
	0:19 - 1:05
	0:15 - 0:19
	

	
	75/25
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	

	below -8 to -14 °C
(below 18 to 7 °F)
	100/0
	0:15 - 1:12
	0:23 - 0:42
	1:50 - 2:17
	0:57 - 1:50
	0:30 - 0:57
	0:19 - 1:0510
	0:15 - 0:1910
	

	
	75/25
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	

	below -14 to -18 °C
(below 7 to 0 °F)
	100/0
	0:19 - 0:30
	0:01 - 0:05
	0:23 - 0:34
	0:07 - 0:23
	0:02 - 0:07
	
	

	below -18 to -25 °C
(below 0 to -13 °F)
	100/0
	0:19 - 0:30
	0:00 - 0:02
	0:08 - 0:15
	0:02 - 0:08
	0:01 - 0:02
	
	

	below -25 to -26 °C
(below -13 to -15 °F)
	100/0
	0:19 - 0:30
	0:00 - 0:01
	0:05 - 0:08
	0:02 - 0:05
	0:00 - 0:02
	
	


THIS TABLE IS FOR USE WHEN FLAPS/SLATS ARE DEPLOYED PRIOR TO DE/ANTI-ICING. HOLDOVER TIMES HAVE BEEN ADJUSTED TO 76 PERCENT.
NOTES
1. Ensure that the lowest operational use temperature (LOUT) is respected. Consider use of Type I fluid when Type IV fluid cannot be used.
1. Freezing mist is best confirmed by observation. It is never reported by METAR; however, it can occur when mist is present at 0 °C (32 °F) and below. 
1. Use freezing fog holdover times in conditions of ice crystals mixed with freezing fog or freezing mist.
1. To determine snowfall intensity, the Snowfall Intensities as a Function of Prevailing Visibility table (Table 57) is required. No holdover times exist if the reported visibility correlates to a “heavy” precipitation intensity.
Use snow holdover times in conditions of very light, light, or moderate snow mixed with ice crystals.
Includes light, moderate and heavy freezing drizzle. Use light freezing rain holdover times if positive identification of freezing drizzle is not possible.
These holdover times apply to conditions of “moderate” precipitation intensity. In cases of very light or light snow mixed with light rain or drizzle, use light freezing rain holdover times. The Snowfall Intensities as a Function of Prevailing Visibility table (Table 57) is required to confirm the precipitation intensity. No holdover times exist if the reported visibility correlates to a “heavy” precipitation intensity.
No holdover time guidelines exist for this condition for 0 °C (32 °F) and below.
Heavy snow, ice pellets, moderate and heavy freezing rain, small hail and hail (Table Adj-55 provides adjusted allowance times for Type IV PG fluids in ice pellets and small hail).
No holdover time guidelines exist for this condition below -10 °C (14 °F).
CAUTIONS
The cautions that apply to the holdover times in the table above can be found on page A-27.

[bookmark: _Toc231475412]Table Adj-39: Adjusted Type IV Holdover Times for 
ESSPO CHEMICALS D.O.O Nordwing PG4
	Outside Air 
Temperature1
	Fluid 
Concentration 
Fluid/Water 
By % Volume
	Freezing Fog, Freezing Mist2, or Ice Crystals3
	Snow 
mixed with 
Freezing Fog4
	Very Light Snow, Snow Grains or Snow Pellets4,5
	Light 
Snow, Snow Grains or Snow Pellets4,5
	Moderate Snow, Snow Grains or Snow Pellets4,5
	Freezing 
Drizzle6
	Light 
Freezing Rain
	Moderate
Snow mixed with Rain7,8
	Rain on 
Cold‑Soaked Wing8
	Other9

	-3 °C and above
(27 °F and above)
	100/0
	1:12 - 2:24
	0:23 - 0:42
	1:58 - 2:24
	0:57 - 1:58
	0:27 - 0:57
	0:49 - 1:20
	0:38 - 0:46
	0:11 - 0:11
	0:15 - 1:20
	 

	
	75/25
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	 

	
	50/50
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	CAUTION: 
No holdover time 
guidelines exist

	below -3 to -8 °C
(below 27 to 18 °F)
	100/0
	0:42 - 1:50
	0:19 - 0:38
	1:39 - 2:02
	0:49 - 1:39
	0:23 - 0:49
	0:42 - 1:08
	0:27 - 0:38
	

	
	75/25
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	

	below -8 to -14 °C
(below 18 to 7 °F)
	100/0
	0:42 - 1:50
	0:15 - 0:34
	1:27 - 1:50
	0:42 - 1:27
	0:23 - 0:42
	0:42 - 1:0810
	0:27 - 0:3810
	

	
	75/25
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	

	below -14 to -18 °C
(below 7 to 0 °F)
	100/0
	0:23 - 0:34
	0:08 - 0:19
	1:01 - 1:20
	0:27 - 1:01
	0:11 - 0:27
	
	

	below -18 to -25 °C
(below 0 to -13 °F)
	100/0
	0:23 - 0:34
	0:05 - 0:11
	0:38 - 0:53
	0:15 - 0:38
	0:07 - 0:15
	
	

	below -25 to -30 °C
(below -13 to -22 °F)
	100/0
	0:15 - 0:27
	0:03 - 0:07
	0:23 - 0:30
	0:11 - 0:23
	0:04 - 0:11
	
	


THIS TABLE IS FOR USE WHEN FLAPS/SLATS ARE DEPLOYED PRIOR TO DE/ANTI-ICING. HOLDOVER TIMES HAVE BEEN ADJUSTED TO 76 PERCENT.
NOTES
1. Ensure that the lowest operational use temperature (LOUT) is respected. Consider use of Type I fluid when Type IV fluid cannot be used.
1. Freezing mist is best confirmed by observation. It is never reported by METAR; however, it can occur when mist is present at 0 °C (32 °F) and below. 
1. Use freezing fog holdover times in conditions of ice crystals mixed with freezing fog or freezing mist.
1. To determine snowfall intensity, the Snowfall Intensities as a Function of Prevailing Visibility table (Table 57) is required. No holdover times exist if the reported visibility correlates to a “heavy” precipitation intensity.
Use snow holdover times in conditions of very light, light, or moderate snow mixed with ice crystals.
Includes light, moderate and heavy freezing drizzle. Use light freezing rain holdover times if positive identification of freezing drizzle is not possible.
These holdover times apply to conditions of “moderate” precipitation intensity. In cases of very light or light snow mixed with light rain or drizzle, use light freezing rain holdover times. The Snowfall Intensities as a Function of Prevailing Visibility table (Table 57) is required to confirm the precipitation intensity. No holdover times exist if the reported visibility correlates to a “heavy” precipitation intensity.
No holdover time guidelines exist for this condition for 0 °C (32 °F) and below.
Heavy snow, ice pellets, moderate and heavy freezing rain, small hail and hail.
No holdover time guidelines exist for this condition below -10 °C (14 °F).
CAUTIONS
The cautions that apply to the holdover times in the table above can be found on page A-27.

[bookmark: _Toc436349485][bookmark: _Toc517088971][bookmark: _Toc517253628][bookmark: _Toc519674731][bookmark: _Toc519674838][bookmark: _Toc520288590][bookmark: _Toc520289462][bookmark: _Toc9500370][bookmark: _Toc14166580][bookmark: _Toc14867917][bookmark: _Toc43986233][bookmark: _Toc44053699][bookmark: _Toc44054118][bookmark: _Toc45715352][bookmark: _Toc75345490][bookmark: _Toc77777056][bookmark: _Toc77777106][bookmark: _Toc105048949][bookmark: _Toc105049303][bookmark: _Toc105049426][bookmark: _Toc105399243][bookmark: _Toc105399454][bookmark: _Toc107305604][bookmark: _Toc231475413][bookmark: _Toc436349489]Table Adj-40: Adjusted Type IV Holdover Times for 
Inland Technologies ECO-SHIELD®
	Outside Air 
Temperature1
	Fluid 
Concentration 
Fluid/Water 
By % Volume
	Freezing Fog, Freezing Mist2, or Ice Crystals3
	Snow 
mixed with 
Freezing Fog4
	Very Light Snow, Snow Grains or Snow Pellets4,5
	Light 
Snow, Snow Grains or Snow Pellets4,5
	Moderate Snow, Snow Grains or Snow Pellets4,5
	Freezing 
Drizzle6
	Light 
Freezing Rain
	Moderate
Snow mixed with Rain7,8
	Rain on 
Cold‑Soaked Wing8
	Other9

	-3 °C and above
(27 °F and above)
	100/0
	0:57 - 2:02
	0:27 - 0:46
	1:50 - 2:09
	1:01 - 1:50
	0:34 - 1:01
	0:30 - 1:08
	0:27 - 0:30
	0:07 - 0:07
	0:11 - 1:12
	 

	
	75/25
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	 

	
	50/50
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	CAUTION: 
No holdover time 
guidelines exist

	below -3 to -8 °C
(below 27 to 18 °F)
	100/0
	0:53 - 1:58
	0:23 - 0:42
	1:35 - 1:54
	0:53 - 1:35
	0:30 - 0:53
	0:38 - 1:05
	0:23 - 0:30
	

	
	75/25
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	

	below -8 to -14 °C
(below 18 to 7 °F)
	100/0
	0:53 - 1:58
	0:19 - 0:38
	1:27 - 1:43
	0:49 - 1:27
	0:27 - 0:49
	0:38 - 1:0510
	0:23 - 0:3010
	

	
	75/25
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	

	below -14 to -18 °C
(below 7 to 0 °F)
	100/0
	0:23 - 0:46
	0:01 - 0:05
	0:23 - 0:34
	0:07 - 0:23
	0:02 - 0:07
	
	

	below -18 to -25 °C
(below 0 to -13 °F)
	100/0
	0:23 - 0:46
	0:00 - 0:02
	0:08 - 0:15
	0:02 - 0:08
	0:01 - 0:02
	
	

	below -25 to -25.5 °C
(below -13 to -14 °F)
	100/0
	0:23 - 0:46
	0:00 - 0:01
	0:05 - 0:08
	0:02 - 0:05
	0:00 - 0:02
	
	


THIS TABLE IS FOR USE WHEN FLAPS/SLATS ARE DEPLOYED PRIOR TO DE/ANTI-ICING. HOLDOVER TIMES HAVE BEEN ADJUSTED TO 76 PERCENT.
NOTES
1. Ensure that the lowest operational use temperature (LOUT) is respected. Consider use of Type I fluid when Type IV fluid cannot be used.
1. Freezing mist is best confirmed by observation. It is never reported by METAR; however, it can occur when mist is present at 0 °C (32 °F) and below. 
1. Use freezing fog holdover times in conditions of ice crystals mixed with freezing fog or freezing mist.
1. To determine snowfall intensity, the Snowfall Intensities as a Function of Prevailing Visibility table (Table 57) is required. No holdover times exist if the reported visibility correlates to a “heavy” precipitation intensity.
Use snow holdover times in conditions of very light, light, or moderate snow mixed with ice crystals.
Includes light, moderate and heavy freezing drizzle. Use light freezing rain holdover times if positive identification of freezing drizzle is not possible.
These holdover times apply to conditions of “moderate” precipitation intensity. In cases of very light or light snow mixed with light rain or drizzle, use light freezing rain holdover times. The Snowfall Intensities as a Function of Prevailing Visibility table (Table 57) is required to confirm the precipitation intensity. No holdover times exist if the reported visibility correlates to a “heavy” precipitation intensity.
No holdover time guidelines exist for this condition for 0 °C (32 °F) and below.
Heavy snow, ice pellets, moderate and heavy freezing rain, small hail and hail.
No holdover time guidelines exist for this condition below -10 °C (14 °F).
CAUTIONS
The cautions that apply to the holdover times in the table above can be found on page A-27.
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JSC RCP Nordix Defrost ECO 4
	Outside Air 
Temperature1
	Fluid 
Concentration 
Fluid/Water 
By % Volume
	Freezing Fog, Freezing Mist2, or Ice Crystals3
	Snow 
mixed with 
Freezing Fog4
	Very Light Snow, Snow Grains or Snow Pellets4,5
	Light 
Snow, Snow Grains or Snow Pellets4,5
	Moderate Snow, Snow Grains or Snow Pellets4,5
	Freezing 
Drizzle6
	Light 
Freezing Rain
	Moderate
Snow mixed with Rain7,8
	Rain on 
Cold‑Soaked Wing8
	Other9

	-3 °C and above
(27 °F and above)
	100/0
	1:08 - 2:02
	0:23 - 0:42
	1:54 - 2:24
	0:57 - 1:54
	0:27 - 0:57
	0:49 - 1:08
	0:30 - 0:49
	0:08 - 0:08
	0:11 - 0:53
	 

	
	75/25
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	 

	
	50/50
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	CAUTION: 
No holdover time 
guidelines exist

	below -3 to -8 °C
(below 27 to 18 °F)
	100/0
	0:42 - 1:58
	0:19 - 0:38
	1:43 - 2:05
	0:49 - 1:43
	0:27 - 0:49
	0:38 - 1:01
	0:27 - 0:38
	

	
	75/25
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	

	below -8 to -14 °C
(below 18 to 7 °F)
	100/0
	0:42 - 1:58
	0:19 - 0:34
	1:35 - 1:58
	0:46 - 1:35
	0:23 - 0:46
	0:38 - 1:0110
	0:27 - 0:3810
	

	
	75/25
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	

	below -14 to -18 °C
(below 7 to 0 °F)
	100/0
	0:23 - 0:38
	0:01 - 0:05
	0:23 - 0:34
	0:07 - 0:23
	0:02 - 0:07
	
	

	below -18 to -25 °C
(below 0 to -13 °F)
	100/0
	0:23 - 0:38
	0:00 - 0:02
	0:08 - 0:15
	0:02 - 0:08
	0:01 - 0:02
	
	

	below -25 to -25.5 °C
(below -13 to -14 °F)
	100/0
	0:23 - 0:38
	0:00 - 0:01
	0:05 - 0:08
	0:02 - 0:05
	0:00 - 0:02
	
	


THIS TABLE IS FOR USE WHEN FLAPS/SLATS ARE DEPLOYED PRIOR TO DE/ANTI-ICING. HOLDOVER TIMES HAVE BEEN ADJUSTED TO 76 PERCENT.
NOTES
1. Ensure that the lowest operational use temperature (LOUT) is respected. Consider use of Type I fluid when Type IV fluid cannot be used.
1. Freezing mist is best confirmed by observation. It is never reported by METAR; however, it can occur when mist is present at 0 °C (32 °F) and below. 
1. Use freezing fog holdover times in conditions of ice crystals mixed with freezing fog or freezing mist.
1. To determine snowfall intensity, the Snowfall Intensities as a Function of Prevailing Visibility table (Table 57) is required. No holdover times exist if the reported visibility correlates to a “heavy” precipitation intensity.
Use snow holdover times in conditions of very light, light, or moderate snow mixed with ice crystals.
Includes light, moderate and heavy freezing drizzle. Use light freezing rain holdover times if positive identification of freezing drizzle is not possible.
These holdover times apply to conditions of “moderate” precipitation intensity. In cases of very light or light snow mixed with light rain or drizzle, use light freezing rain holdover times. The Snowfall Intensities as a Function of Prevailing Visibility table (Table 57) is required to confirm the precipitation intensity. No holdover times exist if the reported visibility correlates to a “heavy” precipitation intensity.
No holdover time guidelines exist for this condition for 0 °C (32 °F) and below.
Heavy snow, ice pellets, moderate and heavy freezing rain, small hail and hail (Table Adj-55 provides adjusted allowance times for Type IV PG fluids in ice pellets and small hail).
No holdover time guidelines exist for this condition below -10 °C (14 °F).
CAUTIONS
The cautions that apply to the holdover times in the table above can be found on page A-27.

[bookmark: _Toc75345493][bookmark: _Toc77777059][bookmark: _Toc77777109][bookmark: _Toc105048952][bookmark: _Toc105049306][bookmark: _Toc105049429][bookmark: _Toc105399246][bookmark: _Toc105399457][bookmark: _Toc107305607][bookmark: _Toc231475415][bookmark: _Toc43986236][bookmark: _Toc44053702][bookmark: _Toc44054121][bookmark: _Toc45715355]Table Adj-42: Adjusted Type IV Holdover Times for 
JSC RCP Nordix Defrost NORTH 4
	Outside Air 
Temperature1
	Fluid 
Concentration 
Fluid/Water 
By % Volume
	Freezing Fog, Freezing Mist2, or Ice Crystals3
	Snow 
mixed with 
Freezing Fog4
	Very Light Snow, Snow Grains or Snow Pellets4,5
	Light 
Snow, Snow Grains or Snow Pellets4,5
	Moderate Snow, Snow Grains or Snow Pellets4,5
	Freezing 
Drizzle6
	Light 
Freezing Rain
	Moderate
Snow mixed with Rain7,8
	Rain on 
Cold‑Soaked Wing8
	Other9

	-3 °C and above
(27 °F and above)
	100/0
	1:39 - 3:02
	0:19 - 0:38
	1:50 - 2:21
	0:53 - 1:50
	0:23 - 0:53
	0:49 - 1:31
	0:23 - 0:38
	0:05 - 0:05
	0:07 - 1:27
	 

	
	75/25
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	 

	
	50/50
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	CAUTION: 
No holdover time 
guidelines exist

	below -3 to -8 °C
(below 27 to 18 °F)
	100/0
	2:02 - 3:02
	0:19 - 0:38
	1:50 - 2:21
	0:53 - 1:50
	0:23 - 0:53
	0:49 - 1:31
	0:30 - 0:46
	

	
	75/25
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	

	below -8 to -14 °C
(below 18 to 7 °F)
	100/0
	2:02 - 3:02
	0:19 - 0:38
	1:50 - 2:21
	0:53 - 1:50
	0:23 - 0:53
	0:49 - 1:3110
	0:30 - 0:4610
	

	
	75/25
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	

	below -14 to -18 °C
(below 7 to 0 °F)
	100/0
	0:34 - 1:27
	0:05 - 0:15
	0:38 - 0:49
	0:19 - 0:38
	0:08 - 0:19
	
	

	below -18 to -25 °C
(below 0 to -13 °F)
	100/0
	0:34 - 1:27
	0:02 - 0:08
	0:30 - 0:42
	0:11 - 0:30
	0:04 - 0:11
	
	

	below -25 to -26 °C
(below -13 to -15 °F)
	100/0
	0:34 - 1:27
	0:01 - 0:05
	0:19 - 0:27
	0:06 - 0:19
	0:02 - 0:06
	
	


THIS TABLE IS FOR USE WHEN FLAPS/SLATS ARE DEPLOYED PRIOR TO DE/ANTI-ICING. HOLDOVER TIMES HAVE BEEN ADJUSTED TO 76 PERCENT.
NOTES
1. Ensure that the lowest operational use temperature (LOUT) is respected. Consider use of Type I fluid when Type IV fluid cannot be used.
1. Freezing mist is best confirmed by observation. It is never reported by METAR; however, it can occur when mist is present at 0 °C (32 °F) and below. 
1. Use freezing fog holdover times in conditions of ice crystals mixed with freezing fog or freezing mist.
1. To determine snowfall intensity, the Snowfall Intensities as a Function of Prevailing Visibility table (Table 57) is required. No holdover times exist if the reported visibility correlates to a “heavy” precipitation intensity.
Use snow holdover times in conditions of very light, light, or moderate snow mixed with ice crystals.
Includes light, moderate and heavy freezing drizzle. Use light freezing rain holdover times if positive identification of freezing drizzle is not possible.
These holdover times apply to conditions of “moderate” precipitation intensity. In cases of very light or light snow mixed with light rain or drizzle, use light freezing rain holdover times. The Snowfall Intensities as a Function of Prevailing Visibility table (Table 57) is required to confirm the precipitation intensity. No holdover times exist if the reported visibility correlates to a “heavy” precipitation intensity.
No holdover time guidelines exist for this condition for 0 °C (32 °F) and below.
Heavy snow, ice pellets, moderate and heavy freezing rain, small hail and hail (Table Adj-54 provides adjusted allowance times for Type IV EG fluids in ice pellets and small hail).
No holdover time guidelines exist for this condition below -10 °C (14 °F).
CAUTIONS
The cautions that apply to the holdover times in the table above can be found on page A-27.

[bookmark: _Toc75345494][bookmark: _Toc77777060][bookmark: _Toc77777110][bookmark: _Toc105048953][bookmark: _Toc105049307][bookmark: _Toc105049430][bookmark: _Toc105399247][bookmark: _Toc105399458][bookmark: _Toc107305608][bookmark: _Toc231475416][bookmark: _Toc198813148]Table Adj-43: Adjusted Type IV Holdover Times for 
Kilfrost ABC-S Plus
	Outside Air 
Temperature1
	Fluid 
Concentration 
Fluid/Water 
By % Volume
	Freezing Fog, Freezing Mist2, or Ice Crystals3
	Snow 
mixed with 
Freezing Fog4
	Very Light Snow, Snow Grains or Snow Pellets4,5
	Light 
Snow, Snow Grains or Snow Pellets4,5
	Moderate Snow, Snow Grains or Snow Pellets4,5
	Freezing 
Drizzle6
	Light 
Freezing Rain
	Moderate
Snow mixed with Rain7,8
	Rain on 
Cold‑Soaked Wing8
	Other9

	-3 °C and above
(27 °F and above)
	100/0
	1:39 - 3:02
	0:42 - 1:12
	2:43 - 3:00
	1:35 - 2:43
	0:57 - 1:35
	1:24 - 1:31
	0:49 - 1:31
	0:11 - 0:11
	0:19 - 1:31
	 

	
	75/25
	1:05 - 2:02
	0:23 - 0:42
	1:35 - 1:50
	0:57 - 1:35
	0:34 - 0:57
	0:46 - 1:01
	0:23 - 0:38
	0:06 - 0:06
	0:08 - 1:01
	 

	
	50/50
	0:23 - 0:42
	0:11 - 0:19
	0:46 - 0:53
	0:23 - 0:46
	0:11 - 0:23
	0:11 - 0:30
	0:11 - 0:15
	CAUTION: 
No holdover time 
guidelines exist

	below -3 to -8 °C
(below 27 to 18 °F)
	100/0
	0:42 - 2:40
	0:38 - 1:05
	2:24 - 2:51
	1:24 - 2:24
	0:49 - 1:24
	0:19 - 1:12
	0:15 - 0:23
	

	
	75/25
	0:34 - 1:24
	0:23 - 0:38
	1:24 - 1:39
	0:49 - 1:24
	0:30 - 0:49
	0:15 - 0:53
	0:11 - 0:19
	

	below -8 to -14 °C
(below 18 to 7 °F)
	100/0
	0:42 - 2:40
	0:34 - 0:57
	2:13 - 2:40
	1:20 - 2:13
	0:46 - 1:20
	0:19 - 1:1210
	0:15 - 0:2310
	

	
	75/25
	0:34 - 1:24
	0:19 - 0:34
	1:20 - 1:31
	0:46 - 1:20
	0:27 - 0:46
	0:15 - 0:5310
	0:11 - 0:1910
	

	below -14 to -18 °C
(below 7 to 0 °F)
	100/0
	0:30 - 0:46
	0:01 - 0:05
	0:23 - 0:34
	0:07 - 0:23
	0:02 - 0:07
	
	

	below -18 to -25 °C
(below 0 to -13 °F)
	100/0
	0:30 - 0:46
	0:00 - 0:02
	0:08 - 0:15
	0:02 - 0:08
	0:01 - 0:02
	
	

	below -25 to -28 °C
(below -13 to -18 °F)
	100/0
	0:30 - 0:46
	0:00 - 0:01
	0:05 - 0:08
	0:02 - 0:05
	0:00 - 0:02
	
	


THIS TABLE IS FOR USE WHEN FLAPS/SLATS ARE DEPLOYED PRIOR TO DE/ANTI-ICING. HOLDOVER TIMES HAVE BEEN ADJUSTED TO 76 PERCENT.
NOTES
1. Ensure that the lowest operational use temperature (LOUT) is respected. Consider use of Type I fluid when Type IV fluid cannot be used.
1. Freezing mist is best confirmed by observation. It is never reported by METAR; however, it can occur when mist is present at 0 °C (32 °F) and below. 
1. Use freezing fog holdover times in conditions of ice crystals mixed with freezing fog or freezing mist.
1. To determine snowfall intensity, the Snowfall Intensities as a Function of Prevailing Visibility table (Table 57) is required. No holdover times exist if the reported visibility correlates to a “heavy” precipitation intensity.
Use snow holdover times in conditions of very light, light, or moderate snow mixed with ice crystals.
Includes light, moderate and heavy freezing drizzle. Use light freezing rain holdover times if positive identification of freezing drizzle is not possible.
These holdover times apply to conditions of “moderate” precipitation intensity. In cases of very light or light snow mixed with light rain or drizzle, use light freezing rain holdover times. The Snowfall Intensities as a Function of Prevailing Visibility table (Table 57) is required to confirm the precipitation intensity. No holdover times exist if the reported visibility correlates to a “heavy” precipitation intensity.
No holdover time guidelines exist for this condition for 0 °C (32 °F) and below.
Heavy snow, ice pellets, moderate and heavy freezing rain, small hail and hail.
No holdover time guidelines exist for this condition below -10 °C (14 °F).
CAUTIONS
The cautions that apply to the holdover times in the table above can be found on page A-27.

[bookmark: _Toc231475417]Table Adj-44: Adjusted Type IV Holdover Times for 
LNT Solutions P450
	Outside Air 
Temperature1
	Fluid 
Concentration 
Fluid/Water 
By % Volume
	Freezing Fog, Freezing Mist2, or Ice Crystals3
	Snow 
mixed with 
Freezing Fog4
	Very Light Snow, Snow Grains or Snow Pellets4,5
	Light 
Snow, Snow Grains or Snow Pellets4,5
	Moderate Snow, Snow Grains or Snow Pellets4,5
	Freezing 
Drizzle6
	Light 
Freezing Rain
	Moderate
Snow mixed with Rain7,8
	Rain on 
Cold‑Soaked Wing8
	Other9

	-3 °C and above
(27 °F and above)
	100/0
	2:24 - 3:02
	0:30 - 1:12
	3:00 - 3:00
	1:35 - 3:00
	0:42 - 1:35
	1:31 - 1:31
	0:49 - 1:16
	0:15 - 0:15
	0:23 - 1:27
	 

	
	75/25
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	 

	
	50/50
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	CAUTION: 
No holdover time 
guidelines exist

	below -3 to -8 °C
(below 27 to 18 °F)
	100/0
	0:53 - 2:13
	0:27 - 0:57
	2:43 - 3:00
	1:12 - 2:43
	0:34 - 1:12
	0:27 - 1:24
	0:19 - 0:38
	

	
	75/25
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	

	below -8 to -14 °C
(below 18 to 7 °F)
	100/0
	0:53 - 2:13
	0:23 - 0:46
	2:17 - 2:59
	1:01 - 2:17
	0:27 - 1:01
	0:27 - 1:2410
	0:19 - 0:3810
	

	
	75/25
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	

	below -14 to -18 °C
(below 7 to 0 °F)
	100/0
	0:11 - 0:19
	0:01 - 0:05
	0:23 - 0:34
	0:07 - 0:23
	0:02 - 0:07
	
	

	below -18 to -25 °C
(below 0 to -13 °F)
	100/0
	0:11 - 0:19
	0:00 - 0:02
	0:08 - 0:15
	0:02 - 0:08
	0:01 - 0:02
	
	

	below -25 to -29 °C
(below -13 to -20 °F)
	100/0
	0:11 - 0:19
	0:00 - 0:01
	0:05 - 0:08
	0:02 - 0:05
	0:00 - 0:02
	
	


THIS TABLE IS FOR USE WHEN FLAPS/SLATS ARE DEPLOYED PRIOR TO DE/ANTI-ICING. HOLDOVER TIMES HAVE BEEN ADJUSTED TO 76 PERCENT.
NOTES
1. Ensure that the lowest operational use temperature (LOUT) is respected. Consider use of Type I fluid when Type IV fluid cannot be used.
1. Freezing mist is best confirmed by observation. It is never reported by METAR; however, it can occur when mist is present at 0 °C (32 °F) and below. 
1. Use freezing fog holdover times in conditions of ice crystals mixed with freezing fog or freezing mist.
1. To determine snowfall intensity, the Snowfall Intensities as a Function of Prevailing Visibility table (Table 57) is required. No holdover times exist if the reported visibility correlates to a “heavy” precipitation intensity.
Use snow holdover times in conditions of very light, light, or moderate snow mixed with ice crystals.
Includes light, moderate and heavy freezing drizzle. Use light freezing rain holdover times if positive identification of freezing drizzle is not possible.
These holdover times apply to conditions of “moderate” precipitation intensity. In cases of very light or light snow mixed with light rain or drizzle, use light freezing rain holdover times. The Snowfall Intensities as a Function of Prevailing Visibility table (Table 57) is required to confirm the precipitation intensity. No holdover times exist if the reported visibility correlates to a “heavy” precipitation intensity.
No holdover time guidelines exist for this condition for 0 °C (32 °F) and below.
Heavy snow, ice pellets, moderate and heavy freezing rain, small hail and hail.
No holdover time guidelines exist for this condition below -10 °C (14 °F).
CAUTIONS
The cautions that apply to the holdover times in the table above can be found on page A-27.

[bookmark: _Toc231475418]Table Adj-45: Adjusted Type IV Holdover Times for 
MAX TECH LLC MTL 4-EG
	Outside Air 
Temperature1
	Fluid 
Concentration 
Fluid/Water 
By % Volume
	Freezing Fog, Freezing Mist2, or Ice Crystals3
	Snow 
mixed with 
Freezing Fog4
	Very Light Snow, Snow Grains or Snow Pellets4,5
	Light 
Snow, Snow Grains or Snow Pellets4,5
	Moderate Snow, Snow Grains or Snow Pellets4,5
	Freezing 
Drizzle6
	Light 
Freezing Rain
	Moderate
Snow mixed with Rain7,8
	Rain on 
Cold‑Soaked Wing8
	Other9

	-3 °C and above
(27 °F and above)
	100/0
	2:02 - 3:02
	0:42 - 1:35
	3:00 - 3:00
	2:09 - 3:00
	0:53 - 2:09
	0:57 - 1:31
	0:34 - 0:57
	0:08 - 0:08
	0:11 - 1:24
	 

	
	75/25
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	 

	
	50/50
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	CAUTION: 
No holdover time 
guidelines exist

	below -3 to -8 °C
(below 27 to 18 °F)
	100/0
	1:58 - 2:59
	0:27 - 1:05
	3:00 - 3:00
	1:27 - 3:00
	0:38 - 1:27
	0:46 - 1:31
	0:38 - 0:57
	

	
	75/25
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	

	below -8 to -14 °C
(below 18 to 7 °F)
	100/0
	1:05 - 3:02
	0:23 - 0:53
	2:43 - 3:00
	1:08 - 2:43
	0:30 - 1:08
	0:38 - 1:3110
	0:34 - 1:0110
	

	
	75/25
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	

	below -14 to -18 °C
(below 7 to 0 °F)
	100/0
	0:38 - 3:02
	0:15 - 0:34
	1:43 - 2:09
	0:46 - 1:43
	0:23 - 0:46
	
	

	below -18 to -25 °C
(below 0 to -13 °F)
	100/0
	0:19 - 0:46
	0:11 - 0:23
	1:08 - 1:31
	0:30 - 1:08
	0:15 - 0:30
	
	

	below -25 to -26.5 °C
(below -13 to -16 °F)
	100/0
	0:19 - 0:46
	0:11 - 0:23
	1:05 - 1:24
	0:30 - 1:05
	0:15 - 0:30
	
	


THIS TABLE IS FOR USE WHEN FLAPS/SLATS ARE DEPLOYED PRIOR TO DE/ANTI-ICING. HOLDOVER TIMES HAVE BEEN ADJUSTED TO 76 PERCENT.
NOTES
1. Ensure that the lowest operational use temperature (LOUT) is respected. Consider use of Type I fluid when Type IV fluid cannot be used.
1. Freezing mist is best confirmed by observation. It is never reported by METAR; however, it can occur when mist is present at 0 °C (32 °F) and below. 
1. Use freezing fog holdover times in conditions of ice crystals mixed with freezing fog or freezing mist.
1. To determine snowfall intensity, the Snowfall Intensities as a Function of Prevailing Visibility table (Table 57) is required. No holdover times exist if the reported visibility correlates to a “heavy” precipitation intensity.
Use snow holdover times in conditions of very light, light, or moderate snow mixed with ice crystals.
Includes light, moderate and heavy freezing drizzle. Use light freezing rain holdover times if positive identification of freezing drizzle is not possible.
These holdover times apply to conditions of “moderate” precipitation intensity. In cases of very light or light snow mixed with light rain or drizzle, use light freezing rain holdover times. The Snowfall Intensities as a Function of Prevailing Visibility table (Table 57) is required to confirm the precipitation intensity. No holdover times exist if the reported visibility correlates to a “heavy” precipitation intensity.
No holdover time guidelines exist for this condition for 0 °C (32 °F) and below.
Heavy snow, ice pellets, moderate and heavy freezing rain, small hail and hail. 
No holdover time guidelines exist for this condition below -10 °C (14 °F).
CAUTIONS
The cautions that apply to the holdover times in the table above can be found on page A-27.

[bookmark: _Toc231475419]Table Adj-46: Adjusted Type IV Holdover Times for 
MAX TECH LLC MTL 4-PG
	Outside Air 
Temperature1
	Fluid 
Concentration 
Fluid/Water 
By % Volume
	Freezing Fog, Freezing Mist2, or Ice Crystals3
	Snow 
mixed with 
Freezing Fog4
	Very Light Snow, Snow Grains or Snow Pellets4,5
	Light 
Snow, Snow Grains or Snow Pellets4,5
	Moderate Snow, Snow Grains or Snow Pellets4,5
	Freezing 
Drizzle6
	Light 
Freezing Rain
	Moderate
Snow mixed with Rain7,8
	Rain on 
Cold‑Soaked Wing8
	Other9

	-3 °C and above
(27 °F and above)
	100/0
	1:50 - 3:02
	0:27 - 0:57
	2:55 - 3:00
	1:16 - 2:55
	0:34 - 1:16
	0:57 - 1:31
	0:42 - 0:53
	0:11 - 0:11
	0:15 - 1:08
	 

	
	75/25
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	 

	
	50/50
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	CAUTION: 
No holdover time 
guidelines exist

	below -3 to -8 °C
(below 27 to 18 °F)
	100/0
	1:12 - 2:59
	0:15 - 0:38
	1:58 - 2:32
	0:53 - 1:58
	0:23 - 0:53
	0:23 - 1:24
	0:11 - 0:23
	

	
	75/25
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	

	below -8 to -14 °C
(below 18 to 7 °F)
	100/0
	0:30 - 1:39
	0:11 - 0:30
	1:31 - 1:58
	0:38 - 1:31
	0:19 - 0:38
	0:19 - 1:0810
	0:11 - 0:2310
	

	
	75/25
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	

	below -14 to -18 °C
(below 7 to 0 °F)
	100/0
	0:23 - 1:08
	0:08 - 0:19
	0:46 - 0:57
	0:23 - 0:46
	0:11 - 0:23
	
	

	below -18 to -25 °C
(below 0 to -13 °F)
	100/0
	0:19 - 0:30
	0:05 - 0:11
	0:30 - 0:34
	0:15 - 0:30
	0:08 - 0:15
	
	

	below -25 to -27 °C
(below -13 to -17 °F)
	100/0
	0:19 - 0:30
	0:05 - 0:11
	0:27 - 0:30
	0:11 - 0:27
	0:06 - 0:11
	
	


THIS TABLE IS FOR USE WHEN FLAPS/SLATS ARE DEPLOYED PRIOR TO DE/ANTI-ICING. HOLDOVER TIMES HAVE BEEN ADJUSTED TO 76 PERCENT.
NOTES
1. Ensure that the lowest operational use temperature (LOUT) is respected. Consider use of Type I fluid when Type IV fluid cannot be used.
1. Freezing mist is best confirmed by observation. It is never reported by METAR; however, it can occur when mist is present at 0 °C (32 °F) and below. 
1. Use freezing fog holdover times in conditions of ice crystals mixed with freezing fog or freezing mist.
1. To determine snowfall intensity, the Snowfall Intensities as a Function of Prevailing Visibility table (Table 57) is required. No holdover times exist if the reported visibility correlates to a “heavy” precipitation intensity.
Use snow holdover times in conditions of very light, light, or moderate snow mixed with ice crystals.
Includes light, moderate and heavy freezing drizzle. Use light freezing rain holdover times if positive identification of freezing drizzle is not possible.
These holdover times apply to conditions of “moderate” precipitation intensity. In cases of very light or light snow mixed with light rain or drizzle, use light freezing rain holdover times. The Snowfall Intensities as a Function of Prevailing Visibility table (Table 57) is required to confirm the precipitation intensity. No holdover times exist if the reported visibility correlates to a “heavy” precipitation intensity.
No holdover time guidelines exist for this condition for 0 °C (32 °F) and below.
Heavy snow, ice pellets, moderate and heavy freezing rain, small hail and hail. 
No holdover time guidelines exist for this condition below -10 °C (14 °F).
CAUTIONS
The cautions that apply to the holdover times in the table above can be found on page A-27.
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MKS DevO Chemicals COREICEPHOB TYPE-IV PG
	Outside Air 
Temperature1
	Fluid 
Concentration 
Fluid/Water 
By % Volume
	Freezing Fog, Freezing Mist2, or Ice Crystals3
	Snow 
mixed with 
Freezing Fog4
	Very Light Snow, Snow Grains or Snow Pellets4,5
	Light 
Snow, Snow Grains or Snow Pellets4,5
	Moderate Snow, Snow Grains or Snow Pellets4,5
	Freezing 
Drizzle6
	Light 
Freezing Rain
	Moderate
Snow mixed with Rain7,8
	Rain on 
Cold‑Soaked Wing8
	Other9

	-3 °C and above
(27 °F and above)
	100/0
	1:46 - 2:55
	0:27 - 0:57
	2:47 - 3:00
	1:16 - 2:47
	0:34 - 1:16
	1:05 - 1:31
	0:38 - 1:01
	0:07 - 0:07
	0:08 - 1:16
	 

	
	75/25
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	 

	
	50/50
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	CAUTION: 
No holdover time 
guidelines exist

	below -3 to -8 °C
(below 27 to 18 °F)
	100/0
	0:11 - 0:27
	0:19 - 0:42
	1:58 - 2:32
	0:53 - 1:58
	0:27 - 0:53
	0:30 - 1:08
	0:15 - 0:27
	

	
	75/25
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	

	below -8 to -14 °C
(below 18 to 7 °F)
	100/0
	0:11 - 0:27
	0:15 - 0:34
	1:35 - 2:02
	0:42 - 1:35
	0:19 - 0:42
	0:30 - 1:0810
	0:15 - 0:2710
	

	
	75/25
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	

	below -14 to -18 °C
(below 7 to 0 °F)
	100/0
	0:11 - 0:23
	0:01 - 0:05
	0:23 - 0:34
	0:07 - 0:23
	0:02 - 0:07
	
	

	below -18 to -25 °C
(below 0 to -13 °F)
	100/0
	0:11 - 0:23
	0:00 - 0:02
	0:08 - 0:15
	0:02 - 0:08
	0:01 - 0:02
	
	

	below -25 to -29 °C
(below -13 to -20 °F)
	100/0
	0:11 - 0:23
	0:00 - 0:01
	0:05 - 0:08
	0:02 - 0:05
	0:00 - 0:02
	
	


THIS TABLE IS FOR USE WHEN FLAPS/SLATS ARE DEPLOYED PRIOR TO DE/ANTI-ICING. HOLDOVER TIMES HAVE BEEN ADJUSTED TO 76 PERCENT.
NOTES
1. Ensure that the lowest operational use temperature (LOUT) is respected. Consider use of Type I fluid when Type IV fluid cannot be used.
1. Freezing mist is best confirmed by observation. It is never reported by METAR; however, it can occur when mist is present at 0 °C (32 °F) and below. 
1. Use freezing fog holdover times in conditions of ice crystals mixed with freezing fog or freezing mist.
1. To determine snowfall intensity, the Snowfall Intensities as a Function of Prevailing Visibility table (Table 57) is required. No holdover times exist if the reported visibility correlates to a “heavy” precipitation intensity.
Use snow holdover times in conditions of very light, light, or moderate snow mixed with ice crystals.
Includes light, moderate and heavy freezing drizzle. Use light freezing rain holdover times if positive identification of freezing drizzle is not possible.
These holdover times apply to conditions of “moderate” precipitation intensity. In cases of very light or light snow mixed with light rain or drizzle, use light freezing rain holdover times. The Snowfall Intensities as a Function of Prevailing Visibility table (Table 57) is required to confirm the precipitation intensity. No holdover times exist if the reported visibility correlates to a “heavy” precipitation intensity.
No holdover time guidelines exist for this condition for 0 °C (32 °F) and below.
Heavy snow, ice pellets, moderate and heavy freezing rain, small hail and hail.
No holdover time guidelines exist for this condition below -10 °C (14 °F).
CAUTIONS
The cautions that apply to the holdover times in the table above can be found on page A-27. 

[bookmark: _Toc231475421]Table Adj-48: Adjusted Type IV Holdover Times for
Newave Aerochemical FCY 9311
	Outside Air 
Temperature1
	Fluid 
Concentration 
Fluid/Water 
By % Volume
	Freezing Fog, Freezing Mist2, or Ice Crystals3
	Snow 
mixed with 
Freezing Fog4
	Very Light Snow, Snow Grains or Snow Pellets4,5
	Light 
Snow, Snow Grains or Snow Pellets4,5
	Moderate Snow, Snow Grains or Snow Pellets4,5
	Freezing 
Drizzle6
	Light 
Freezing Rain
	Moderate
Snow mixed with Rain7,8
	Rain on 
Cold‑Soaked Wing8
	Other9

	-3 °C and above
(27 °F and above)
	100/0
	1:27 - 3:02
	0:19 - 0:42
	1:46 - 2:13
	0:53 - 1:46
	0:27 - 0:53
	0:53 - 1:31
	0:30 - 0:49
	0:07 - 0:07
	0:11 - 1:05
	 

	
	75/25
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	 

	
	50/50
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	CAUTION: 
No holdover time 
guidelines exist

	below -3 to -8 °C
(below 27 to 18 °F)
	100/0
	0:27 - 1:35
	0:15 - 0:30
	1:24 - 1:46
	0:42 - 1:24
	0:23 - 0:42
	0:27 - 1:01
	0:15 - 0:27
	

	
	75/25
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	

	below -8 to -14 °C
(below 18 to 7 °F)
	100/0
	0:27 - 1:35
	0:15 - 0:27
	1:12 - 1:31
	0:38 - 1:12
	0:19 - 0:38
	0:27 - 1:0110
	0:15 - 0:2710
	

	
	75/25
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	

	below -14 to -18 °C
(below 7 to 0 °F)
	100/0
	0:23 - 0:42
	0:08 - 0:15
	0:46 - 0:57
	0:23 - 0:46
	0:11 - 0:23
	
	

	below -18 to -25 °C
(below 0 to -13 °F)
	100/0
	0:23 - 0:42
	0:04 - 0:08
	0:27 - 0:30
	0:11 - 0:27
	0:05 - 0:11
	
	

	below -25 to -29.5 °C
(below -13 to -21 °F)
	100/0
	0:23 - 0:42
	0:04 - 0:08
	0:23 - 0:30
	0:11 - 0:23
	0:05 - 0:11
	
	


THIS TABLE IS FOR USE WHEN FLAPS/SLATS ARE DEPLOYED PRIOR TO DE/ANTI-ICING. HOLDOVER TIMES HAVE BEEN ADJUSTED TO 76 PERCENT.
NOTES
1. Ensure that the lowest operational use temperature (LOUT) is respected. Consider use of Type I fluid when Type IV fluid cannot be used.
1. Freezing mist is best confirmed by observation. It is never reported by METAR; however, it can occur when mist is present at 0 °C (32 °F) and below. 
1. Use freezing fog holdover times in conditions of ice crystals mixed with freezing fog or freezing mist.
1. To determine snowfall intensity, the Snowfall Intensities as a Function of Prevailing Visibility table (Table 57) is required. No holdover times exist if the reported visibility correlates to a “heavy” precipitation intensity.
Use snow holdover times in conditions of very light, light, or moderate snow mixed with ice crystals.
Includes light, moderate and heavy freezing drizzle. Use light freezing rain holdover times if positive identification of freezing drizzle is not possible.
These holdover times apply to conditions of “moderate” precipitation intensity. In cases of very light or light snow mixed with light rain or drizzle, use light freezing rain holdover times. The Snowfall Intensities as a Function of Prevailing Visibility table (Table 57) is required to confirm the precipitation intensity. No holdover times exist if the reported visibility correlates to a “heavy” precipitation intensity.
No holdover time guidelines exist for this condition for 0 °C (32 °F) and below.
Heavy snow, ice pellets, moderate and heavy freezing rain, small hail and hail (Table Adj-55 provides adjusted allowance times for Type IV PG fluids in ice pellets and small hail).
No holdover time guidelines exist for this condition below -10 °C (14 °F).
CAUTIONS
The cautions that apply to the holdover times in the table above can be found on page A-27.

[bookmark: _Toc75345496][bookmark: _Toc77777062][bookmark: _Toc77777112][bookmark: _Toc105048955][bookmark: _Toc105049309][bookmark: _Toc105049432][bookmark: _Toc105399249][bookmark: _Toc105399460][bookmark: _Toc107305610][bookmark: _Toc231475422][bookmark: _Toc517088977][bookmark: _Toc517253634][bookmark: _Toc519674737][bookmark: _Toc519674844][bookmark: _Toc520288596][bookmark: _Toc520289468][bookmark: _Toc9500376][bookmark: _Toc14166586][bookmark: _Toc14867923][bookmark: _Toc43986239][bookmark: _Toc44053705][bookmark: _Toc44054124][bookmark: _Toc45715358]Table Adj-49: Adjusted Type IV Holdover Times for
Newave Aerochemical FCY-EGIV
	Outside Air 
Temperature1
	Fluid 
Concentration 
Fluid/Water 
By % Volume
	Freezing Fog, Freezing Mist2, or Ice Crystals3
	Snow 
mixed with 
Freezing Fog4
	Very Light Snow, Snow Grains or Snow Pellets4,5
	Light 
Snow, Snow Grains or Snow Pellets4,5
	Moderate Snow, Snow Grains or Snow Pellets4,5
	Freezing 
Drizzle6
	Light 
Freezing Rain
	Moderate
Snow mixed with Rain7,8
	Rain on 
Cold‑Soaked Wing8
	Other9

	-3 °C and above
(27 °F and above)
	100/0
	1:58 - 3:02
	0:19 - 0:42
	1:58 - 2:32
	0:53 - 1:58
	0:27 - 0:53
	1:01 - 1:31
	0:30 - 0:49
	0:08 - 0:08
	0:11 - 1:31
	 

	
	75/25
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	 

	
	50/50
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	CAUTION: 
No holdover time 
guidelines exist

	below -3 to -8 °C
(below 27 to 18 °F)
	100/0
	1:05 - 2:36
	0:15 - 0:34
	1:39 - 2:05
	0:46 - 1:39
	0:19 - 0:46
	0:38 - 1:31
	0:34 - 0:49
	

	
	75/25
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	

	below -8 to -14 °C
(below 18 to 7 °F)
	100/0
	1:05 - 2:36
	0:15 - 0:30
	1:27 - 1:50
	0:38 - 1:27
	0:19 - 0:38
	0:38 - 1:3110
	0:34 - 0:4910
	

	
	75/25
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	

	below -14 to -18 °C
(below 7 to 0 °F)
	100/0
	0:27 - 1:27
	0:11 - 0:23
	1:12 - 1:35
	0:30 - 1:12
	0:11 - 0:30
	
	

	below -18 to -25 °C
(below 0 to -13 °F)
	100/0
	0:27 - 1:27
	0:07 - 0:15
	0:53 - 1:12
	0:23 - 0:53
	0:11 - 0:23
	
	

	below -25 to -29 °C
(below -13 to -20 °F)
	100/0
	0:27 - 1:27
	0:06 - 0:15
	0:46 - 1:01
	0:19 - 0:46
	0:08 - 0:19
	
	


THIS TABLE IS FOR USE WHEN FLAPS/SLATS ARE DEPLOYED PRIOR TO DE/ANTI-ICING. HOLDOVER TIMES HAVE BEEN ADJUSTED TO 76 PERCENT.
NOTES
1. Ensure that the lowest operational use temperature (LOUT) is respected. Consider use of Type I fluid when Type IV fluid cannot be used.
1. Freezing mist is best confirmed by observation. It is never reported by METAR; however, it can occur when mist is present at 0 °C (32 °F) and below. 
1. Use freezing fog holdover times in conditions of ice crystals mixed with freezing fog or freezing mist.
1. To determine snowfall intensity, the Snowfall Intensities as a Function of Prevailing Visibility table (Table 57) is required. No holdover times exist if the reported visibility correlates to a “heavy” precipitation intensity.
Use snow holdover times in conditions of very light, light, or moderate snow mixed with ice crystals.
Includes light, moderate and heavy freezing drizzle. Use light freezing rain holdover times if positive identification of freezing drizzle is not possible.
These holdover times apply to conditions of “moderate” precipitation intensity. In cases of very light or light snow mixed with light rain or drizzle, use light freezing rain holdover times. The Snowfall Intensities as a Function of Prevailing Visibility table (Table 57) is required to confirm the precipitation intensity. No holdover times exist if the reported visibility correlates to a “heavy” precipitation intensity.
No holdover time guidelines exist for this condition for 0 °C (32 °F) and below.
Heavy snow, ice pellets, moderate and heavy freezing rain, small hail and hail (Table Adj-54 provides adjusted allowance times for Type IV EG fluids in ice pellets and small hail).
No holdover time guidelines exist for this condition below -10 °C (14 °F).
CAUTIONS
The cautions that apply to the holdover times in the table above can be found on page A-27.

[bookmark: _Toc231475423]Table Adj-50: Adjusted Type IV Holdover Times for 
Newave Aerochemical FCY-EGIV PLUS
	Outside Air 
Temperature1
	Fluid 
Concentration 
Fluid/Water 
By % Volume
	Freezing Fog, Freezing Mist2, or Ice Crystals3
	Snow 
mixed with 
Freezing Fog4
	Very Light Snow, Snow Grains or Snow Pellets4,5
	Light 
Snow, Snow Grains or Snow Pellets4,5
	Moderate Snow, Snow Grains or Snow Pellets4,5
	Freezing 
Drizzle6
	Light 
Freezing Rain
	Moderate
Snow mixed with Rain7,8
	Rain on 
Cold‑Soaked Wing8
	Other9

	-3 °C and above
(27 °F and above)
	100/0
	2:21 - 3:02
	0:23 - 0:46
	2:09 - 2:43
	1:01 - 2:09
	0:30 - 1:01
	0:57 - 1:31
	0:30 - 0:42
	0:08 - 0:08
	0:11 - 1:31
	 

	
	75/25
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	 

	
	50/50
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	CAUTION: 
No holdover time 
guidelines exist

	below -3 to -8 °C
(below 27 to 18 °F)
	100/0
	1:12 - 2:28
	0:19 - 0:38
	1:43 - 2:13
	0:49 - 1:43
	0:23 - 0:49
	0:57 - 1:31
	0:23 - 0:34
	

	
	75/25
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	

	below -8 to -14 °C
(below 18 to 7 °F)
	100/0
	1:12 - 2:28
	0:15 - 0:30
	1:31 - 1:54
	0:42 - 1:31
	0:19 - 0:42
	0:57 - 1:3110
	0:23 - 0:3410
	

	
	75/25
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	

	below -14 to -18 °C
(below 7 to 0 °F)
	100/0
	0:23 - 0:53
	0:11 - 0:23
	1:08 - 1:27
	0:30 - 1:08
	0:15 - 0:30
	
	

	below -18 to -25 °C
(below 0 to -13 °F)
	100/0
	0:23 - 0:53
	0:07 - 0:15
	0:49 - 1:05
	0:23 - 0:49
	0:11 - 0:23
	
	

	below -25 to -29 °C
(below -13 to -20 °F)
	100/0
	0:23 - 0:53
	0:06 - 0:15
	0:46 - 0:57
	0:19 - 0:46
	0:08 - 0:19
	
	


THIS TABLE IS FOR USE WHEN FLAPS/SLATS ARE DEPLOYED PRIOR TO DE/ANTI-ICING. HOLDOVER TIMES HAVE BEEN ADJUSTED TO 76 PERCENT.
NOTES
1. Ensure that the lowest operational use temperature (LOUT) is respected. Consider use of Type I fluid when Type IV fluid cannot be used.
1. Freezing mist is best confirmed by observation. It is never reported by METAR; however, it can occur when mist is present at 0 °C (32 °F) and below. 
1. Use freezing fog holdover times in conditions of ice crystals mixed with freezing fog or freezing mist.
1. To determine snowfall intensity, the Snowfall Intensities as a Function of Prevailing Visibility table (Table 57) is required. No holdover times exist if the reported visibility correlates to a “heavy” precipitation intensity.
Use snow holdover times in conditions of very light, light, or moderate snow mixed with ice crystals.
Includes light, moderate and heavy freezing drizzle. Use light freezing rain holdover times if positive identification of freezing drizzle is not possible.
These holdover times apply to conditions of “moderate” precipitation intensity. In cases of very light or light snow mixed with light rain or drizzle, use light freezing rain holdover times. The Snowfall Intensities as a Function of Prevailing Visibility table (Table 57) is required to confirm the precipitation intensity. No holdover times exist if the reported visibility correlates to a “heavy” precipitation intensity.
No holdover time guidelines exist for this condition for 0 °C (32 °F) and below.
Heavy snow, ice pellets, moderate and heavy freezing rain, small hail and hail.
No holdover time guidelines exist for this condition below -10 °C (14 °F).
CAUTIONS
The cautions that apply to the holdover times in the table above can be found on page A-27.

[bookmark: _Toc231475424]Table Adj-51: Adjusted Type IV Holdover Times for 
Shaanxi Cleanway Cleansurface IV
	Outside Air 
Temperature1
	Fluid 
Concentration 
Fluid/Water 
By % Volume
	Freezing Fog, Freezing Mist2, or Ice Crystals3
	Snow 
mixed with 
Freezing Fog4
	Very Light Snow, Snow Grains or Snow Pellets4,5
	Light 
Snow, Snow Grains or Snow Pellets4,5
	Moderate Snow, Snow Grains or Snow Pellets4,5
	Freezing 
Drizzle6
	Light 
Freezing Rain
	Moderate
Snow mixed with Rain7,8
	Rain on 
Cold‑Soaked Wing8
	Other9

	-3 °C and above
(27 °F and above)
	100/0
	1:54 - 3:02
	0:23 - 0:57
	2:51 - 3:00
	1:16 - 2:51
	0:30 - 1:16
	1:01 - 1:31
	0:30 - 0:53
	0:07 - 0:07
	0:11 - 1:24
	 

	
	75/25
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	 

	
	50/50
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	CAUTION: 
No holdover time 
guidelines exist

	below -3 to -8 °C
(below 27 to 18 °F)
	100/0
	0:42 - 1:35
	0:15 - 0:34
	1:50 - 2:21
	0:46 - 1:50
	0:19 - 0:46
	0:23 - 1:08
	0:19 - 0:27
	

	
	75/25
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	

	below -8 to -14 °C
(below 18 to 7 °F)
	100/0
	0:42 - 1:35
	0:11 - 0:27
	1:20 - 1:43
	0:34 - 1:20
	0:15 - 0:34
	0:23 - 1:0810
	0:19 - 0:2710
	

	
	75/25
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	

	below -14 to -18 °C
(below 7 to 0 °F)
	100/0
	0:19 - 0:27
	0:08 - 0:15
	0:49 - 1:01
	0:23 - 0:49
	0:11 - 0:23
	
	

	below -18 to -25 °C
(below 0 to -13 °F)
	100/0
	0:19 - 0:27
	0:04 - 0:08
	0:27 - 0:34
	0:11 - 0:27
	0:05 - 0:11
	
	

	below -25 to -30 °C
(below -13 to -22 °F)
	100/0
	0:15 - 0:23
	0:03 - 0:07
	0:23 - 0:27
	0:11 - 0:23
	0:05 - 0:11
	
	


THIS TABLE IS FOR USE WHEN FLAPS/SLATS ARE DEPLOYED PRIOR TO DE/ANTI-ICING. HOLDOVER TIMES HAVE BEEN ADJUSTED TO 76 PERCENT.
NOTES
1. Ensure that the lowest operational use temperature (LOUT) is respected. Consider use of Type I fluid when Type IV fluid cannot be used.
1. Freezing mist is best confirmed by observation. It is never reported by METAR; however, it can occur when mist is present at 0 °C (32 °F) and below. 
1. Use freezing fog holdover times in conditions of ice crystals mixed with freezing fog or freezing mist.
1. To determine snowfall intensity, the Snowfall Intensities as a Function of Prevailing Visibility table (Table 57) is required. No holdover times exist if the reported visibility correlates to a “heavy” precipitation intensity.
Use snow holdover times in conditions of very light, light, or moderate snow mixed with ice crystals.
Includes light, moderate and heavy freezing drizzle. Use light freezing rain holdover times if positive identification of freezing drizzle is not possible.
These holdover times apply to conditions of “moderate” precipitation intensity. In cases of very light or light snow mixed with light rain or drizzle, use light freezing rain holdover times. The Snowfall Intensities as a Function of Prevailing Visibility table (Table 57) is required to confirm the precipitation intensity. No holdover times exist if the reported visibility correlates to a “heavy” precipitation intensity.
No holdover time guidelines exist for this condition for 0 °C (32 °F) and below.
Heavy snow, ice pellets, moderate and heavy freezing rain, small hail and hail. 
No holdover time guidelines exist for this condition below -10 °C (14 °F).
CAUTIONS
The cautions that apply to the holdover times in the table above can be found on page A-27.

[bookmark: _Toc231475425]Table Adj-52: Adjusted Type IV Holdover Times for 
Xinjiang Zhongtian Liyang Aviation Clearice-IV
	Outside Air 
Temperature1
	Fluid 
Concentration 
Fluid/Water 
By % Volume
	Freezing Fog, Freezing Mist2, or Ice Crystals3
	Snow 
mixed with 
Freezing Fog4
	Very Light Snow, Snow Grains or Snow Pellets4,5
	Light 
Snow, Snow Grains or Snow Pellets4,5
	Moderate Snow, Snow Grains or Snow Pellets4,5
	Freezing 
Drizzle6
	Light 
Freezing Rain
	Moderate
Snow mixed with Rain7,8
	Rain on 
Cold‑Soaked Wing8
	Other9

	-3 °C and above
(27 °F and above)
	100/0
	1:50 - 3:02
	0:19 - 0:38
	1:43 - 2:09
	0:49 - 1:43
	0:23 - 0:49
	0:49 - 1:27
	0:27 - 0:42
	0:07 - 0:07
	0:11 - 1:08
	 

	
	75/25
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	 

	
	50/50
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	CAUTION: 
No holdover time 
guidelines exist

	below -3 to -8 °C
(below 27 to 18 °F)
	100/0
	1:01 - 1:39
	0:15 - 0:30
	1:24 - 1:46
	0:42 - 1:24
	0:19 - 0:42
	0:42 - 1:12
	0:27 - 0:38
	

	
	75/25
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	

	below -8 to -14 °C
(below 18 to 7 °F)
	100/0
	1:01 - 1:39
	0:11 - 0:27
	1:12 - 1:31
	0:34 - 1:12
	0:15 - 0:34
	0:42 - 1:1210
	0:27 - 0:3810
	

	
	75/25
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	

	below -14 to -18 °C
(below 7 to 0 °F)
	100/0
	0:23 - 0:46
	0:11 - 0:23
	0:57 - 1:12
	0:30 - 0:57
	0:15 - 0:30
	
	

	below -18 to -25 °C
(below 0 to -13 °F)
	100/0
	0:23 - 0:46
	0:11 - 0:19
	0:53 - 1:05
	0:27 - 0:53
	0:11 - 0:27
	
	

	below -25 to -29 °C
(below -13 to -20 °F)
	100/0
	0:23 - 0:46
	0:08 - 0:19
	0:49 - 1:01
	0:23 - 0:49
	0:11 - 0:23
	
	


THIS TABLE IS FOR USE WHEN FLAPS/SLATS ARE DEPLOYED PRIOR TO DE/ANTI-ICING. HOLDOVER TIMES HAVE BEEN ADJUSTED TO 76 PERCENT.
NOTES
1. Ensure that the lowest operational use temperature (LOUT) is respected. Consider use of Type I fluid when Type IV fluid cannot be used.
1. Freezing mist is best confirmed by observation. It is never reported by METAR; however, it can occur when mist is present at 0 °C (32 °F) and below. 
1. Use freezing fog holdover times in conditions of ice crystals mixed with freezing fog or freezing mist.
1. To determine snowfall intensity, the Snowfall Intensities as a Function of Prevailing Visibility table (Table 57) is required. No holdover times exist if the reported visibility correlates to a “heavy” precipitation intensity.
Use snow holdover times in conditions of very light, light, or moderate snow mixed with ice crystals.
Includes light, moderate and heavy freezing drizzle. Use light freezing rain holdover times if positive identification of freezing drizzle is not possible.
These holdover times apply to conditions of “moderate” precipitation intensity. In cases of very light or light snow mixed with light rain or drizzle, use light freezing rain holdover times. The Snowfall Intensities as a Function of Prevailing Visibility table (Table 57) is required to confirm the precipitation intensity. No holdover times exist if the reported visibility correlates to a “heavy” precipitation intensity.
No holdover time guidelines exist for this condition for 0 °C (32 °F) and below.
Heavy snow, ice pellets, moderate and heavy freezing rain, small hail and hail. 
No holdover time guidelines exist for this condition below -10 °C (14 °F).
CAUTIONS
The cautions that apply to the holdover times in the table above can be found on page A-27.
Appendix A: FAA Adjusted Holdover Time Guidelines	Winter 2026-2027

Original Issue	Page A-37	August 11, 2026
[bookmark: SnowZFogCautionsAdj][bookmark: _Toc107305614][bookmark: _Toc231475426]Adjusted Allowance Times Tables for Winter 2026-2027

The HOT Guidelines are provided for information and guidance purposes. The HOT Guidelines on their own do not change, create, amend or permit deviations from regulatory requirements.

The HOT Guidelines may use mandatory terms such as “must”, “shall” and “is/are required” so as to convey the intent of meeting regulatory requirements and SAE Standards, where applicable. The term “should” is to be understood, unless an alternative method of achieving safety is implemented that would meet or exceed the intent of the recommendation.



[bookmark: AllowanceTimesCautionsAdj]CAUTIONS
The responsibility for the application of these data remains with the user.
Fluids used during ground de/anti-icing do not provide in-flight icing protection. 
This table is for departure planning only and should be used in conjunction with pre-takeoff check procedures.
Allowance time cannot be extended by an inspection of the aircraft critical surfaces. 
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[bookmark: _TABLE_6-90%._90][bookmark: _Ref75337960][bookmark: _Toc75345498][bookmark: _Toc77777064][bookmark: _Toc77777114][bookmark: _Toc105048957][bookmark: _Toc105049311][bookmark: _Toc105049434][bookmark: _Toc105399251][bookmark: _Toc105399462][bookmark: _Toc107305615][bookmark: _Toc231475427][bookmark: _Ref9506000][bookmark: _Toc517088979][bookmark: _Toc517253636][bookmark: _Toc519674739][bookmark: _Toc519674846][bookmark: _Toc520288598][bookmark: _Toc520289470][bookmark: _Toc9500378][bookmark: _Toc14166588][bookmark: _Toc14867925][bookmark: _Toc43986241][bookmark: _Toc44053707][bookmark: _Toc44054126][bookmark: _Toc45715360]Table Adj-53: Adjusted Allowance Times for SAE Type III Fluids1,2
	Precipitation Types or Combinations
and Applicable METAR Codes4
	Outside Air Temperature3

	
	Above 0 °C
(Above 32 °F)
	0 to -5 °C
(32 to 23 °F)
	Below -5 
to -10 °C
(Below 23 to 14 °F)
	Below -10 °C
(Below 14 °F)

	Light Ice Pellets (or Small Hail5,6)
-PL
	8 minutes
	8 minutes 
	8 minutes 
	Caution: 
No allowance times currently exist

	Light Ice Pellets (or Small Hail5,6) Mixed with Light Snow 
-PLSN, -SNPL
	8 minutes 
	8 minutes 
	8 minutes
	

	Light Ice Pellets (or Small Hail5,6) Mixed with Light Freezing Drizzle 

-PLFZDZ, -FZDZPL
	
	5 minutes 
	4 minutes 
	

	Light Ice Pellets (or Small Hail5,6) Mixed with Light Drizzle
-PLDZ, -DZPL
	5 minutes
	
	

	Light Ice Pellets (or Small Hail5,6) Mixed with Light Freezing Rain 
-PLFZRA, -FZRAPL
	
	5 minutes
	4 minutes 
	

	Light Ice Pellets (or Small Hail5,6) Mixed with Light Rain 
-PLRA, -RAPL
	5 minutes
	
	

	Moderate Ice Pellets (or Small Hail5,6) 
PL
	4 minutes 
	4 minutes 
	4 minutes 
	


THIS TABLE IS FOR USE WHEN FLAPS/SLATS ARE DEPLOYED PRIOR TO DE/ANTI-ICING. ALLOWANCE TIMES HAVE BEEN ADJUSTED TO 76 PERCENT.
NOTES
1. These allowance times are for use with undiluted (100/0) fluids applied unheated on aircraft with rotation speeds of 100 knots or greater. To use the allowance times in this table, ensure the fluid being used is listed in the Validation Status of Fluids for Use with Allowance Times (Table 53).
Takeoff is allowed up to 90 minutes after start of fluid application if the precipitation stops at or before the allowance time expires and does not restart. Takeoff is not permitted if the OAT decreases during the 90 minutes in conditions of light ice pellets mixed with either: light freezing drizzle; light drizzle; light freezing rain; or light rain.
Ensure that the lowest operational use temperature (LOUT) is respected. 
Applicable METAR codes include only Ice Pellet conditions (i.e., PL). While allowance times can be used when Small Hail is reported instead of Ice Pellets, the corresponding METAR codes for Small Hail are not listed in the table.
The reporting of Small Hail by METAR varies by country, which can result in different HOTs or allowance times when the same METAR code is used in different regions. For details, refer to the METAR Codes and Holdover or Allowance Times Used by Country table in the FAA Ground Deicing Program General Information Document.
If the METAR does not report an intensity for small hail, use the “moderate ice pellets or small hail” allowance times. If the METAR reports an intensity with small hail, the condition with the equivalent intensity can be used, e.g., if light small hail is reported, the “light ice pellets” allowance times can be used. This also applies in mixed conditions, e.g., if light small hail mixed with light snow is reported, use the “light ice pellets mixed with light snow” allowance times.
CAUTIONS
The cautions that apply to the allowance times in the table above can be found on page A-61.


[bookmark: _Ref75338163][bookmark: _Toc75345499][bookmark: _Toc77777065][bookmark: _Toc77777115][bookmark: _Toc105048958][bookmark: _Toc105049312][bookmark: _Toc105049435][bookmark: _Toc105399252][bookmark: _Toc105399463][bookmark: _Toc107305616][bookmark: _Toc231475428]Table Adj-54: Adjusted Allowance Times for SAE Type IV
Ethylene Glycol (EG) Fluids1,2
	Precipitation Types or Combinations 
and Applicable METAR Codes5
	Outside Air Temperature3

	
	Above 0 °C4
(Above 32 °F)
	0 to -5 °C4
(32 to 23 °F)
	Below -5 
to -10 °C4
(Below 23 to 14 °F)
	Below -10 
to -16 °C4
(Below 14 to 3 °F)
	Below -16 
to -22 °C4
(Below 3 to -8 °F)

	Light Ice Pellets (or Small Hail6,7)
-PL
	53 minutes
	53 minutes
	53 minutes
	38 minutes
	23 minutes

	Light Ice Pellets (or Small Hail6,7) Mixed with Light Snow 
-PLSN, -SNPL
	38 minutes
	38 minutes
	23 minutes
	19 minutes
	

	Light Ice Pellets (or Small Hail6,7) Mixed with Light Freezing Drizzle 
-PLFZDZ, -FZDZPL
	
	30 minutes
	23 minutes
	Caution: 
No allowance times 
currently exist

	Light Ice Pellets (or Small Hail6,7) Mixed with Light Drizzle
-PLDZ, -DZPL
	30 minutes
	
	

	Light Ice Pellets (or Small Hail6,7) Mixed with Light Freezing Rain 
-PLFZRA, -FZRAPL
	
	30 minutes
	23 minutes
	

	Light Ice Pellets (or Small Hail6,7) Mixed with Light Rain 
-PLRA, -RAPL
	30 minutes
	
	

	Light Ice Pellets (or Small Hail6,7) Mixed with Light Freezing Rain and Light Snow
-PLFZRASN, -PLSNFZRA, -FZRAPLSN, 
-FZRASNPL, -SNPLFZRA, -SNFZRAPL 
	
	15 minutes
	
	

	Light Ice Pellets (or Small Hail6,7) Mixed with Light Rain and Light Snow
-PLRASN, -PLSNRA, -RAPLSN, -RASNPL, 
-SNPLRA, -SNRAPL
	15 minutes
	
	

	Moderate Ice Pellets (or Small Hail6,7) 
PL
	27 minutes
	27 minutes
	27 minutes
	11 minutes
	8 minutes

	Moderate Ice Pellets (or Small Hail6,7)
Mixed with Moderate Snow
PLSN, SNPL
	19 minutes
	19 minutes
	11 minutes
	8 minutes
	

	Moderate Ice Pellets (or Small Hail6,7) Mixed with Light or Moderate Freezing Drizzle 
PLFZDZ, FZDZPL
	
	15 minutes
	8 minutes
	
	

	Moderate Ice Pellets (or Small Hail6,7) Mixed with Light or Moderate Drizzle
PLDZ, DZPL
	15 minutes
	Caution: 
No allowance times 
currently exist 

	Moderate Ice Pellets (or Small Hail6,7) Mixed with Moderate Rain 
PLRA, RAPL
	11 minutes
	


THIS TABLE IS FOR USE WHEN FLAPS/SLATS ARE DEPLOYED PRIOR TO DE/ANTI-ICING. ALLOWANCE TIMES HAVE BEEN ADJUSTED TO 76 PERCENT.
NOTES
The notes that apply to the allowance times in the table above can be found on page A-64.
CAUTIONS
The cautions that apply to the allowance times in the table above can be found on page A-61.

Table Adj-54 (CONT’D): ADJUSTED ALLOWANCE TIMES FOR SAE TYPE IV
EthYLENE GLYCOL (EG) FLUIDS
NOTES
1. [bookmark: _Ref199241689]These allowance times are for use with undiluted (100/0) EG-based fluids. To use the allowance times in this table, ensure the fluid being used is listed in the Validation Status of Fluids for Use with Allowance Times (Table 53).
1. Takeoff is allowed up to 90 minutes after start of fluid application if the precipitation stops at or before the allowance time expires and does not restart. Takeoff is not permitted if the OAT decreases during the 90 minutes in conditions of light ice pellets mixed with either: light freezing drizzle; light drizzle; light freezing rain; light rain; light rain and light snow; or light freezing rain and light snow, as well as in conditions of moderate ice pellets mixed with either: light or moderate freezing drizzle; light or moderate drizzle; or moderate rain.
1. Ensure that the lowest operational use temperature (LOUT) is respected.
368 No allowance times exist for EG-based fluids when used on aircraft with rotation speeds less than 100 knots. 
369 Applicable METAR codes include only Ice Pellet conditions (i.e., PL). While allowance times can be used when Small Hail is reported instead of Ice Pellets, the corresponding METAR codes for Small Hail are not listed in the table.
The reporting of Small Hail by METAR varies by country, which can result in different HOTs or allowance times when the same METAR code is used in different regions. For details, refer to the METAR Codes and Holdover or Allowance Times Used by Country table in the FAA Ground Deicing Program General Information Document.
370 If the METAR does not report an intensity for small hail, use the “moderate ice pellets or small hail” allowance times. If the METAR reports an intensity with small hail, the condition with the equivalent intensity can be used, e.g., if light small hail is reported, the “light ice pellets” allowance times can be used. This also applies in mixed conditions, e.g., if light small hail mixed with light snow is reported, use the “light ice pellets mixed with light snow” allowance times.
[bookmark: _Ref190167275][bookmark: _Ref199241802][bookmark: _Toc231475429]
Table Adj-55: Adjusted Allowance Times for SAE Type IV
Propylene Glycol (PG) Fluids1,2
	Precipitation Types or Combinations
and Applicable METAR Codes6
	Outside Air Temperature3

	
	Above 0 °C4
 (Above 32 °F)
	0 to -5 °C4
(32 to 23 °F)
	Below -5 
to -10 °C4
(Below 23 to 14 °F)
	Below -10 
to -16 °C5
(Below 14 to 3 °F)
	Below -16 
to -22 °C5
(Below 3 to -8 °F)

	Light Ice Pellets (or Small Hail7,8)
-PL
	38 minutes
	38 minutes
	23 minutes
	23 minutes
	15 minutes

	Light Ice Pellets (or Small Hail7,8) Mixed with Light Snow
-PLSN, -SNPL
	30 minutes
	30 minutes
	11 minutes
	11 minutes
	

	Light Ice Pellets (or Small Hail7,8) Mixed with Light Freezing Drizzle 
-PLFZDZ, -FZDZPL
	
	19 minutes
	8 minutes
	Caution: 
No allowance times 
currently exist

	Light Ice Pellets (or Small Hail7,8) Mixed with Light Drizzle
-PLDZ, -DZPL
	19 minutes
	
	

	Light Ice Pellets (or Small Hail7,8) Mixed with Light Freezing Rain
-PLFZRA, -FZRAPL
	
	19 minutes
	8 minutes
	

	Light Ice Pellets (or Small Hail7,8) Mixed with Light Rain
-PLRA, -RAPL
	19 minutes
	
	
	

	Light Ice Pellets (or Small Hail7,8) Mixed with Light Freezing Rain and Light Snow
-PLFZRASN, -PLSNFZRA, -FZRAPLSN, 
-FZRASNPL, -SNPLFZRA, -SNFZRAPL 
	
	15 minutes
	
	

	Light Ice Pellets (or Small Hail7,8) Mixed with Light Rain and Light Snow
-PLRASN, -PLSNRA, -RAPLSN, -RASNPL, 
-SNPLRA, -SNRAPL
	15 minutes
	
	
	

	Moderate Ice Pellets (or Small Hail7,8)
PL
	11 minutes
	11 minutes
	8 minutes
	8 minutes
	

	Moderate Ice Pellets (or Small Hail7,8)
Mixed with Moderate Snow
PLSN, SNPL
	11 minutes
	11 minutes
	4 minutes
	4 minutes
	

	Moderate Ice Pellets (or Small Hail7,8) Mixed with Light or Moderate Freezing Drizzle
PLFZDZ, FZDZPL
	
	8 minutes
	5 minutes
	
	

	Moderate Ice Pellets (or Small Hail7,8) Mixed with Light or Moderate Drizzle
PLDZ, DZPL
	8 minutes
	Caution: 
No allowance times 
currently exist 

	Moderate Ice Pellets (or Small Hail7,8) Mixed with Moderate Rain
PLRA, RAPL
	8 minutes
	


THIS TABLE IS FOR USE WHEN FLAPS/SLATS ARE DEPLOYED PRIOR TO DE/ANTI-ICING. ALLOWANCE TIMES HAVE BEEN ADJUSTED TO 76 PERCENT.
NOTES
The notes that apply to the allowance times in the table above can be found on page A-66.
CAUTIONS
The cautions that apply to the allowance times in the table above can be found on page A-61.

Table Adj-55 (CONT’D): ADJUSTED ALLOWANCE TIMES FOR SAE TYPE IV
PROPYLENE GLYCOL (PG) FLUIDS
NOTES
1. [bookmark: _Ref199241668]These allowance times are for use with undiluted (100/0) PG-based fluids applied on aircraft with rotation speeds of 100 knots or greater. To use the allowance times in this table, ensure the fluid being used is listed in the Validation Status of Fluids for Use with Allowance Times (Table 53).
Takeoff is allowed up to 90 minutes after start of fluid application if the precipitation stops at or before the allowance time expires and does not restart. Takeoff is not permitted if the OAT decreases during the 90 minutes in conditions of light ice pellets mixed with either: light freezing drizzle; light drizzle; light freezing rain; light rain; light rain and light snow; or light freezing rain and light snow, as well as in conditions of moderate ice pellets mixed with either: light or moderate freezing drizzle; light or moderate drizzle; or moderate rain.
Ensure that the lowest operational use temperature (LOUT) is respected.
No allowance times exist for PG-based fluids when used on aircraft with rotation speeds less than 100 knots. 
No allowance times exist for PG-based fluids when used on aircraft with rotation speeds less than 115 knots. 
Applicable METAR codes include only Ice Pellet conditions (i.e., PL). While allowance times can be used when Small Hail is reported instead of Ice Pellets, the corresponding METAR codes for Small Hail are not listed in the table.
The reporting of Small Hail by METAR varies by country, which can result in different HOTs or allowance times when the same METAR code is used in different regions. For details, refer to the METAR Codes and Holdover or Allowance Times Used by Country table in the FAA Ground Deicing Program General Information Document.
[bookmark: _Ref199241629]If the METAR does not report an intensity for small hail, use the “moderate ice pellets or small hail” allowance times. If the METAR reports an intensity with small hail, the condition with the equivalent intensity can be used, e.g., if light small hail is reported, the “light ice pellets” allowance times can be used. This also applies in mixed conditions, e.g., if light small hail mixed with light snow is reported, use the “light ice pellets mixed with light snow” allowance times.
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TESTING LABORATORIES
The following laboratories are known to provide testing for de/anti-icing fluids given they verifiably adhere to internationally accepted standards and recommended practices that are associated with the holdover times published by the FAA. 
Please enquire directly with the laboratories for a full list of testing available. 
· Anti-icing Materials International Laboratory (AMIL): 555, boulevard de l'Université, Chicoutimi, Québec, G7H 2B1, Canada, 418-545-5011 ext. 2406 www.lima.uqac.ca. Provides testing for anti-icing performance (described in AMS1424, AMS1428, and AS5901), aerodynamic acceptance (described in AMS1424, AMS1428 and AS5900), physical properties including fluid stability (described in AMS1424 and AMS1428), environmental information (described in AMS1424 and AMS1428) and most of tests to evaluate materials compatibility (described in AMS1424 and AMS1428). 
· APS Aviation Inc.: 6700, chemin de la Côte-de-Liesse, Suite 102, Saint-Laurent, Quebec, H4T 2B5, Canada, 514-878-4388 www.apsaviation.ca. Provides endurance time testing (described in ARP5485B and ARP5945A). 
· Scientific Material International (SMI): 12219 SW 131st Avenue, Miami, Florida, USA 33186-6401; 305‑971-7047, www.smiinc.com. Provides testing for physical properties including fluid stability (described in AMS1424 and AMS1428), environmental information (described in AMS1424 and AMS1428) and most of tests to evaluate materials compatibility (described in AMS1424 and AMS1428).
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Table C-1: ADF/AAF MANUFACTURERS CONTACT INFORMATION1
	Fluid Manufacturer
	Primary contact
	Email Address

	ABAX Industries
	Alejandra Villa Rodriguez
	a.rodriguez@abax.eu 

	ADDCON EUROPE GmbH
	Norman Kilian
	norman.kilian@addcon.com

	Aero Mag 2000 SYR LLC
	Mark Vilcek
	m.vilcek@aeromag2000.com

	AFLRUS LLC
	Olga Tengeri
	office@aflrus.qa

	ALAB Industries
	Marat Zhazbek
	info@alab.kz

	Alab International
	Kuanyshbay Bissenov
	deicing@alab.kz 

	AllClear Systems LLC
	Steve Szafara
	SSzafara@allclearsys.com

	Arcton Ltd.
	Bulat Hamitov
	bulathamitov@yandex.ru

	ASGlobal
	Paulo de Oliveira
	paulo@asglobal.biz

	AVIAFLUID International Ltd
	Igor Derbasov
	iderbasov@aviafluid.ru

	Aviation Xi’an High-Tech Physical Chemical Co. Ltd.
	Arella
	xiangaokelihua@163.com

	Beijing Wangye Aviation Chemical Product Co Ltd.
	Sina Gong
	hswgyh@sina.com

	Beijing Yadilite Aviation Advanced Materials Corporation
	Kewei Wang
	wangkewei@yadilite.com

	CHEMCO Inc.
	Claude Grenon
	claude.grenon@chemco-inc.com

	Chongqing Joba Chemical Co.,Ltd.
	Cherry Wang
	info@changfengchem.com 

	Clariant Produkte (Deutschland) GmbH
	Andreas Brueck
	andreas.brueck@clariant.com

	Cryotech Deicing Technology
	Melissa Copeland 
	melissa.copeland@cryotech.com 

	ESSPO CHEMICALS D.O.O.
	Lukas Pakeltis
	lukas@esspo.lt

	Dow Inc.
	Arash Nowbahar
	ARNowbahar@dow.com

	HOC Industries
	Jeremy Wilcoxson
	jwilcoxson@hocindustries.com

	Inland Technologies Inc.
	Alex McLeod
	amcleod@inlandgroup.ca

	JSC RCP Nordix
	Mikhail Rogozhin
	rogozhin@rhz.ru

	Kilfrost Limited
	Nicole McLeod
	nicole.mcleod@kilfrost.com

	LNT Solutions
	Philip Newton
	philip.newton@lntsolutions.com

	MAX TECH AIRCRAFT MAINTENANCE AND REPAIR LLC
	Alex May
	supply@max-tech.aero

	MKS DevO Chemicals  
	Efe Dikergil
	efe.dikergil@mksdevo.com

	Newave Aerochemical Co. Ltd.
	Shao Jing
	lwgs@newave.cn

	ROMCHIM PROTECT SRL
	Eugenia Hongu
	contact@romchimprotect.ro

	Shaanxi Cleanway Aviation Chemical Co., Ltd
	Arella
	xiangaokelihua@163.com

	Topan LLC
	Almat Kurmanov
	almat.kurmanov@topan.kz

	Turbotect Slovakia, s.r.o
	Olha Lapenko
	chemia@rekos.sk

	Xinjiang Zhongtian Liyang Aviation Newmaterial Technology Co., Ltd.
	Huang Liang
	heima.54@foxmail.com


1 Contact information provided above is the latest information as of the time of publication, August 11, 2026.
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