**PA-01 Vapor Lost Communications Procedure Summary:**

The UAS operators will have redundant communications with the ATC authority, which include the use of a 2-way base station radio and cellular phones. In the event of a loss of communications with the ATC authority, the aircraft will be commanded to the lost link flightplan, which is a RTB and landing.

The UAS Pilot and Observers will be collocated and on 2-way radio or cellular phone communication at all times. In the event of a loss of communications between the Observer and Pilot, the aircraft will be commanded to the lost link flightplan, which is a RTB and landing.